# Class CIM_LogicalPort
extends CIM_LogicalDevice

The abstraction of a port or connection point of a Device. This object should be instantiated when the Port has independent management characteristics from the Device that includes it. Examples are a Fibre Channel Port and a USB Port.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_LogicalPort

## Direct Known Subclasses

CIM_ATAPort
CIM_DAPort
CIM_FibrePort
CIM_NetworkPort
CIM_ParallelPort
CIM_PCIPort
CIM_SASSATAPort
CIM_SerialPort
CIM_SPIPort
CIM_USBPort

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | The abstraction of a port or connection point of a Device. This object should be instantiated when the Port has independent management characteristics from the Device that includes it. Examples are a Fibre Channel Port and a USB Port.
UMLPackagePath | string | CIM::Device::Ports
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
MaxSpeed | uint64 |
Description | string | The maximum bandwidth of the Port in Bits per Second.
PUnit | string | bit / second
Units | string | Bits per Second
OtherPortType | string |
Description | string | Describes the type of module, when PortType is set to 1 ("Other").
ModelCorrespondence | string | CIM_LogicalPort.PortType
PortType | uint16 |
Description | string | PortType is defined to force consistent naming of the 'type' property in subclasses and to guarantee unique enum values for all instances of NetworkPort. When set to 1 ("Other"), related property OtherPortType contains a string description of the type of port. A range of values, DMTF_Reserved, has been defined that allows subclasses to override and define their specific types of ports.
ModelCorrespondence | string | CIM_NetworkPort.OtherNetworkPortType
ValueMap | string | 0, 1, 2, 3..15999, 16000..65535
Values | string | Unknown, Other, Not Applicable, DMTF Reserved, Vendor Reserved
RequestedSpeed | uint64 |
Description | string | The requested bandwidth of the Port in Bits per Second. The actual bandwidth is reported in LogicalPort.Speed.
ModelCorrespondence | string | CIM_LogicalPort.Speed
PUnit | string | bit / second
Units | string | Bits per Second
Write | boolean | true
Speed | uint64 |
Description | string | The bandwidth of the Port in Bits per Second.
PUnit | string | bit / second
Units | string | Bits per Second
UsageRestriction | uint16 |
Description | string | In some circumstances, a LogicalPort might be identifiable as a front end or back end port. An example of this situation would be a storage array that might have back end ports to communicate with disk drives and front end ports to communicate with hosts. If there is no restriction on the use of the port, then the value should be set to 'not restricted'.
ValueMap | string | 0, 2, 3, 4
Values | string | Unknown, Front-end only, Back-end only, Not restricted

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice