# Class CIM_Printer
extends CIM_LogicalDevice

Capabilities and management of the Printer LogicalDevice. The ABNF for CIM references to PWG Standards and MIBs is in the directory 'ftp://ftp.pwg.org/pub/pwg/general/process' in the file 'pwg-cim-references-format-20060309.txt'. Examples include: (a) a MappingStrings reference to a PWG Standard is 'PWG5101-1.PWG|Section 4 Media Color Names'; (b) a MappingStrings reference to a PWG MIB is 'MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMonitorCompletedJobs'. Note: A Printer shall be associated with at least one of every required component (e.g., PrintMarker) via an instance of the PrinterComponent class. A Printer may be associated with zero or more optional components (e.g., PrintSupply) via an instance of the ConcreteComponent class. See: Model in section 2 of Printer MIB (RFC 3805).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Printer

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of the Printer LogicalDevice. The ABNF for CIM references to PWG Standards and MIBs is in the directory 'ftp://ftp.pwg.org/pub/pwg/general/process' in the file 'pwg-cim-references-format-20060309.txt'. Examples include: (a) a MappingStrings reference to a PWG Standard is 'PWG5101-1.PWG|Section 4 Media Color Names'; (b) a MappingStrings reference to a PWG MIB is 'MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMonitorCompletedJobs'. Note: A Printer shall be associated with at least one of every required component (e.g., PrintMarker) via an instance of the PrinterComponent class. A Printer may be associated with zero or more optional components (e.g., PrintSupply) via an instance of the ConcreteComponent class. See: Model in section 2 of Printer MIB (RFC 3805).
MappingStrings | string | MIB.IETF|Printer-MIB.prtGeneralEntry
UMLPackagePath | string | CIM::Device::Printing
Version | string | 2.25.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AllAlerts | uint32 |
Description | string | A running counter of the total number of alerts (critical and non-critical) that have occurred on this Printer and have been recorded in corresponding instances of PrintAlertRecord. Note: This should be a persistent (lifetime) property.
Experimental | boolean | true
MappingStrings | string | MIB.IETF|Printer-MIB.prtAlertAllEvents
ConsoleDisabled | boolean |
Description | string | Denotes whether or not the local console is disabled. If this value of this property is true, then input is not accepted from the local console. (i.e., console is locked).
Experimental | boolean | true
MappingStrings | string | MIB.IETF|Printer-MIB.prtConsoleDisable
ConsoleNaturalLanguage | string |
Description | string | Identifies the current language that is being used by the Printer for the local console. The language listed in the ConsoleNaturalLanguage property should also be listed in NaturalLanguagesSupported. ConsoleDisplayBufferText values shall be in this natural language.
Experimental | boolean | true
MappingStrings | string | MIB.IETF|Printer-MIB.prtConsoleLocalization, MIB.IETF|Printer-MIB.prtLocalizationLanguage, MIB.IETF|Printer-MIB.prtLocalizationCountry
ModelCorrespondence | string | CIM_Printer.NaturalLanguagesSupported, CIM_Printer.ConsoleDisplayBufferText
CriticalAlerts | uint32 |
Description | string | A running counter of the number of critical alerts that have occurred on this Printer and have been recorded in corresponding instances of PrintAlertRecord. Note: This should be a persistent (lifetime) property.
Experimental | boolean | true
MappingStrings | string | MIB.IETF|Printer-MIB.prtAlertCriticalEvents
CurrentCharSet | string |
Description | string | Specifies the current character set that is being used for the output of text that relates to the management of the Printer. The character set that is described by this property should also be listed in CharsetsSupported. The string that is specified by this property should conform to the semantics and syntax that are specified by section 4.1.2 ("Charset parameter") in RFC 2046 (MIME Part 2) and contained in the IANA character-set registry. Examples include "utf-8", "us-ascii" and "iso-8859-1". Note: For compatiblity with the IETF Printer MIB (RFC 3805) and IETF IPP/1.1 (RFC 2911), values in this array property shall be parallel to values in CharSetsSupported.
MappingStrings | string | MIB.IETF|Printer-MIB.prtGeneralCurrentLocalization, MIB.IETF|Printer-MIB.prtLocalizationCharacterSet, MIB.IETF|IANA-CHARSET-MIB.IANACharset, RFC2911.IETF|Section 4.4.19 charset-configured
ModelCorrespondence | string | CIM_Printer.CharSetsSupported
CurrentLanguage | uint16 |
Deprecated | string | CIM_PrintInterpreter.LangType
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use the Printer component classes PrintInterpreter and PrintChannel and the association class AssociatedPrintInterpreter value of DefaultType (JCL or PDL) to the PrintInterpreter.LangType property for default language(s) for each PrintChannel instance. Deprecated description: Indicates the current printer language being used. A language that is being used by the Printer should also be listed in LanguagesSupported. Note: For legacy compatiblity reasons, this property is NOT exactly aligned (in order of values) with the authoritative PrtInterpreterLangFamilyTC in the IANA Printer MIB, unlike the newer property PrintInterpreter.LangType (which is exactly aligned with the IANA Printer MIB).
MappingStrings | string | MIB.IETF|Printer-MIB.prtChannelDefaultPageDescLangIndex, MIB.IETF|Printer-MIB.prtInterpreterLangFamily, MIB.IETF|IANA-PRINTER-MIB.PrtInterpreterLangFamilyTC, RFC2911.IETF|Section 4.4.21 document-format-default
ModelCorrespondence | string | CIM_Printer.LanguagesSupported, CIM_Printer.CurrentMimeType
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64, 65, 66, 67, 68, 69, ..
Values | string | Other, Unknown, PCL, HPGL, PJL, PS, PSPrinter, IPDS, PPDS, EscapeP, Epson, DDIF, Interpress, ISO6429, Line Data, MODCA, REGIS, SCS, SPDL, TEK4014, PDS, IGP, CodeV, DSCDSE, WPS, LN03, CCITT, QUIC, CPAP, DecPPL, Simple Text, NPAP, DOC, imPress, Pinwriter, NPDL, NEC201PL, Automatic, Pages, LIPS, TIFF, Diagnostic, CaPSL, EXCL, LCDS, XES, MIME, TIPSI, Prescribe, LinePrinter, IDP, XJCL, PDF, RPDL, IntermecIPL, UBIFingerprint, UBIDirectProtocol, Fujitsu, PCLXL, ART, CGM, JPEG, CALS1, CALS2, NIRS, C4, XPS, OpenXPS, DMTF Reserved
CurrentMimeType | string |
Deprecated | string | CIM_PrintInterpreter.LangType
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use the Printer component classes PrintInterpreter and PrintChannel and the association class AssociatedPrintInterpreter value of DefaultType (JCL or PDL) to the PrintInterpreter.LangType property for default language(s) for each PrintChannel instance. Deprecated description: Specifies the MIME type that is currently in use by the Printer if the CurrentLanguage is set to indicate that a MIME type is in use (value=47).
MappingStrings | string | RFC2911.IETF|Section 4.4.21 document-format-default
ModelCorrespondence | string | CIM_Printer.CurrentLanguage
CurrentNaturalLanguage | string |
Description | string | Identifies the current language that is being used by the Printer for management. The language listed in the CurrentNaturalLanguage property should also be listed in NaturalLanguagesSupported.
MappingStrings | string | MIB.IETF|Printer-MIB.prtGeneralCurrentLocalization, MIB.IETF|Printer-MIB.prtLocalizationLanguage, MIB.IETF|Printer-MIB.prtLocalizationCountry, RFC2911.IETF|Section 4.4.19 natural-language-configured
ModelCorrespondence | string | CIM_Printer.NaturalLanguagesSupported
CurrentOperator | string |
Description | string | The name of the person who is responsible for operating this Printer. It is suggested that this string include information that would enable other humans to reach the operator, such as a phone number. As a convention to facilitate automatic notification of the operator by the agent or network management station, the phone number, fax number or email address should be indicated by the URL schemes 'tel:', 'fax:' and 'mailto:', respectively. If either the phone, fax, or email information is not available, then a line should not be included for this information. NOTE: For interoperability purposes, it is advisable to use email addresses formatted according to [RFC2822] requirements.
Experimental | boolean | true
MappingStrings | string | MIB.IETF|Printer-MIB.prtGeneralCurrentOperator
MaxLen | uint32 | 255
MinLen | uint32 | 0
CurrentPaperType | string |
Deprecated | string | No value
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use the MediaType, MediaName, and MediaSizeName and IsDefault properties in PrintInputTray. Deprecated description: Specifies the paper type that the Printer is currently using. The string should be a value of PaperTypesAvailable. The values of the property SHOULD conform to the requirements of the PWG Media Standardized Names specification [PWG5101.1], which defines the normative values for this property. See older Appendix B 'Media Size Names' and Appendix C 'Media Names' of IETF Printer MIB v2 [RFC3805] which list the values of standardized media names defined in ISO DPA [ISO10175].
MappingStrings | string | PWG5101-1.PWG|Media Standardized Names, MIB.IETF|Printer-MIB.prtInputDefaultIndex, MIB.IETF|Printer-MIB.prtInputMediaName, RFC2911.IETF|Printer.media-default, RFC2911.IETF|Section 4.2 Job Template Attributes, RFC2911.IETF|Section 4.2.11 media, RFC2911.IETF|APPENDIX C 'media' keyword values
ModelCorrespondence | string | CIM_Printer.PaperTypesAvailable
DefaultCopies | uint32 |
Description | string | Note: The use of this property will be deprecated in favor of new PrintServiceSettings.Copies in the future. The number of copies that will be produced for a single Job unless otherwise specified.
MappingStrings | string | RFC2911.IETF|Printer.copies-default, RFC2911.IETF|Section 4.2 Job Template Attributes, RFC2911.IETF|Section 4.2.5 copies
DefaultLanguage | uint16 |
Deprecated | string | CIM_PrintInterpreter.LangType
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use the Printer component classes PrintInterpreter and PrintChannel and the association class AssociatedPrintInterpreter value of DefaultType (JCL or PDL) to the PrintInterpreter.LangType property for default language(s) for each PrintChannel instance. Deprecated description: Indicates the default printer language. A language that is used as a default by the Printer should also be listed in LanguagesSupported. Note: For legacy compatiblity reasons, this property is NOT exactly aligned (in order of values) with the authoritative PrtInterpreterLangFamilyTC in the IANA Printer MIB, unlike the newer property PrintInterpreter.LangType (which is exactly aligned with the IANA Printer MIB).
MappingStrings | string | MIB.IETF|Printer-MIB.prtChannelDefaultPageDescLangIndex, MIB.IETF|Printer-MIB.prtInterpreterLangFamily, MIB.IETF|IANA-PRINTER-MIB.PrtInterpreterLangFamilyTC, RFC2911.IETF|Section 4.4.21 document-format-default
ModelCorrespondence | string | CIM_Printer.LanguagesSupported, CIM_Printer.DefaultMimeType
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64, 65, 66, 67, 68, 69, ..
Values | string | Other, Unknown, PCL, HPGL, PJL, PS, PSPrinter, IPDS, PPDS, EscapeP, Epson, DDIF, Interpress, ISO6429, Line Data, MODCA, REGIS, SCS, SPDL, TEK4014, PDS, IGP, CodeV, DSCDSE, WPS, LN03, CCITT, QUIC, CPAP, DecPPL, Simple Text, NPAP, DOC, imPress, Pinwriter, NPDL, NEC201PL, Automatic, Pages, LIPS, TIFF, Diagnostic, CaPSL, EXCL, LCDS, XES, MIME, TIPSI, Prescribe, LinePrinter, IDP, XJCL, PDF, RPDL, IntermecIPL, UBIFingerprint, UBIDirectProtocol, Fujitsu, PCLXL, ART, CGM, JPEG, CALS1, CALS2, NIRS, C4, XPS, OpenXPS, DMTF Reserved
DefaultMimeType | string |
Deprecated | string | CIM_PrintInterpreter.LangType
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use the Printer component classes PrintInterpreter and PrintChannel and the association class AssociatedPrintInterpreter value of DefaultType (JCL or PDL) to the PrintInterpreter.LangType property for default language(s) for each PrintChannel instance. Deprecated description: Specifies the default MIME type that is used by the Printer if the DefaultLanguage is set to indicate that a MIME type is in use (value=47).
MappingStrings | string | RFC2911.IETF|Section 4.4.21 document-format-default
ModelCorrespondence | string | CIM_Printer.DefaultLanguage
DefaultNumberUp | uint32 |
Description | string | Note: The use of this property will be deprecated in favor of new PrintServiceSettings.NumberUp in the future. The number of print-stream pages that the Printer will render onto a single media sheet unless a Job specifies otherwise.
MappingStrings | string | RFC2911.IETF|Printer.number-up-default, RFC2911.IETF|Section 4.2 Job Template Attributes, RFC2911.IETF|Section 4.2.9 number-up
DefaultPaperType | string |
Deprecated | string | No value
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use the MediaType, MediaName, and MediaSizeName and IsDefault properties in PrintInputTray. Deprecated description: Specifies the paper type that the Printer will use if a PrintJob does not specify a particular type. The string should be a value of PaperTypesAvailable. The values of the property SHOULD conform to the requirements of the PWG Media Standardized Names specification [PWG5101.1], which defines the normative values for this property. See older Appendix B 'Media Size Names' and Appendix C 'Media Names' of IETF Printer MIB v2 [RFC3805] which list the values of standardized media names defined in ISO DPA [ISO10175].
MappingStrings | string | PWG5101-1.PWG|Media Standardized Names, MIB.IETF|Printer-MIB.prtInputDefaultIndex, MIB.IETF|Printer-MIB.prtInputMediaName, RFC2911.IETF|Printer.media-default, RFC2911.IETF|Section 4.2 Job Template Attributes, RFC2911.IETF|Section 4.2.11 media, RFC2911.IETF|APPENDIX C 'media' keyword values
ModelCorrespondence | string | CIM_Printer.PaperTypesAvailable
DetectedErrorState | uint16 |
Description | string | Printer error info mapped from hrPrinterDetectedErrorState in Host Resources MIB (RFC 2790), as follows: 0 (Unknown) means no error information is available 1 (Other) means some non-standard error has occurred - see Printer.ErrorInformation for more information 2 (No Error) means there are no error conditions 3 (Low Paper) means PrintInputTray is low on paper 4 (No Paper) means all PrintInputTray(s) are empty 5 (Low Toner) means PrintMarker is low on toner 6 (No Toner) means PrintMarker is out of toner 7 (Door Open) means PrintInterlock is open 8 (Jammed) means PrintMarker or PrintMediaPath is jammed 9 (Offline) means Printer is offline (see PrinterStatus) 10 (Service Requested) means intervention is required 11 (Output Bin Full) means PrintOutputTray is full 12 (Input Tray Missing) means PrintInputTray is missing 13 (Output Tray Missing) means PrintOutputTray is missing 14 (Marker Supply Missing) means PrintSupply is missing 15 (Output Near Full) means PrintOutputTray is nearly full 16 (Input Tray Empty) means PrintInputTray is empty 17 (Overdue Prevent Maint) means Printer needs service.
MappingStrings | string | MIB.IETF|HOST-RESOURCES-MIB.hrPrinterDetectedErrorState
ModelCorrespondence | string | CIM_Printer.ErrorInformation
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, ..
Values | string | Unknown, Other, No Error, Low Paper, No Paper, Low Toner, No Toner, Door Open, Jammed, Offline, Service Requested, Output Bin Full, Input Tray Missing, Output Tray Missing, Marker Supply Missing, Output Near Full, Input Tray Empty, Overdue Prevent Maint, DMTF Reserved
ElementName | string |
Description | string | The user-friendly name for this instance of Printer. In addition, the user-friendly name can be used as an index property for a search or query. (Note: The name does not have to be unique within a namespace.) This name shall be generated as a factory default by the manufacturer and may be changed out-of-band to a site-specific name by the system administrator.
MappingStrings | string | MIB.IETF|Printer-MIB.prtGeneralPrinterName
ModelCorrespondence | string | CIM_ManagedElement.ElementName
Override | string | ElementName
Required | boolean | true
HorizontalResolution | uint32 |
Deprecated | string | CIM_PrintMarker.XFeedAddressability
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use the XFeedAddressability property in the Printer component classes PrintMarker and PrintInterpreter. Deprecated description: The resolution of the Printer in Pixels per Inch in the cross-feed direction, i.e., short-edge in portrait feed mode.
MappingStrings | string | MIB.IETF|Printer-MIB.prtMarkerAddressabilityXFeedDir, RFC2911.IETF|Section 4.2.12 printer-resolution
ModelCorrespondence | string | CIM_PrintJob.HorizontalResolution
PUnit | string | pixel / inch
Units | string | Pixels per Inch
JobCountSinceLastReset | uint32 |
Counter | boolean | true
Description | string | Printer jobs that are processed since last reset. These jobs can be processed from one or more PrintQueues.
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMonitorCompletedJobs
MarkingTechnology | uint16 |
Deprecated | string | CIM_PrintMarker.MarkTech
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use PrintMarker.MarkTech. Deprecated description: Specifies the marking technology that is used by the Printer.
MappingStrings | string | MIB.IETF|Printer-MIB.prtMarkerMarkTech, MIB.IETF|IANA-PRINTER-MIB.PrtMarkerMarkTechTC
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, ..
Values | string | Other, Unknown, Electrophotographic LED, Electrophotographic Laser, Electrophotographic Other, Impact Moving Head Dot Matrix 9pin, Impact Moving Head Dot Matrix 24pin, Impact Moving Head Dot Matrix Other, Impact Moving Head Fully Formed, Impact Band, Impact Other, Inkjet Aqueous, Inkjet Solid, Inkjet Other, Pen, Thermal Transfer, Thermal Sensitive, Thermal Diffusion, Thermal Other, Electroerosion, Electrostatic, Photographic Microfiche, Photographic Imagesetter, Photographic Other, Ion Deposition, eBeam, Typesetter, DMTF Reserved
MaxCopies | uint32 |
Description | string | Note: The use of this property will be deprecated in favor of new PrintServiceCapabilities.Copies in the future. The maximum number of copies that can be produced by the Printer from a single Job.
MappingStrings | string | RFC2911.IETF|Printer.copies-supported, RFC2911.IETF|Section 4.2 Job Template Attributes, RFC2911.IETF|Section 4.2.5 copies
ModelCorrespondence | string | CIM_PrintJob.Copies
MaxNumberUp | uint32 |
Description | string | Note: The use of this property will be deprecated in favor of new PrintServiceCapabilities.NumberUp in the future. The maximum number of print-stream pages that the Printer can render onto a single media sheet.
MappingStrings | string | RFC2911.IETF|Printer.number-up-supported, RFC2911.IETF|Section 4.2 Job Template Attributes, RFC2911.IETF|Section 4.2.9 number-up
ModelCorrespondence | string | CIM_PrintJob.NumberUp
MaxSizeSupported | uint32 |
Description | string | Note: The use of this property will be deprecated in favor of new PrintServiceCapabilities.MaxJobSize in the future. Specifies the largest Job (as a byte stream) that the Printer will accept in units of Kbytes. A value of 0 indicates that no limit has been set.
MappingStrings | string | RFC2911.IETF|Section 4.4.33 job-k-octets-supported
ModelCorrespondence | string | CIM_PrintJob.JobSize
PUnit | string | byte * 10^3
Units | string | KiloBytes
PrinterStatus | uint16 |
Description | string | Status information for a Printer, beyond that specified in the LogicalDevice.Availability property. Values mapped directly from hrPrinterStatus in Host Resources MIB (RFC 2790) are: 1 (Other) means the printer is in some non-standard state - see Printer.ErrorInformation for more information 2 (Unknown) means the printer state is unknown 3 (Idle) means the printer is ready but idle 4 (Printing) means the printer is processing job(s) 5 (Warmup) means the printer is warming up - not ready Note: The values 6 (Stopped Printing) and 7 (Offline) are redundant with DetectedErrorState (below) and not mapped from hrPrinterStatus in Host Resources MIB (RFC 2790).
MappingStrings | string | MIB.IETF|HOST-RESOURCES-MIB.hrPrinterStatus, MIB.IETF|HOST-RESOURCES-MIB.hrPrinterDetectedErrorState
ModelCorrespondence | string | CIM_LogicalDevice.Availability, CIM_Printer.DetectedErrorState, CIM_Printer.ErrorInformation
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, ..
Values | string | Other, Unknown, Idle, Printing, Warmup, Stopped Printing, Offline, DMTF Reserved
SerialNumber | string |
Description | string | A serial number for this Printer (that may index adevice catalog or inventory). The original value is a factory default set by the device manufacturer and may be changed out-of-band to a site-specific name by the system administrator.
Experimental | boolean | true
MappingStrings | string | MIB.IETF|Printer-MIB.prtGeneralSerialNumber
MaxLen | uint32 | 255
MinLen | uint32 | 0
ServicePerson | string |
Description | string | The name of the person responsible for servicing this Printer. It is suggested that this string include information that would enable other humans to reach the service person, such as a phone number. As a convention to facilitate automatic notification of the operator by the agent or network management station, the phone number, fax number or email address should be indicated by the URL schemes 'tel:', 'fax:' and 'mailto:', respectively. If either the phone, fax, or email information is not available, then a line should not be included for this information. NOTE: For interoperability purposes, it is advisable to use email addresses formatted per [RFC2822] requirements.
Experimental | boolean | true
MappingStrings | string | MIB.IETF|Printer-MIB.prtGeneralServicePerson
MaxLen | uint32 | 255
MinLen | uint32 | 0
TimeOfLastReset | datetime |
Description | string | Time of the last reset of the Printer Device.
MappingStrings | string | MIB.IETF|SNMPv2-MIB.sysUpTime, MIB.IETF|HOST-RESOURCES-MIB.hrSystemUptime, MIB.IETF|HOST-RESOURCES-MIB.hrSystemDate, RFC2911.IETF|Section 4.4.29 printer-up-time, RFC2911.IETF|Section 4.4.30 printer-current-time
VerticalResolution | uint32 |
Deprecated | string | CIM_PrintMarker.FeedAddressability
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use the FeedAddressability property in the Printer component classes PrintMarker and PrintInterpreter. Deprecated description: The resolution of the Printer in Pixels per Inch in the feed direction, i.e., long-edge in portrait feed mode.
MappingStrings | string | MIB.IETF|Printer-MIB.prtMarkerAddressabilityFeedDir, RFC2911.IETF|Section 4.2.12 printer-resolution
ModelCorrespondence | string | CIM_PrintJob.VerticalResolution
PUnit | string | pixel / inch
Units | string | Pixels per Inch
AvailableJobSheets | string[] |
Description | string | Describes all of the job sheets that are available on the Printer. This method can also be used to describe the banner that a Printer might provide at the beginning of each Job or that can describe other user specified options.
MappingStrings | string | MIB.IETF|Printer-MIB.prtAuxiliarySheetStartupPage, MIB.IETF|Printer-MIB.prtAuxiliarySheetBannerPage, RFC2911.IETF|Printer.job-sheets-supported, RFC2911.IETF|Section 4.2 Job Template Attributes, RFC2911.IETF|Section 4.2.3 job-sheets
ModelCorrespondence | string | CIM_PrintJob.RequiredJobSheets
Capabilities | uint16[] |
ArrayType | string | Indexed
Deprecated | string | No value
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use the Printer component classes, e.g., PrintInputTray, PrintMarker, PrintFinisher, etc. For example, 3 (Duplex Printing) support can be found in the PrintMediaPath.Type property. Deprecated description: An array of integers that indicates Printer capabilities. Information such as "Duplex Printing" (value=3) or "Transparency Printing" (value=7) is specified in this property.
ModelCorrespondence | string | CIM_Printer.CapabilityDescriptions, CIM_PrintJob.Finishing, CIM_PrintService.Capabilities
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, ..
Values | string | Unknown, Other, Color Printing, Duplex Printing, Copies, Collation, Stapling, Transparency Printing, Punch, Cover, Bind, Black and White Printing, One Sided, Two Sided Long Edge, Two Sided Short Edge, Portrait, Landscape, Reverse Portrait, Reverse Landscape, Quality High, Quality Normal, Quality Low, DMTF Reserved
CapabilityDescriptions | string[] |
ArrayType | string | Indexed
Deprecated | string | No value
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use the Printer component classes, e.g., PrintInputTray, PrintMarker, PrintFinisher, etc. Deprecated description: An array of free-form strings that provides more detailed explanations for any of the Printer features that are indicated in the Capabilities array. Note, each entry of this array is related to the entry in the Capabilities array that is located at the same index.
ModelCorrespondence | string | CIM_Printer.Capabilities
CharSetsSupported | string[] |
ArrayType | string | Indexed
Description | string | Identifies the available character sets for the output of text that is related to managing the Printer. Strings provided in this property should conform to the semantics and syntax specified by section 4.1.2 ("Charset parameter") in RFC 2046 (MIME Part 2) and contained in the IANA character-set registry. Examples include "utf-8", "us-ascii" and "iso-8859-1". Note: For compatiblity with the IETF Printer MIB (RFC 3805) and IETF IPP/1.1 (RFC 2911), values in this array property shall be parallel to values in NaturalLanguagesSupported.
MappingStrings | string | MIB.IETF|Printer-MIB.prtLocalizationCharacterSet, MIB.IETF|IANA-CHARSET-MIB.IANACharset, RFC2911.IETF|Section 4.4.18 charset-supported
ModelCorrespondence | string | CIM_PrintJob.CharSet
ConsoleDisplayBufferText | string[] |
ArrayType | string | Indexed
Description | string | A sequence of strings, each a line of human-readable text from the local console of the Printer, in the language specified by ConsoleNaturalLanguage.
Experimental | boolean | true
MappingStrings | string | MIB.IETF|Printer-MIB.prtConsoleDisplayBufferText
ModelCorrespondence | string | CIM_Printer.NaturalLanguagesSupported, CIM_Printer.ConsoleNaturalLanguage
CurrentCapabilities | uint16[] |
Deprecated | string | No value
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use the Printer component classes, e.g., PrintInputTray, PrintMarker, PrintFinisher, etc. Deprecated description: Specifies which finishings and other capabilities of the Printer are currently being used. An entry in this property should also be listed in the Capabilities array.
ModelCorrespondence | string | CIM_Printer.Capabilities
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, ..
Values | string | Unknown, Other, Color Printing, Duplex Printing, Copies, Collation, Stapling, Transparency Printing, Punch, Cover, Bind, Black and White Printing, One Sided, Two Sided Long Edge, Two Sided Short Edge, Portrait, Landscape, Reverse Portrait, Reverse Landscape, Quality High, Quality Normal, Quality Low, DMTF Reserved
DefaultCapabilities | uint16[] |
Deprecated | string | No value
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use the Printer component classes, e.g., PrintInputTray, PrintMarker, PrintFinisher, etc. Deprecated description: Specifies which finishings and other capabilities of the Printer will be used by default. An entry in Default Capabilities should also be listed in the Capabilities array.
ModelCorrespondence | string | CIM_Printer.Capabilities
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, ..
Values | string | Unknown, Other, Color Printing, Duplex Printing, Copies, Collation, Stapling, Transparency Printing, Punch, Cover, Bind, Black and White Printing, One Sided, Two Sided Long Edge, Two Sided Short Edge, Portrait, Landscape, Reverse Portrait, Reverse Landscape, Quality High, Quality Normal, Quality Low, DMTF Reserved
ErrorInformation | string[] |
Description | string | An array that provides supplemental information for the current error state, that is indicated in DetectedErrorState.
MappingStrings | string | RFC2911.IETF|Section 4.4.13 printer-state-message
ModelCorrespondence | string | CIM_Printer.DetectedErrorState
LanguagesSupported | uint16[] |
Deprecated | string | CIM_PrintInterpreter.LangType
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use PrintInterpreter.LangType. Deprecated description: An array that indicates the print languages that are natively supported Note: For legacy compatiblity reasons, this property is NOT exactly aligned (in order of values) with the authoritative PrtInterpreterLangFamilyTC in the IANA Printer MIB, unlike the newer property PrintInterpreter.LangType (which is exactly aligned with the IANA Printer MIB).
MappingStrings | string | MIB.IETF|Printer-MIB.prtInterpreterLangFamily, MIB.IETF|IANA-PRINTER-MIB.PrtInterpreterLangFamilyTC, RFC2911.IETF|Section 4.4.22 document-format-supported
ModelCorrespondence | string | CIM_Printer.MimeTypesSupported, CIM_PrintJob.Language, CIM_PrintService.LanguagesSupported, CIM_PrintInterpreter.LangType
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64, 65, 66, 67, 68, 69, ..
Values | string | Other, Unknown, PCL, HPGL, PJL, PS, PSPrinter, IPDS, PPDS, EscapeP, Epson, DDIF, Interpress, ISO6429, Line Data, MODCA, REGIS, SCS, SPDL, TEK4014, PDS, IGP, CodeV, DSCDSE, WPS, LN03, CCITT, QUIC, CPAP, DecPPL, Simple Text, NPAP, DOC, imPress, Pinwriter, NPDL, NEC201PL, Automatic, Pages, LIPS, TIFF, Diagnostic, CaPSL, EXCL, LCDS, XES, MIME, TIPSI, Prescribe, LinePrinter, IDP, XJCL, PDF, RPDL, IntermecIPL, UBIFingerprint, UBIDirectProtocol, Fujitsu, PCLXL, ART, CGM, JPEG, CALS1, CALS2, NIRS, C4, XPS, OpenXPS, DMTF Reserved
MimeTypesSupported | string[] |
Deprecated | string | CIM_PrintInterpreter.LangType
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use PrintInterpreter.LangType. Deprecated description: An array of free-form strings that provides more detailed explanations of any MIME types that are supported by the Printer. If data is provided for this property, then the (value=47), "Mime", should be included in the Languages Supported property.
MappingStrings | string | RFC2911.IETF|Section 4.4.22 document-format-supported
ModelCorrespondence | string | CIM_Printer.LanguagesSupported, CIM_PrintJob.MimeTypes, CIM_PrintService.MimeTypesSupported, CIM_PrintInterpreter.LangType
NaturalLanguagesSupported | string[] |
ArrayType | string | Indexed
Description | string | Identifies the available languages for strings that are used by the Printer for the output of management information. The strings should conform to RFC 1766, for example, "en" is used for English.
MappingStrings | string | MIB.IETF|Printer-MIB.prtLocalizationLanguage, MIB.IETF|Printer-MIB.prtLocalizationCountry, RFC2911.IETF|Printer.generated-natural-language-supported, RFC2911.IETF|Section 4.4.20
ModelCorrespondence | string | CIM_Printer.CurrentNaturalLanguage, CIM_Printer.ConsoleNaturalLanguage, CIM_PrintJob.NaturalLanguage
PaperSizesSupported | uint16[] |
Deprecated | string | CIM_PrintInputTray.MediaSizeName
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use PrintInputTray.MediaSizeName. Deprecated description: An integer array that indicates the sizes of paper supported.
MappingStrings | string | PWG5101-1.PWG|Media Standardized Names, MIB.IETF|Printer-MIB.prtInputMediaName, MIB.IETF|Printer-MIB.prtInputMediaDimFeedDirChosen, MIB.IETF|Printer-MIB.prtInputMediaDimXFeedDirChosen, RFC2911.IETF|Printer.media-supported, RFC2911.IETF|Section 4.2 Job Template Attributes, RFC2911.IETF|Section 4.2.11 media, RFC2911.IETF|APPENDIX C 'media' keyword values
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64, 65, 66, 67, 68, 69, 70, 71, 72, 73, 74, 75, ..
Values | string | Unknown, Other, A, B, C, D, E, Letter, Legal, NA-10x13-Envelope, NA-9x12-Envelope, NA-Number-10-Envelope, NA-7x9-Envelope, NA-9x11-Envelope, NA-10x14-Envelope, NA-Number-9-Envelope, NA-6x9-Envelope, NA-10x15-Envelope, A0, A1, A2, A3, A4, A5, A6, A7, A8, A9, A10, B0, B1, B2, B3, B4, B5, B6, B7, B8, B9, B10, C0, C1, C2, C3, C4, C5, C6, C7, C8, ISO-Designated, JIS B0, JIS B1, JIS B2, JIS B3, JIS B4, JIS B5, JIS B6, JIS B7, JIS B8, JIS B9, JIS B10, NA-Letter, NA-Legal, B4-Envelope, B5-Envelope, C3-Envelope, C4-Envelope, C5-Envelope, C6-Envelope, Designated-Long-Envelope, Monarch-Envelope, Executive, Folio, Invoice, Ledger, Quarto, DMTF Reserved
PaperTypesAvailable | string[] |
ArrayType | string | Indexed
Deprecated | string | No value
Description | string | Note: The use of this property has been deprecated, due to ambiguity. Instead use the MediaType, MediaName, and MediaSizeName and IsDefault properties in PrintInputTray. Deprecated description: An array of free-form strings specifying the types and sizes of paper that are currently available on the Printer. The values of the property SHOULD conform to the requirements of the PWG Media Standardized Names specification [PWG5101.1], which defines the normative values for this property. See older Appendix B 'Media Size Names' and Appendix C 'Media Names' of IETF Printer MIB v2 [RFC3805] which list the values of standardized media names defined in ISO DPA [ISO10175].
MappingStrings | string | PWG5101-1.PWG|Media Standardized Names, MIB.IETF|Printer-MIB.prtInputMediaName, RFC2911.IETF|Printer.media-ready, RFC2911.IETF|Section 4.2 Job Template Attributes, RFC2911.IETF|Section 4.2.11 media, RFC2911.IETF|APPENDIX C 'media' keyword values
ModelCorrespondence | string | CIM_PrintJob.RequiredPaperType, CIM_PrintService.PaperTypesAvailable

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice