# Class CIM_EWMAMeterService
extends CIM_MeterService

This is a concrete subclass of the MeterService class that represents an exponentially weighted moving average meter. This meter is a simple low-pass filter that measures the rate of incoming packets over a small, fixed sampling interval. Any admitted packet that pushes the average rate over a pre-defined limit is defined to be non-conforming.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_ConditioningService
|
+--CIM_MeterService
|
+--CIM_EWMAMeterService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This is a concrete subclass of the MeterService class that represents an exponentially weighted moving average meter. This meter is a simple low-pass filter that measures the rate of incoming packets over a small, fixed sampling interval. Any admitted packet that pushes the average rate over a pre-defined limit is defined to be non-conforming.
UMLPackagePath | string | CIM::Network::QoS
Version | string | 2.7.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AverageRate | uint32 |
Description | string | This property is a 32-bit unsigned integer that defines the average rate against which the sampled arrival rate of packets should be measured. Any packet that causes the sampled rate to exceed this rate is deemed non-conforming. The value is specified in kilobits per second.
PUnit | string | bit / second * 10^3
Units | string | KiloBits Per Second
DeltaInterval | uint64 |
Description | string | This property is a 64-bit unsigned integer that defines the sampling interval used to measure the arrival rate. The calculated rate is averaged over this interval and checked against the AverageRate property. All packets whose computed average arrival rate is less than the AverageRate are deemed conforming. The value is specified in microseconds.
PUnit | string | second * 10^-6
Units | string | MicroSeconds
Gain | uint32 |
Description | string | This property is a 32-bit unsigned integer representing the reciprocal of the time constant (e.g., frequency response) of what is essentially a simple low-pass filter. For example, the value 64 for this property represents a time constant value of 1/64.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
ConformanceLevels | uint16 | CIM_MeterService
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
Enabled | boolean | CIM_ConditioningService
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
MeterType | uint16 | CIM_MeterService
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherMeterType | string | CIM_MeterService
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
RequestStateChange | uint32 | CIM_EnabledLogicalElement
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service