# Class CIM_LAGPortPartnerSettings
extends CIM_SettingData

LAGPortPartnerSettings contains the configuration information for a protocol Partner of a LAG port. This allows manually configured aggregation. The configuration information is associated with an instance of LAGPort8023ad via ElementSettingData.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_LAGPortPartnerSettings

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | LAGPortPartnerSettings contains the configuration information for a protocol Partner of a LAG port. This allows manually configured aggregation. The configuration information is associated with an instance of LAGPort8023ad via ElementSettingData.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::8023LAG
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
PortPartnerAdminKey | uint16 |
Description | string | The current administrative value of the 16-bit Key for the protocol Partner. The assigned value is used, along with the values of the other properties of this class, in order to achieve manually configured aggregation. For more information, refer to the IEEE 802.3 document, Subclause 30.7.2.1.10.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortPartnerAdminKey
ModelCorrespondence | string | CIM_LAGPortPartnerSettings.PortPartnerAdminSystemID, CIM_LAGPortPartnerSettings.PortPartnerAdminSystemPriority, CIM_LAGPortPartnerSettings.PortPartnerAdminPort, CIM_LAGPortPartnerSettings.PortPartnerAdminPortPriority, CIM_LAGPortPartnerConnection.PortPartnerOperKey
Write | boolean | true
PortPartnerAdminPort | uint16 |
Description | string | The current administrative value of the port number for the protocol Partner. This is a 16-bit value. The assigned value is used, along with the values of the other properties of this class, in order to achieve manually configured aggregation. For more information, refer to the IEEE 802.3 document, Subclause 30.7.2.1.16.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortPartnerAdminPort
ModelCorrespondence | string | CIM_LAGPortPartnerSettings.PortPartnerAdminSystemID, CIM_LAGPortPartnerSettings.PortPartnerAdminSystemPriority, CIM_LAGPortPartnerSettings.PortPartnerAdminKey, CIM_LAGPortPartnerSettings.PortPartnerAdminPortPriority, CIM_LAGPortPartnerConnection.PortPartnerOperPort
Write | boolean | true
PortPartnerAdminPortPriority | uint16 |
Description | string | The current administrative value of the port priority for the protocol Partner. This is a 16-bit value. The assigned value is used, along with the values of the other properties of this class, in order to achieve manually configured aggregation. For more information, refer to the IEEE 802.3 document, Subclause 30.7.2.1.18.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortPartnerAdminPortPriority
ModelCorrespondence | string | CIM_LAGPortPartnerSettings.PortPartnerAdminSystemID, CIM_LAGPortPartnerSettings.PortPartnerAdminSystemPriority, CIM_LAGPortPartnerSettings.PortPartnerAdminKey, CIM_LAGPortPartnerSettings.PortPartnerAdminPort, CIM_LAGPortPartnerConnection.PortPartnerOperPortPriority
Write | boolean | true
PortPartnerAdminSystemID | string |
Description | string | A 6-octet MACAddress value representing the administrative value of the Aggregation Port's protocol Partner's System ID. The assigned value is used, along with the values of the other properties of this class, in order to achieve manually configured aggregation. For more information, refer to the IEEE 802.3 document, Subclause 30.7.2.1.8. Note that the MAC address is formatted as twelve hexadecimal digits (e.g., "010203040506"), with each pair representing one of the six octets of the MAC address in "canonical" bit order according to RFC 2469.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortPartnerAdminSystemID
MaxLen | uint32 | 12
ModelCorrespondence | string | CIM_LAGPortPartnerSettings.PortPartnerAdminSystemPriority, CIM_LAGPortPartnerSettings.PortPartnerAdminKey, CIM_LAGPortPartnerSettings.PortPartnerAdminPort, CIM_LAGPortPartnerSettings.PortPartnerAdminPortPriority, CIM_LAGPortPartnerConnection.PortPartnerOperSystemID
Write | boolean | true
PortPartnerAdminSystemPriority | uint16 |
Description | string | A 2-octet value used to define the administrative value of priority associated with the Partner's System ID. The assigned value is used, along with the values of the other properties of this class, in order to achieve manually configured aggregation. For more information, refer to the IEEE 802.3 document, Subclause 30.7.2.1.6.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortPartnerAdminSystemPriority
ModelCorrespondence | string | CIM_LAGPortPartnerSettings.PortPartnerAdminSystemID, CIM_LAGPortPartnerSettings.PortPartnerAdminKey, CIM_LAGPortPartnerSettings.PortPartnerAdminPort, CIM_LAGPortPartnerSettings.PortPartnerAdminPortPriority, CIM_LAGPortPartnerConnection.PortPartnerOperSystemPriority
Write | boolean | true

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_SettingData

## Class Methods