# Class CIM_SmartCardReader
extends CIM_LogicalDevice

SmartCardReader is the logical representation of Smart Card Reader Device. It includes the configuration, setup or operation of aSmart Card Reader Device.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_SmartCardReader

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | SmartCardReader is the logical representation of Smart Card Reader Device. It includes the configuration, setup or operation of aSmart Card Reader Device.
Experimental | boolean | true
Version | string | 2.21.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CacheTimeout | datetime |
Description | string | Specifies the maximum time (as a datetime interval) that the smart card Reader will retain the information for a contactless smart card.
IsCardDetected | boolean |
Description | string | A Boolean indicates whether the Smart Card is inserted. True if card is detected and False if card is not detected.
OtherSmartCardTypesSupported | string[] |
Description | string | An array of the free-form string providing a description of the SmartCardTypesSupported when 1,"Other", is specified for the SmartCardTypesSupported.
MaxLen | uint32 | 256
ModelCorrespondence | string | CIM_SmartCard.OtherSmartCardType, CIM_SmartCard.SmartCardType, CIM_SmartCardReader.SmartCardTypesSupported
SmartCardTypesSupported | uint16[] |
Description | string | An array of integer enumeration that indicates the supported Smart Card Type
ModelCorrespondence | string | CIM_SmartCard.SmartCardType, CIM_SmartCard.OtherSmartCardType, CIM_SmartCardReader.OtherSmartCardTypesSupported
ValueMap | string | 0, 1, 3, 4, .., 32768..65535
Values | string | Unknown, Other, Contacted, Contactless, DMTF Reserved, Vendor Specified

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice