# Class CIM_PCIBridge
extends CIM_PCIDevice

Capabilities and management of a PCI controller that provide bridge-to-bridge capability.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Controller
|
+--CIM_PCIController
|
+--CIM_PCIDevice
|
+--CIM_PCIBridge

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of a PCI controller that provide bridge-to-bridge capability.
UMLPackagePath | string | CIM::Device::Controller
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
BridgeType | uint16 |
Description | string | The type of bridge. Except for "Host" (value=0) and "PCIe-to-PCI" (value=10), the type of bridge is PCI-to-<value>. For type "Host", the device is a Host-to-PCI bridge. For type "PCIe-to-PCI", the device is a PCI Express-to-PCI bridge.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 128, ..
Values | string | Host, ISA, EISA, Micro Channel, PCI, PCMCIA, NuBus, CardBus, RACEway, AGP, PCIe, PCIe-to-PCI, Other, DMTF Reserved
IOBase | uint8 |
Description | string | Base address of I/O addresses supported by the bus. The upper 4 bits of this property specify the address bits, AD[15::12], of the I/O address. Each of the remaining 12 bits of the I/O address are assumed to be 0.
IOBaseUpper16 | uint16 |
Description | string | Upper 16 bits of the supported I/O base address when 32-bit I/O addressing is used. The lower 16 bits are assumed to be 0.
IOLimit | uint8 |
Description | string | End address of the I/O addresses supported by the bus. The upper 4 bits of this property specify the address bits, AD[15::12], of the I/O address. Each of the remaining 12 bits of the I/O address are assumed to be 1.
IOLimitUpper16 | uint16 |
Description | string | Upper 16 bits of the supported I/O end address when 32-bit I/O addressing is used. The lower 16 bits are each assumed to be 1.
MemoryBase | uint16 |
Description | string | Base address of the memory supported by the bus. The upper 12 bits of this property specify the address bits, AD[31::20], of a 32-bit memory address. Each of the remaining 20 bits of the address are assumed to be 0.
MemoryLimit | uint16 |
Description | string | End address of the memory supported by the bus. The upper 12 bits of this property specify the address bits, AD[31::20], of a 32-bit memory address. Each of the remaining 20 bits of the address are assumed to be 1.
PrefetchBaseUpper32 | uint32 |
Description | string | Upper 32 bits of the supported prefetch base address when 64-bit addressing is used. The lower 32 bits are assumed to be 0.
PrefetchLimitUpper32 | uint32 |
Description | string | Upper 32 bits of the supported prefetch end address when 64-bit addressing is used. The lower 32 bits are each assumed to be 1.
PrefetchMemoryBase | uint16 |
Description | string | Base address of the memory that can be prefetched by the bus. The upper 12 bits of this property specify the address bits, AD[31::20], of a 32-bit memory address. Each of the remaining 20 bits of the address are assumed to be 0.
PrefetchMemoryLimit | uint16 |
Description | string | End address of the memory that can be prefetched by the bus. The upper 12 bits of this property specify the address bits, AD[31::20], of a 32-bit memory address. Each of the remaining 20 bits of the address are assumed to be 1.
PrimaryBusNumber | uint8 |
Description | string | The number of the PCI bus segment to which the primary interface of the bridge is connected.
SecondaryBusDeviceSelectTiming | uint16 |
Description | string | The slowest device-select timing for a target device on the secondary bus.
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Unknown, Other, Fast, Medium, Slow, DMTF Reserved
SecondaryLatencyTimer | uint8 |
Description | string | The timeslice for the secondary interface when the bridge is acting as an initiator. A 0 value indicates no requirement.
PUnit | string | cycle
Units | string | PCI clock cycles
SecondaryStatusRegister | uint16 |
Description | string | The contents of the SecondaryStatusRegister of the Bridge. For more information on the contents of this register, refer to the PCI-to-PCI Bridge Architecture Specification.
SecondayBusNumber | uint8 |
Description | string | The number of the PCI bus segment to which the secondary interface of the bridge is connected.
SubordinateBusNumber | uint8 |
Description | string | The number of the highest numbered bus that exists behind the bridge.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Availability | uint16 | CIM_LogicalDevice
BusNumber | uint8 | CIM_PCIDevice
CacheLineSize | uint8 | CIM_PCIController
Caption | string | CIM_ManagedElement
ClassCode | uint8 | CIM_PCIController
CommandRegister | uint16 | CIM_PCIController
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
DeviceNumber | uint8 | CIM_PCIDevice
DeviceSelectTiming | uint16 | CIM_PCIController
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
ExpansionROMBaseAddress | uint32 | CIM_PCIController
FunctionNumber | uint8 | CIM_PCIDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
InterruptPin | uint16 | CIM_PCIController
LastErrorCode | uint32 | CIM_LogicalDevice
LatencyTimer | uint8 | CIM_PCIController
LocationIndicator | uint16 | CIM_LogicalDevice
MaxLatency | uint8 | CIM_PCIDevice
MaxNumberControlled | uint32 | CIM_Controller
MaxQuiesceTime | uint64 | CIM_LogicalDevice
MinGrantTime | uint8 | CIM_PCIDevice
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PCIDeviceID | uint16 | CIM_PCIDevice
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolDescription | string | CIM_Controller
ProtocolSupported | uint16 | CIM_Controller
RequestedState | uint16 | CIM_EnabledLogicalElement
RevisionID | uint8 | CIM_PCIDevice
SelfTestEnabled | boolean | CIM_PCIController
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SubsystemID | uint16 | CIM_PCIDevice
SubsystemVendorID | uint16 | CIM_PCIDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastReset | datetime | CIM_Controller
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
VendorID | uint16 | CIM_PCIDevice
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
BaseAddress | uint32[] | CIM_PCIDevice
BaseAddress64 | uint64[] | CIM_PCIDevice
Capabilities | uint16[] | CIM_PCIController
CapabilityDescriptions | string[] | CIM_PCIController
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
BISTExecution | uint8 | CIM_PCIController
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice