# Class CIM_LACPPortStatistics
extends CIM_StatisticalData

Statistics for Link Aggregation Control Protocol (LACP). These statistics are for each LAGPort8023ad where LACP is enabled in a device.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalData
|
+--CIM_LACPPortStatistics

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Statistics for Link Aggregation Control Protocol (LACP). These statistics are for each LAGPort8023ad where LACP is enabled in a device.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::8023LAG
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
PortStatsIllegalRx | uint32 |
Counter | boolean | true
Description | string | The number of frames received that carry the Slow Protocols Ethernet Type value (43B.4), but contain a badly formed PDU or an illegal value of Protocol Subtype (43B.4).
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortStatsIllegalRx
PortStatsLACPDUsRx | uint32 |
Counter | boolean | true
Description | string | The number of valid LACPDUs received on this Aggregation Port.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortStatsLACPDUsRx
PortStatsLACPDUsTx | uint32 |
Counter | boolean | true
Description | string | The number of LACPDUs transmitted on this Aggregation Port.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortStatsLACPDUsTx
PortStatsMarkerPDUsRx | uint32 |
Counter | boolean | true
Description | string | The number of valid Marker PDUs received on this Aggregation Port.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortStatsMarkerPDUsRx
PortStatsMarkerPDUsTx | uint32 |
Counter | boolean | true
Description | string | The number of Marker PDUs transmitted on thisAggregation Port.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortStatsMarkerPDUsTx
PortStatsMarkerResponsePDUsRx | uint32 |
Counter | boolean | true
Description | string | The number of valid Marker Response PDUs received on this Aggregation Port.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortStatsMarkerResponsePDUsRx
PortStatsMarkerResponsePDUsTx | uint32 |
Counter | boolean | true
Description | string | The number of Marker Response PDUs transmitted on this Aggregation Port.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortStatsMarkerResponsePDUsTx
PortStatsUnknownRx | uint32 |
Counter | boolean | true
Description | string | The number of frames received that either: * carry the Slow Protocols Ethernet Type value (43B.4), but contain an unknown PDU, or: * are addressed to the Slow Protocols group MAC Address (43B.3), but do not carry the Slow Protocols Ethernet Type.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortStatsUnknownRx

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_StatisticalData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_StatisticalData
SampleInterval | datetime | CIM_StatisticalData
StartStatisticTime | datetime | CIM_StatisticalData
StatisticTime | datetime | CIM_StatisticalData

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ResetSelectedStats | uint32 | CIM_StatisticalData