# Class CIM_EthernetNICDiagnosticTest
extends CIM_DiagnosticTest

This class specializes CIM_DiagnosticTest to define the tests specific to Ethernet NICs.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_DiagnosticService
|
+--CIM_DiagnosticTest
|
+--CIM_EthernetNICDiagnosticTest

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class specializes CIM_DiagnosticTest to define the tests specific to Ethernet NICs.
Experimental | boolean | true
UMLPackagePath | string | CIM::System::Diagnostics
Version | string | 2.28.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
EthernetNICTestType | uint16 |
Description | string | The descriptions for each Ethernet NIC test type are below: * "MAC Register" (value=2) is specified for the tests that verify the functionality of the general CPU instruction. CIM_DiagnosticTest.TestTypes shall be set to "Functional" (value=2). * "Physical Register" (value=3) is specified for the tests that verify the functionality of the FPU instructions. CIM_DiagnosticTest.TestTypes shall be set to "Functional" (value=2). * "Internal Loopback" (value=4) is specified for the tests that verify that all internal data paths of an Ethernet NIC is working properly. CIM_DiagnosticTest.TestTypes shall be set to "Functional" (value=2). * "External Loopback" (value=5) is specified for the tests that verify that all external data paths of an Ethernet NIC is working properly. CIM_DiagnosticTest.TestTypes shall be set to "Access Test" (value=5). * "Beacon" (value=6) is specified for the tests that cause at least one of the LEDs of a Ethernet NIC to flash on and off. CIM_DiagnosticTest.TestTypes shall be set to "Functional" (value=2). * "Self" (value=7) is specified for the tests that verify the functionality of all possible components of the Ethernet NIC CIM_DiagnosticTest.TestTypes shall be set to "Functional" (value=2). * "Status" (value=8) is specified for the tests that verify the healthof the Ethernet NIC. CIM_DiagnosticTest.TestTypes shall be set to "Health Check" (value=4). * "Ping" (value=9) is specified for the tests that verify access to the network. CIM_DiagnosticTest.TestTypes shall be set to "Stress" (value=3). * "Embedded Processor" (value=10) is specified for the tests that verify functionality of the embedded processor. CIM_DiagnosticTest.TestTypes shall be set to "Functional" (value=2). * "IRQ" (value=11) is specified for the tests that verify functionality of raising interrupts. CIM_DiagnosticTest.TestTypes shall be set to "Functional" (value=2)."
ModelCorrespondence | string | CIM_EthernetNICDiagnosticTest.OtherEthernetNICTestTypeDescription
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, .., 0x8000..
Values | string | Unknown, Other, MAC Register, Physical Register, Internal Loopback, External Loopback, Beacon, Self, Status, Ping, Embedded Processor, IRQ, DMTF Reserved, Vendor Reserved
OtherEthernetNICTestTypeDescription | string |
Description | string | A string that describes the test when the EthernetNICTestType property is set to 1 ("Other"). This property must be set to null when EthernetNICTestType is any value other than 1.
ModelCorrespondence | string | CIM_EthernetNICDiagnosticTest.EthernetNICTestType

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsInUse | boolean | CIM_DiagnosticTest
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherCharacteristicDescription | string | CIM_DiagnosticTest
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
Characteristics | uint16[] | CIM_DiagnosticTest
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherCharacteristicsDescriptions | string[] | CIM_DiagnosticTest
OtherTestTypesDescriptions | string[] | CIM_DiagnosticTest
ResourcesUsed | uint16[] | CIM_DiagnosticTest
StatusDescriptions | string[] | CIM_ManagedSystemElement
TestTypes | uint16[] | CIM_DiagnosticTest

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
ClearResults | uint32 | CIM_DiagnosticTest
DiscontinueTest | uint32 | CIM_DiagnosticTest
RequestStateChange | uint32 | CIM_EnabledLogicalElement
RunDiagnostic | uint32 | CIM_DiagnosticService
RunDiagnosticService | uint32 | CIM_DiagnosticService
RunTest | uint32 | CIM_DiagnosticTest
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service