# Class CIM_PhysicalComputerSystemView
extends CIM_View

This class defines a view class for a physical computer system.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_View
|
+--CIM_PhysicalComputerSystemView

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class defines a view class for a physical computer system.
Experimental | boolean | true
UMLPackagePath | string | CIM::Core::CoreElements
Version | string | 2.30.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CurrentBIOSBuildNumber | uint16 |
Description | string | The build number component of the current BIOS version information.
ModelCorrespondence | string | CIM_SoftwareIdentity.BuildNumber
CurrentBIOSMajorVersion | uint16 |
Description | string | The major number component of the current BIOS version information.
ModelCorrespondence | string | CIM_SoftwareIdentity.MajorVersion
CurrentBIOSMinorVersion | uint16 |
Description | string | The minor number component of the current BIOS version information.
ModelCorrespondence | string | CIM_SoftwareIdentity.MinorVersion
CurrentBIOSRevisionNumber | uint16 |
Description | string | The revision number component of the current BIOS version information.
ModelCorrespondence | string | CIM_SoftwareIdentity.RevisionNumber
CurrentBIOSVersionString | string |
Description | string | The BIOS version information in string format.
ModelCorrespondence | string | CIM_SoftwareIdentity.VersionString
CurrentManagementFirmwareBuildNumber | uint16 |
Description | string | The build number component of the version information for the current management firmware on this physical computer system.
ModelCorrespondence | string | CIM_SoftwareIdentity.BuildNumber
CurrentManagementFirmwareElementName | string |
Description | string | The user-friendly name for the current management firmware on this physical computer system.
ModelCorrespondence | string | CIM_SoftwareIdentity.ElementName
CurrentManagementFirmwareMajorVersion | uint16 |
Description | string | The major number component of the version information for the current management firmware on this physical computer system.
ModelCorrespondence | string | CIM_SoftwareIdentity.MajorVersion
CurrentManagementFirmwareMinorVersion | uint16 |
Description | string | The minor number component of the version information for the current management firmware on this physical computer system.
ModelCorrespondence | string | CIM_SoftwareIdentity.MinorVersion
CurrentManagementFirmwareRevisionNumber | uint16 |
Description | string | The revision number component of the version information for the current management firmware on this physical computer system.
ModelCorrespondence | string | CIM_SoftwareIdentity.RevisionNumber
CurrentManagementFirmwareVersionString | string |
Description | string | The version string for the current management firmware on this physical computer system.
ModelCorrespondence | string | CIM_SoftwareIdentity.VersionString
EnabledState | uint16 |
Description | string | This property corresponds to the EnabledState property of the underlying physical computer system represented by CIM_ComputerSystem. See CIM_EnabledLogicalElement.EnabledState for details on EnabledState.
ModelCorrespondence | string | CIM_ComputerSystem.EnabledState
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11..32767, 32768..65535
Values | string | Unknown, Other, Enabled, Disabled, Shutting Down, Not Applicable, Enabled but Offline, In Test, Deferred, Quiesce, Starting, DMTF Reserved, Vendor Reserved
FRUInfoSupported | boolean |
Description | string | This property indicates the availability of the FRU Information on this physical computer system. See CIM_PhysicalAssetCapabilities.FRUInfoSupported for details.
ModelCorrespondence | string | CIM_PhysicalAssetCapabilities.FRUInfoSupported
HealthState | uint16 |
Description | string | This property corresponds to the HealthState property of the underlying physical computer system represented by CIM_ComputerSystem. See CIM_ManagedSystemElement.HealthState for details.
ModelCorrespondence | string | CIM_ComputerSystem.HealthState
ValueMap | string | 0, 5, 10, 15, 20, 25, 30, .., 32768..65535
Values | string | Unknown, OK, Degraded/Warning, Minor failure, Major failure, Critical failure, Non-recoverable error, DMTF Reserved, Vendor Specific
InstanceID | string |
Description | string | InstanceID is the property that may be used to opaquely and uniquely identify an instance of this class within the scope of the instantiating Namespace.
Key | boolean | true
Override | string | InstanceID
Manufacturer | string |
Description | string | The name of the organization responsible for producing the physical computer system.
ModelCorrespondence | string | CIM_PhysicalElement.Manufacturer
MemoryBlockSize | uint64 |
Description | string | See CIM_Memory.BlockSize for details.
ModelCorrespondence | string | CIM_Memory.BlockSize
MemoryConsumableBlocks | uint64 |
Description | string | See CIM_Memory.ConsumableBlocks for details.
ModelCorrespondence | string | CIM_Memory.ConsumableBlocks
MemoryNumberOfBlocks | uint64 |
Description | string | See CIM_Memory.NumberOfBlocks for details.
ModelCorrespondence | string | CIM_Memory.NumberOfBlocks
Model | string |
Description | string | The name by which the physical computer system is known.
ModelCorrespondence | string | CIM_PhysicalElement.Model
NumberOfProcessorCores | uint16 |
Description | string | See CIM_ProcessorCapabilities.NumberOfProcessorCores for details.
ModelCorrespondence | string | CIM_ProcessorCapabilities.NumberOfProcessorCores
NumberOfProcessors | uint16 |
Description | string | This property identifies the number of processors on this physical computer system.
NumberOfProcessorThreads | uint16 |
Description | string | See CIM_ProcessorCapabilities.NumberOfProcessorThreads for details.
ModelCorrespondence | string | CIM_ProcessorCapabilities.NumberOfProcessorThreads
OneTimeBootSource | uint8 |
Description | string | This property identifies the boot source that is used for the next one-time boot. The value of this property is an index referencing an element in the array of StructuredBootString.
OSEnabledState | uint16 |
Description | string | EnabledState of the current or last running operating system on this physcial computer system.
ModelCorrespondence | string | CIM_OperatingSystem.EnabledState
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11..32767, 32768..65535
Values | string | Unknown, Other, Enabled, Disabled, Shutting Down, Not Applicable, Enabled but Offline, In Test, Deferred, Quiesce, Starting, DMTF Reserved, Vendor Reserved
OSType | uint16 |
Description | string | Type information of the current or last running operating system on this physical computer system. See CIM_OperatingSystem.OSType for details.
ModelCorrespondence | string | CIM_OperatingSystem.OSType
OSVersion | string |
Description | string | Version information of the current or last running operating system on this physical computer system. See CIM_OperatingSystem.Version for details.
ModelCorrespondence | string | CIM_OperatingSystem.Version
PartNumber | string |
Description | string | The part number assigned by the organization that is responsible for producing the physical computer system.
ModelCorrespondence | string | CIM_PhysicalElement.PartNumber
PowerAllocationLimit | uint64 |
Description | string | This property specifies the maximum amount of power this computer system can consume.
ModelCorrespondence | string | CIM_PowerAllocationSettingData.Limit
PUnit | string | watt * 10^-3
PowerUtilizationMode | uint16 |
Description | string | This property corresponds to the PowerUtilizationMode of the CIM_PowerUtilizationManagementService. See CIM_PowerUtilizationManagementService.PowerUtilizationMode for details.
ModelCorrespondence | string | CIM_PowerUtilizationManagementService.PowerUtilizationMode
ValueMap | string | 2, 3, 4, .., 32768..65535
Values | string | None, Dynamic, Static, DMTF Reserved, Vendor Reserved
ProcessorFamily | uint16 |
Description | string | See CIM_Processor.Family for details.
ModelCorrespondence | string | CIM_Processor.Family
ProcessorMaxClockSpeed | uint32 |
Description | string | See CIM_Processor.MaxClockSpeed for details.
ModelCorrespondence | string | CIM_Processor.MaxClockSpeed
RequestedState | uint16 |
Description | string | This property corresponds to the RequestedState property of the underlying physical computer system represented by CIM_ComputerSystem. See CIM_EnabledLogicalElement.RequestedState for details on RequestedState.
ModelCorrespondence | string | CIM_ComputerSystem.RequestedState
ValueMap | string | 0, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, .., 32768..65535
Values | string | Unknown, Enabled, Disabled, Shut Down, No Change, Offline, Test, Deferred, Quiesce, Reboot, Reset, Not Applicable, DMTF Reserved, Vendor Reserved
SerialNumber | string |
Description | string | A manufacturer-allocated number used to identify the physical computer system.
ModelCorrespondence | string | CIM_PhysicalElement.SerialNumber
SKU | string |
Description | string | The stock-keeping unit number for the physical computer system.
ModelCorrespondence | string | CIM_PhysicalElement.SKU
Tag | string |
Description | string | This property uniquely identifies the physical computer system. It corresponds to CIM_PhysicalElement.Tag. See CIM_PhysicalElement.Tag for details.
ModelCorrespondence | string | CIM_PhysicalElement.Tag
Version | string |
Description | string | The version of the physical computer system.
ModelCorrespondence | string | CIM_PhysicalElement.Version
LogCurrentNumberOfRecords | uint64[] |
ArrayType | string | Indexed
Description | string | See CIM_RecordLog.CurrentNumberOfRecords for details.
ModelCorrespondence | string | CIM_RecordLog.CurrentNumberOfRecords, CIM_PhysicalComputerSystemView.LogInstanceID, CIM_PhysicalComputerSystemView.LogMaxNumberOfRecords
LogInstanceID | string[] |
ArrayType | string | Indexed
Description | string | This property represents the identifiers for the underlying logs on this physical computer system. See CIM_RecordLog.InstanceID for details.
ModelCorrespondence | string | CIM_RecordLog.InstanceID
LogMaxNumberOfRecords | uint64[] |
ArrayType | string | Indexed
Description | string | See CIM_RecordLog.MaxNumberOfRecords for details.
ModelCorrespondence | string | CIM_RecordLog.MaxNumberOfRecords, CIM_PhysicalComputerSystemView.LogInstanceID
LogOvewWritePolicy | uint16[] |
ArrayType | string | Indexed
Description | string | See CIM_RecordLog.OverWritePolicy for details.
ModelCorrespondence | string | CIM_RecordLog.OverWritePolicy, CIM_PhysicalComputerSystemView.LogInstanceID, CIM_PhysicalComputerSystemView.LogMaxNumberOfRecords, CIM_PhysicalComputerSystemView.LogCurrentNumberOfRecords
ValueMap | string | 0, 2, 7, .., 32768..65535
Values | string | Unknown, Wraps When Full, Never Overwrites, DMTF Reserved, Vendor Reserved
LogState | uint16[] |
ArrayType | string | Indexed
Description | string | See CIM_RecordLog.LogState for details.
ModelCorrespondence | string | CIM_RecordLog.LogState, CIM_PhysicalComputerSystemView.LogInstanceID, CIM_PhysicalComputerSystemView.MaxNumberOfRecords, CIM_PhysicalComputerSystemView.CurrentNumberOfRecords, CIM_PhysicalComputerSystemView.OvewWritePolicy
ValueMap | string | 0, 2, 3, 4, .., 32768..65535
Values | string | Unknown, Normal, Erasing, Not Applicable, DMTF Reserved, Vendor Reserved
NumericSensorBaseUnits | uint16[] |
ArrayType | string | Indexed
Description | string | Base units of the values returned by the numeric sensors. See CIM_NumericSensor.BaseUnits for details.
ModelCorrespondence | string | CIM_NumericSensor.BaseUnits, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64, 65, 66
Values | string | Unknown, Other, Degrees C, Degrees F, Degrees K, Volts, Amps, Watts, Joules, Coulombs, VA, Nits, Lumens, Lux, Candelas, kPa, PSI, Newtons, CFM, RPM, Hertz, Seconds, Minutes, Hours, Days, Weeks, Mils, Inches, Feet, Cubic Inches, Cubic Feet, Meters, Cubic Centimeters, Cubic Meters, Liters, Fluid Ounces, Radians, Steradians, Revolutions, Cycles, Gravities, Ounces, Pounds, Foot-Pounds, Ounce-Inches, Gauss, Gilberts, Henries, Farads, Ohms, Siemens, Moles, Becquerels, PPM (parts/million), Decibels, DbA, DbC, Grays, Sieverts, Color Temperature Degrees K, Bits, Bytes, Words (data), DoubleWords, QuadWords, Percentage, Pascals
NumericSensorCurrentReading | sint32[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.CurrentReading for details.
ModelCorrespondence | string | CIM_NumericSensor.CurrentReading, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits
NumericSensorCurrentState | string[] |
ArrayType | string | Indexed
Description | string | Current states of numeric sensors. See CIM_NumericSensor.CurrentState for details.
ModelCorrespondence | string | CIM_NumericSensor.CurrentState, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState
NumericSensorElementName | string[] |
ArrayType | string | Indexed
Description | string | User-friendly names of the numeric sensors on the computer system. See CIM_NumericSensor.ElementName for details.
ModelCorrespondence | string | CIM_NumericSensor.ElementName
NumericSensorEnabledState | uint16[] |
ArrayType | string | Indexed
Description | string | States of numeric sensors. See CIM_NumericSensor.EnabledState for details.
ModelCorrespondence | string | CIM_NumericSensor.EnabledState, CIM_PhysicalComputerSystemView.NumericSensorElementName
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11..32767, 32768..65535
Values | string | Unknown, Other, Enabled, Disabled, Shutting Down, Not Applicable, Enabled but Offline, In Test, Deferred, Quiesce, Starting, DMTF Reserved, Vendor Reserved
NumericSensorHealthState | uint16[] |
ArrayType | string | Indexed
Description | string | Health states of numeric sensors. See CIM_NumericSensor.HealthState for details.
ModelCorrespondence | string | CIM_NumericSensor.HealthState, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState
ValueMap | string | 0, 5, 10, 15, 20, 25, 30, .., 32768..65535
Values | string | Unknown, OK, Degraded/Warning, Minor failure, Major failure, Critical failure, Non-recoverable error, DMTF Reserved, Vendor Specific
NumericSensorOtherSensorTypeDescription | string[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.OtherSensorTypeDescription for details.
ModelCorrespondence | string | CIM_NumericSensor.OtherSensorTypeDescription, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading, CIM_PhysicalComputerSystemView.NumericSensorSensorType
NumericSensorPrimaryStatus | uint16[] |
ArrayType | string | Indexed
Description | string | Primary statuses of numeric sensors. See CIM_NumericSensor.PrimaryStatus for details.
ModelCorrespondence | string | CIM_NumericSensor.PrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState
ValueMap | string | 0, 1, 2, 3, .., 0x8000..
Values | string | Unknown, OK, Degraded, Error, DMTF Reserved, Vendor Reserved
NumericSensorRateUnits | uint16[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.RateUnits for details.
ModelCorrespondence | string | CIM_NumericSensor.RateUnits, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9
Values | string | None, Per MicroSecond, Per MilliSecond, Per Second, Per Minute, Per Hour, Per Day, Per Week, Per Month, Per Year
NumericSensorSensorType | uint16[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.SensorType for details.
ModelCorrespondence | string | CIM_NumericSensor.SensorType, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, .., 32768..65535
Values | string | Unknown, Other, Temperature, Voltage, Current, Tachometer, Counter, Switch, Lock, Humidity, Smoke Detection, Presence, Air Flow, Power Consumption, Power Production, Pressure, DMTF Reserved, Vendor Reserved
NumericSensorUnitModifier | sint32[] |
ArrayType | string | Indexed
Description | string | Unit modifiers for the values returned by the numeric sensors. See CIM_NumericSensor.UnitModifier description for details.
ModelCorrespondence | string | CIM_NumericSensor.UnitModifier, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits
NumericSensorUpperThresholdCritical | sint32[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.UpperThresholdCritical description for details.
ModelCorrespondence | string | CIM_NumericSensor.UpperThresholdCritical, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading, CIM_PhysicalComputerSystemView.NumericSensorSensorType, CIM_PhysicalComputerSystemView.NumericSensorOtherSensorTypeDescription, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdNonCritical
NumericSensorUpperThresholdFatal | sint32[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.UpperThresholdFatal for details.
ModelCorrespondence | string | CIM_NumericSensor.UpperThresholdFatal, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading, CIM_PhysicalComputerSystemView.NumericSensorSensorType, CIM_PhysicalComputerSystemView.NumericSensorOtherSensorTypeDescription, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdNonCritical, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdCritical
NumericSensorUpperThresholdNonCritical | sint32[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.UpperThresholdNonCritical for details.
ModelCorrespondence | string | CIM_NumericSensor.UpperThresholdNonCritical, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading, CIM_PhysicalComputerSystemView.NumericSensorSensorType, CIM_PhysicalComputerSystemView.NumericSensorOtherSensorTypeDescription
OperationalStatus | uint16[] |
Description | string | This property corresponds to the OperationalStatus property of the underlying physical computer system represented by CIM_ComputerSystem. See CIM_ManagedSystemElement.OperationalStatus Description for details.
ModelCorrespondence | string | CIM_ComputerSystem.OperationalStatus
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, .., 0x8000..
Values | string | Unknown, Other, OK, Degraded, Stressed, Predictive Failure, Error, Non-Recoverable Error, Starting, Stopping, Stopped, In Service, No Contact, Lost Communication, Aborted, Dormant, Supporting Entity in Error, Completed, Power Mode, Relocating, DMTF Reserved, Vendor Reserved
PersistentBootConfigOrder | uint8[] |
ArrayType | string | Ordered
Description | string | An array of elements identifying the boot order of the persistent boot configuration that is currently in use on this physical computer system. The value of each element in this array is an index referencing an element in the array of StructuredBootString.
PowerUtilizationModesSupported | uint16[] |
Description | string | This property corresponds to PowerUtilizationModesSupported property of CIM_PowerUtilizationManagementCapabilities. See CIM_PowerUtilizationManagementCapabilities.PowerUtilizationModesSupported for details.
ModelCorrespondence | string | CIM_PowerUtilizationManagementCapabilities.PowerUtilizationModesSupported
ValueMap | string | 3, 4, .., 32768..65535
Values | string | Dynamic, Static, DMTF Reserved, Vendor Reserved
StructuredBootString | string[] |
Description | string | Strings identifying the boot sources on this physical computer system. See CIM_BootSourceSetting.StructuredBootString description for details.
ModelCorrespondence | string | CIM_BootSourceSetting.StructuredBootString

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement

## Class Methods

### Local Class Methods

#### RequestStateChange (uint32)

#### Method Qualifiers (RequestStateChange)

Name | Data Type | Value
--- | --- | ---
Description | string | An extrinsic method for changing the state of this physical computer system. Requests that the state of the element be changed to the value specified in the RequestedState parameter. When the requested state change takes place, the EnabledState and RequestedState of the element will be the same. Invoking the RequestStateChange method multiple times could result in earlier requests being overwritten or lost. A return code of 0 shall indicate the state change was successfully initiated. A return code of 1 shall indicate that the method is not supported. A return code of 2 shall indicate that the method failed.
ValueMap | string | 0, 1, 2, 4096, .., 32768..65535
Values | string | Completed with No Error, Not Supported, Failed, Job Started, DMTF Reserved, Vendor Reserved

#### Method Parameters (RequestStateChange)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
RequestedState | uint16
Description | string | See CIM_ComputerSystem.RequestedStateChange.RequestedState for details.
In | boolean | true
ModelCorrespondence | string | CIM_ComputerSystem.RequestedStateChange.RequestedState
ValueMap | string | 2, 3, 4, 6, 7, 8, 9, 10, 11, .., 32768..65535
Values | string | Enabled, Disabled, Shut Down, Offline, Test, Defer, Quiesce, Reboot, Reset, DMTF Reserved, Vendor Reserved
TimeoutPeriod | datetime
Description | string | See CIM_ComputerSystem.TimeoutPeriod for details.
In | boolean | true
ModelCorrespondence | string | CIM_ComputerSystem.RequestedStateChange.TimeoutPeriod
Job | REF CIM_ConcreteJob
Description | string | May contain a reference to the ConcreteJob created to track the state transition initiated by the method invocation.
In | boolean | false
Out | boolean | true

#### ClearLog (uint32)

#### Method Qualifiers (ClearLog)

Name | Data Type | Value
--- | --- | ---
Description | string | An extrinsic method for clearing a log on this physical computer system.
ValueMap | string | 0, 1, 2, .., 32768..65535
Values | string | Completed with No Error, Not Supported, Failed, DMTF Reserved, Vendor Reserved

#### Method Parameters (ClearLog)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
LogInstanceID | string
Description | string | Idenfier for the log that is requested to be cleared.
In | boolean | true
ModelCorrespondence | string | CIM_RecordLog.InstanceID, CIM_PhysicalComputerSystemView.LogInstanceID

#### InstallSoftwareFromURI (uint32)

#### Method Qualifiers (InstallSoftwareFromURI)

Name | Data Type | Value
--- | --- | ---
Description | string | An extrinsic method for installing software on this physical computer system.
ValueMap | string | 0, 1, 2, 4096, .., 32768..65535
Values | string | Completed with No Error, Not Supported, Failed, Job Started, DMTF Reserved, Vendor Reserved

#### Method Parameters (InstallSoftwareFromURI)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
URI | string
Description | string | See CIM_SoftwareInstallationService.InstallFromURI.URI for details.
In | boolean | true
ModelCorrespondence | string | CIM_SoftwareInstallationService.InstallFromURI.URI
InstallOptions | uint16[]
ArrayType | string | Indexed
Description | string | See CIM_SoftwareInstallationService.InstallFromURI.InstallOptions for details.
In | boolean | true
ModelCorrespondence | string | CIM_SoftwareInstallationService.InstallFromURI.InstallOptions, CIM_PhysicalComputerSystemView.InstallSoftwareFromURI.InstallOptionsValues
ValueMap | string | 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, .., 32768..65535
Values | string | Defer target/system reset, Force installation, Install, Update, Repair, Reboot, Password, Uninstall, Log, SilentMode, AdministrativeMode, ScheduleInstallAt, DMTF Reserved, Vendor Specific
InstallOptionsValues | string[]
ArrayType | string | Indexed
Description | string | See CIM_SoftwareInstallationService.InstallFromURI.InstallOptionsValues for details.
In | boolean | true
ModelCorrespondence | string | CIM_SoftwareInstallationService.InstallFromURI.InstallOptionsValues, CIM_PhysicalComputerSystemView.InstallSoftwareFromURI.InstallOptions
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be null if job completed).
In | boolean | false
Out | boolean | true