# Class CIM_PrintInputTray
extends CIM_PrinterElement

This class represents the PrintInputTray component of a Printer (print device). It contains properties that describe a device capable of providing media for input to the printing process. Note: A PrintInputTray shall be associated with exactly one Printer via an instance of the PrinterComponent class. See: Model in section 2 of Printer MIB (RFC 3805).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_PrinterElement
|
+--CIM_PrintInputTray

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class represents the PrintInputTray component of a Printer (print device). It contains properties that describe a device capable of providing media for input to the printing process. Note: A PrintInputTray shall be associated with exactly one Printer via an instance of the PrinterComponent class. See: Model in section 2 of Printer MIB (RFC 3805).
Experimental | boolean | true
MappingStrings | string | MIB.IETF|Printer-MIB.prtInputEntry
UMLPackagePath | string | CIM::Device::Printing
Version | string | 2.25.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AvailabilityStatus | uint32 |
Description | string | This property contains detailed availability information for this PrintInputTray, as follows: 1 (Other) means other detailed availability information is present in the OtherAvailabilityStatus property. 2 (Unknown) means detailed availability information for this PrintInputTray is unknown. 3 (AvailableIdle) means this PrintInputTray is available and idle, i.e., not currently in use. 4 (AvailableStandy) means this PrintInputTray is available but on standby, e.g., in a power saving mode. 5 (AvailableActive) means this PrintInputTray is available and active, i.e., currently in use. 6 (AvailableBusy) means this PrintInputTray is available but busy, i.e., not immediately available for its primary function. 7 (UnavailableOnRequest) means this PrintInputTray is not available and is on request, i.e., needs human intervention. 8 (UnavailableBroken) means this PrintInputTray is not available and is broken, e.g., needs repair/replacement.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.OperatingStatus, CIM_PrintInputTray.OtherAvailabilityStatus
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, ..
Values | string | Other, Unknown, AvailableIdle, AvailableStandby, AvailableActive, AvailableBusy, UnavailableOnRequest, UnavailableBroken, DMTF Reserved
CapacityUnit | uint32 |
Description | string | The unit of measurement for use in calculating and relaying capacity values for this input tray.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInputCapacityUnit, MIB.IETF|Printer-MIB.PrtCapacityUnitTC
ModelCorrespondence | string | CIM_PrintInputTray.OtherCapacityUnit
ValueMap | string | 1, 2, 3, 4, 8, 16, 17, 18, 19, ..
Values | string | Other, Unknown, TenThousandthsOfInches, Micrometers, Sheets, Feet, Meters, Items, Percent, DMTF Reserved
CriticalAlertsPresent | boolean |
Description | string | If true, there are currently critical alerts on this input tray.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.DetailedStatus
CurrentLevel | uint32 |
Description | string | The current level of the input tray in units specified by CIM_PrintInputTray.CapacityUnit. If this input tray can reliably sense this value, the value is sensed by the input tray and cannot be changed by the system administrator; otherwise, the value may be changed out-of-band by the system administrator.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInputCurrentLevel, MIB.IETF|Printer-MIB.prtInputCapacityUnit, MIB.IETF|Printer-MIB.PrtCapacityUnitTC
MaxValue | sint64 | 2147483647
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_PrintInputTray.CurrentLevelBasis
CurrentLevelBasis | uint16 |
Description | string | The basis for the gauge property CurrentLevel, that specifies whether a meaningful value is available. 1 (Other) means the input tray places no restrictions on capacity and CurrentLevel shall be null. 2 (Unknown) means the input tray cannot sense a meaningful value and CurrentLevel shall be null. 3 (Actual) means the input tray can sense a meaningful value and CurrentLevel shall be present. 4 (AtLeastOne) means that the input tray can only sense that at least one capacity unit remains (i.e., not empty) and CurrentLevel shall be present and shall contain the value zero or one.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInputCurrentLevel
ModelCorrespondence | string | CIM_PrintInputTray.CurrentLevel
ValueMap | string | 1, 2, 3, 4, ..
Values | string | Other, Unknown, Actual, AtLeastOne, DMTF Reserved
ElementName | string |
Description | string | The user-friendly name for this instance of PrintInputTray. In addition, the user-friendly name can be used as an index property for a search or query. (Note: The name does not have to be unique within a namespace.) This name shall be generated as a factory default by the manufacturer and may be changed out-of-band to a site-specific name by the system administrator.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInputName
ModelCorrespondence | string | CIM_ManagedElement.ElementName
Override | string | ElementName
Required | boolean | true
IsDefault | boolean |
Description | string | Denotes whether or not this PrintInputTray is the default PrintInputTray for this Printer. If the default PrintInputTray feature is not supported for this Printer, then this property shall be null. If the default PrintInputTray feature is supported for this Printer, then this property shall be true for at most one instance of CIM_PrintInputTray on this Printer, i.e., the default may not be currently configured.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInputDefaultIndex
LocalizedDescription | string |
Description | string | A free-form text description of this input tray in the localization specified by CIM_Printer.CurrentNaturalLanguage.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInputDescription, MIB.IETF|Printer-MIB.PrtLocalizedDescriptionStringTC
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_Printer.CurrentNaturalLanguage
MaxCapacity | uint32 |
Description | string | The maximum capacity of the input tray in units specified by CIM_PrintInputTray.CapacityUnit. There is no convention associated with the media itself so this value reflects claimed capacity. If this input tray can reliably sense this value, the value is sensed by the input tray and cannot be changed by the system administrator; otherwise, the value may be changed out-of-band by the system administrator.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInputMaxCapacity, MIB.IETF|Printer-MIB.prtInputCapacityUnit, MIB.IETF|Printer-MIB.PrtCapacityUnitTC
MaxValue | sint64 | 2147483647
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_PrintInputTray.MaxCapacityBasis
MaxCapacityBasis | uint16 |
Description | string | The basis for the limit property MaxCapacity, that specifies whether a meaningful value is available. 1 (Other) means the input tray places no restrictions on capacity and MaxCapacity shall be null. 2 (Unknown) means the input tray cannot sense a meaningful value and MaxCapacity shall be null. 3 (Actual) means the input tray can sense a meaningful value and MaxCapacity shall be present.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInputMaxCapacity
ModelCorrespondence | string | CIM_PrintInputTray.MaxCapacity
ValueMap | string | 1, 2, 3, ..
Values | string | Other, Unknown, Actual, DMTF Reserved
MediaColor | string |
Description | string | The name of the color of the media associated with this input tray. The values of this property should conform to the requirements of the PWG Media Standardized Names specification [PWG5101.1], which defines the normative values for this property.
MappingStrings | string | PWG5101-1.PWG|Media Standardized Names, MIB.IETF|Printer-MIB.prtInputMediaColor
MaxLen | uint32 | 63
MinLen | uint32 | 0
MediaName | string |
Description | string | The descriptive name of the media contained in this input tray. This media name is to be used by a client to format and localize a string for display to a human operator. This media name is not processed by the printer. It is used to provide information not expressible in terms of the other media attributes (e.g., CIM_PrintInputTray.MediaWeight and CIM_PrintInputTray.MediaType).
MappingStrings | string | MIB.IETF|Printer-MIB.prtInputMediaName
MaxLen | uint32 | 63
MinLen | uint32 | 0
MediaSizeName | string |
Description | string | This property provides the value of the PWG standard or custom media size name of the media that is (or, if empty, was or will be) in this input tray. The values of this property shall conform to the requirements of the PWG Media Standardized Names specification [PWG5101.1], which defines the normative values for this property. If this input tray can reliably sense this value, the value is sensed by the input tray and cannot be changed by the system administrator; otherwise, the value may be changed out-of-band by the system administrator. The empty value means unknown.
MappingStrings | string | PWG5101-1.PWG|Media Standardized Names, MIB.IETF|Printer-MIB.prtInputMediaDimFeedDirDeclared, MIB.IETF|Printer-MIB.prtInputMediaDimXFeedDirDeclared
MaxLen | uint32 | 63
MinLen | uint32 | 0
MediaType | string |
Description | string | The name of the type of media associated with this input tray. The values of this property should conform to the requirements of the PWG Media Standardized Names specification [PWG5101.1], which defines the normative values for this property. This media type name need not be processed by the printer; it might simply be displayed to an operator.
MappingStrings | string | PWG5101-1.PWG|Media Standardized Names, MIB.IETF|Printer-MIB.prtInputMediaType
MaxLen | uint32 | 63
MinLen | uint32 | 0
MediaWeight | uint32 |
Description | string | The weight of the media associated with this input tray in grams per square meter.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInputMediaWeight
MaxValue | sint64 | 2147483647
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_PrintInputTray.MediaWeightBasis
Punit | string | gram / (meter * meter)
MediaWeightBasis | uint16 |
Description | string | The basis for the media property MediaWeight, that specifies whether a meaningful value is available. 2 (Unknown) means the input tray cannot sense a meaningful value and MediaWeight shall be null. 3 (Actual) means the input tray can sense a meaningful value and MediaWeight shall be present.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInputMediaWeight
ModelCorrespondence | string | CIM_PrintInputTray.MediaWeight
ValueMap | string | 2, 3, ..
Values | string | Unknown, Actual, DMTF Reserved
NonCriticalAlertsPresent | boolean |
Description | string | If true, there are currently non-critical alerts on this input tray.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.DetailedStatus
OtherAvailabilityStatus | string |
Description | string | A free-form string that describes the detailed availability of this PrintInputTray when the value of the AvailabilityStatus property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_PrintInputTray.AvailabilityStatus
OtherCapacityUnit | string |
Description | string | A free-form string that describes the capacity unit when the value of the CapacityUnit property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_PrintInputTray.CapacityUnit
OtherTypeDescription | string |
Description | string | A free-form string that describes the type of technology when the value of the Type property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_PrintInputTray.Type
Type | uint32 |
Description | string | The type of technology (discriminated primarily according to feeder mechanism type) employed by the input tray.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInputType, MIB.IETF|IANA-PRINTER-MIB.PrtInputTypeTC
ModelCorrespondence | string | CIM_PrintInputTray.OtherTypeDescription
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, ..
Values | string | Other, Unknown, SheetFeedAutoRemovableTray, SheetFeedAutoNonRemovableTray, SheetFeedManual, ContinuousRoll, ContinuousFanFold, DMTF Reserved

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_PrinterElement
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
PrimaryStatus | uint16 | CIM_ManagedSystemElement
SNMPRowId | uint32 | CIM_PrinterElement
Status | string | CIM_ManagedSystemElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods