# Class CIM_LinkAggregatorPartnerConnection
extends CIM_ActiveConnection

LinkAggregatorPartnerConnection contains the configuration information for an instance of a Link Aggregator's partner. The partner is defined as a RemoteServiceAccessPoint and it represents the actor's view of the connection. This sub-class of ActiveConnection represents a connection which is configured to communicate or it is actively communicating. If there is no known partner, then this association will not be defined for an instance of LinkAggregator8023ad.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_Dependency
|
+--CIM_SAPSAPDependency
|
+--CIM_ActiveConnection
|
+--CIM_LinkAggregatorPartnerConnection

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Association | boolean | true
Description | string | LinkAggregatorPartnerConnection contains the configuration information for an instance of a Link Aggregator's partner. The partner is defined as a RemoteServiceAccessPoint and it represents the actor's view of the connection. This sub-class of ActiveConnection represents a connection which is configured to communicate or it is actively communicating. If there is no known partner, then this association will not be defined for an instance of LinkAggregator8023ad.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::8023LAG
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
PartnerOperKey | uint16 |
Description | string | The current operational value of the 16-bit Key for the Aggregator's current protocol Partner. If the aggregation is manually configured, this Key value will be a value assigned by the local System.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPartnerOperKey
PartnerSystemID | string |
Description | string | A 6-octet MAC address value consisting of the unique identifier for the current protocol Partner of the referenced Aggregator. If the aggregation is manually configured, this System ID value will be a value assigned by the local System. Note that the MAC address is formatted as twelve hexadecimal digits (e.g., "010203040506"), with each pair representing one of the six octets of the MAC address in "canonical" bit order according to RFC 2469.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPartnerSystemID
MaxLen | uint32 | 12
ModelCorrespondence | string | CIM_LinkAggregatorPartnerConnection.PartnerSystemPriority
PartnerSystemPriority | uint16 |
Description | string | A 2-octet value that indicates the priority value associated with the Partner's System ID. If the aggregation is manually configured, this System Priority value will be a value assigned by the local System.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPartnerSystemPriority
ModelCorrespondence | string | CIM_LinkAggregatorPartnerConnection.PartnerSystemID

### Association References

Name | Class Origin | Reference Class | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Antecedent | CIM_LinkAggregatorPartnerConnection | CIM_LinkAggregator8023ad
Description | string | The Link Aggregator on the local system.
Key | boolean | true
Max | uint32 | 1
Override | string | Antecedent
Dependent | CIM_LinkAggregatorPartnerConnection | CIM_RemoteServiceAccessPoint
Description | string | The remote entity/partner of the referenced LinkAggregator8023ad.
Key | boolean | true
Max | uint32 | 1
Override | string | Dependent

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
IsUnidirectional | boolean | CIM_ActiveConnection
OtherTrafficDescription | string | CIM_ActiveConnection
TrafficType | uint16 | CIM_ActiveConnection

## Class Methods