# Class CIM_EthernetNICDiagnosticSettingData
extends CIM_DiagnosticSettingData

This class define the additional settings to be used for Ethernet NIC diagnostic tests.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_DiagnosticSettingData
|
+--CIM_EthernetNICDiagnosticSettingData

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class define the additional settings to be used for Ethernet NIC diagnostic tests.
Experimental | boolean | true
UMLPackagePath | string | CIM::System::Diagnostics
Version | string | 2.31.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
LinkSpeeds | uint64[] |
Description | string | This array property specifies the link speed to be used for the some of the Ethernet NIC tests. If no link speeds are specified, then the default set of link speeds as defined by the vendor will be used.
ModelCorrespondence | string | CIM_EthernetNICDiagnosticServiceCapabilities.LinkSpeedsSupported
PUnit | string | bit / second * 10^6
LoopbackLayers | uint16[] |
Description | string | This array property is used by a client for the Internal Loopback test to specify the layer to test. If no value is specified by the client, then the vendor-defined default value will be used.
ModelCorrespondence | string | CIM_EthernetNICDiagnosticSettingData.OtherLoopbackLayers, CIM_EthernetNICDiagnosticServiceCapabilities.LoopbackLayersSupported
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Other, PHY Layer, MAC Layer
OtherLoopbackLayers | string[] |
Description | string | A string that describes the Ethernet NIC Layer to test when the LoopbackLayer property is set to 1 ("Other"). This property must be set to null when LoopbackLayer is any value other than 1.
ModelCorrespondence | string | CIM_EthernetNICDiagnosticServiceCapabilities.OtherLoopbackLayersSupported, CIM_EthernetNICDiagnosticSettingData.LoopbackLayers
PacketSizes | uint16[] |
Description | string | This array property specifies the packet sizes to be used for the some of the Ethernet NIC tests. If no packet sizes are specified, then the default set of packet sizes as defined by the vendor will be used.
ModelCorrespondence | string | CIM_EthernetNICDiagnosticServiceCapabilities.PacketSizesSupported
PUnit | string | Byte

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
Generation | uint64 | CIM_ManagedElement
HaltOnError | boolean | CIM_DiagnosticSettingData
InstanceID | string | CIM_SettingData
NonDestructive | boolean | CIM_DiagnosticSettingData
PercentOfTestCoverage | uint8 | CIM_DiagnosticSettingData
QueryTimeout | uint32 | CIM_DiagnosticSettingData
QuickMode | boolean | CIM_DiagnosticSettingData
ResultPersistence | uint32 | CIM_DiagnosticSettingData
LogOptions | uint16[] | CIM_DiagnosticSettingData
LogStorage | uint16[] | CIM_DiagnosticSettingData
LoopControl | uint16[] | CIM_DiagnosticSettingData
LoopControlParameter | string[] | CIM_DiagnosticSettingData
OtherLogOptionsDescriptions | string[] | CIM_DiagnosticSettingData
OtherLogStorageDescriptions | string[] | CIM_DiagnosticSettingData
OtherLoopControlDescriptions | string[] | CIM_DiagnosticSettingData
VerbosityLevel | uint16[] | CIM_DiagnosticSettingData

## Class Methods