# Class CIM_FCIPSettings
extends CIM_SettingData

FCIPSettings class defines the attributes that affect the behavior of an Fibre Channel ProtocolEndpoint. The attributes are tied to the Fibre Channel ProtocolEndpoint though an ElementSettingData association. This class may also be used to specify the default settings for all Fibre Channel ProtocolEndpoint instances created on a ComputerSystem though an ElementSettingData association to the ComputerSystem. Processes that create new instances of Fibre Channel ProtocolEndpoint and the associated setting data should check for a FCIPSettings instance associated with the ComputerSystem and should only create a new instance of FCIPSettings specific to the Fibre Channel ProtocolEndpoint if the default settings need to be overridden for the specific Fibre Channel ProtocolEndpoint instance.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_FCIPSettings

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | FCIPSettings class defines the attributes that affect the behavior of an Fibre Channel ProtocolEndpoint. The attributes are tied to the Fibre Channel ProtocolEndpoint though an ElementSettingData association. This class may also be used to specify the default settings for all Fibre Channel ProtocolEndpoint instances created on a ComputerSystem though an ElementSettingData association to the ComputerSystem. Processes that create new instances of Fibre Channel ProtocolEndpoint and the associated setting data should check for a FCIPSettings instance associated with the ComputerSystem and should only create a new instance of FCIPSettings specific to the Fibre Channel ProtocolEndpoint if the default settings need to be overridden for the specific Fibre Channel ProtocolEndpoint instance.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::ChannelExtender
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ConnectionUsageFlags | uint16 |
Description | string | Identify the types of FCIP SOF values to be carried on the connection. (1) Class F (2) Class 2 (3) Class 3 (4) Class 4.
MappingStrings | string | Fibre Channel Over TCP/IP (FCIP) Draft.IETF|Section 8.1
ValueMap | string | 1, 2, 3, 4
Values | string | SOF(F), SOF(2), SOF(3), SOF(4)
Write | boolean | true
KeepAliveTimeout | uint32 |
Description | string | FC Keep Alive Timeout value to be applied to the new TCP Connection.
MappingStrings | string | Fibre Channel Over TCP/IP (FCIP) Draft.IETF|Section 8.1
PUnit | string | second
Units | string | Seconds
Write | boolean | true
SpecialFrameTimeout | uint32 | 90
Description | string | Timeout to wait for echoed FCIP Special Frame bytes.
MappingStrings | string | Fibre Channel Over TCP/IP (FCIP) Draft.IETF|Section 8.1
MinValue | sint64 | 90
PUnit | string | second
Units | string | Seconds
Write | boolean | true

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_SettingData

## Class Methods