# Class CIM_DesktopMonitor
extends CIM_Display

Capabilities and management of the DesktopMonitor (CRT) LogicalDevice.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_UserDevice
|
+--CIM_Display
|
+--CIM_DesktopMonitor

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of the DesktopMonitor (CRT) LogicalDevice.
UMLPackagePath | string | CIM::Device::UserDevices
Version | string | 2.6.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Bandwidth | uint32 |
Description | string | Monitor's bandwidth in MHertz. If unknown, enter 0.
PUnit | string | hertz * 10^6
Units | string | MegaHertz
DisplayType | uint16 |
Description | string | The type of DesktopMonitor or CRT. For example, multiscan color or monochrome monitors (values 2 or 3, respectively) can be indicated in this property.
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Unknown, Other, Multiscan Color, Multiscan Monochrome, Fixed Frequency Color, Fixed Frequency Monochrome
ScreenHeight | uint32 |
Description | string | The logical height of the Display in screen coordinates.
ScreenWidth | uint32 |
Description | string | The logical width of the Display in screen coordinates.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Availability | uint16 | CIM_LogicalDevice
Brightness | uint32 | CIM_Display
Caption | string | CIM_ManagedElement
ColorModePreset | uint16 | CIM_Display
CommunicationStatus | uint16 | CIM_ManagedSystemElement
Contrast | uint32 | CIM_Display
CreationClassName | string | CIM_LogicalDevice
CurrentResolutionH | uint16 | CIM_Display
CurrentResolutionV | uint16 | CIM_Display
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
DisplayMode | uint16 | CIM_Display
DisplayTechnologyType | uint16 | CIM_Display
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
FrequencyH | uint32 | CIM_Display
FrequencyV | uint32 | CIM_Display
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InputSource | uint16 | CIM_Display
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsLocked | boolean | CIM_UserDevice
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxBrightness | uint32 | CIM_Display
MaxContrast | uint32 | CIM_Display
MaxQuiesceTime | uint64 | CIM_LogicalDevice
MCCSVersionNumber | string | CIM_Display
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherScalerManufacturerDescription | string | CIM_Display
PerformAutoSetup | uint16 | CIM_Display
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
ScalerManufacturer | uint16 | CIM_Display
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
ColorModePresetCapabilities | uint16[] | CIM_Display
DisplayCharacteristics | uint16[] | CIM_Display
DisplayModeCapabilities | uint16[] | CIM_Display
IdentifyingDescriptions | string[] | CIM_LogicalDevice
InputSourceCapabilities | uint16[] | CIM_Display
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ButtonLock | uint32 | CIM_Display
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreFactoryDefault | uint32 | CIM_Display
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice