# Class CIM_MPLSCrossConnect
extends CIM_Service

This class specifies information for switching between Segments within a LSR. It is scoped by a Computer System, that is the Label Switched Router, via the HostedService association. Specific In/Out Segments are associated with the cross-connect using the relationship, MPLSSegmentInXC. The service can support point-to-point, point-to-multipoint and multipoint-to-point connections by defining multiple instances of the association. CrossConnect Services can be aggregated into an overarching MPLSService using the CIM_ServiceComponent association. And, the LSP to which the CrossConnect belongs is indicated by the association, CrossConnectLSP.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_MPLSCrossConnect

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class specifies information for switching between Segments within a LSR. It is scoped by a Computer System, that is the Label Switched Router, via the HostedService association. Specific In/Out Segments are associated with the cross-connect using the relationship, MPLSSegmentInXC. The service can support point-to-point, point-to-multipoint and multipoint-to-point connections by defining multiple instances of the association. CrossConnect Services can be aggregated into an overarching MPLSService using the CIM_ServiceComponent association. And, the LSP to which the CrossConnect belongs is indicated by the association, CrossConnectLSP.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::MPLS
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
IsPersistent | boolean |
Description | string | Denotes whether or not this CrossConnect entry and associated In and Out Segments should be restored automatically after failures.
MappingStrings | string | MIB.IETF|MPLS-LSR-MIB.MPLSXCIsPersistent
LabelStack | uint16[] |
ArrayType | string | Ordered
Description | string | Identifies a stack of labels to be pushed beneath the top label. Note that the top label identified in an instance of OutSegment ensures that all the components of a multipoint-to-point connection have the same outgoing label. This array is 'Ordered' to maintain the sequence of entries.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
RequestStateChange | uint32 | CIM_EnabledLogicalElement
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service