# Class CIM_OpticalDriveDiagnosticSettingData
extends CIM_DiagnosticTest

This class define the additional settings to be used for optical drive diagnostic tests.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_DiagnosticService
|
+--CIM_DiagnosticTest
|
+--CIM_OpticalDriveDiagnosticSettingData

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class define the additional settings to be used for optical drive diagnostic tests.
Experimental | boolean | true
UMLPackagePath | string | CIM::System::Diagnostics
Version | string | 2.31.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Seed | uint32 |
Description | string | This property specifies the seed that initiates the random number sequence used by the test.
ModelCorrespondence | string | CIM_OpticalDriveDiagnosticServiceCapabilities.SeedSupported
DataPatterns | string[] |
Description | string | This array property specifies the data patterns written by the optical drive diagnostic. If NULL, then the the vendor-specific data pattern(s) is used. A data pattern is a string interpreted as a 16-digit hex value. For example, a data pattern of all ones would be 0xFFFFFFFFFFFFFFFF while alternating ones and zeros would be 0x5555555555555555 or 0xAAAAAAAAAAAAAAAA . The pattern will be repeated as necessary to fill the data buffer.
ModelCorrespondence | string | CIM_OpticalDriveDiagnosticServiceCapabilities.DataPatternsSupported

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsInUse | boolean | CIM_DiagnosticTest
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherCharacteristicDescription | string | CIM_DiagnosticTest
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
Characteristics | uint16[] | CIM_DiagnosticTest
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherCharacteristicsDescriptions | string[] | CIM_DiagnosticTest
OtherTestTypesDescriptions | string[] | CIM_DiagnosticTest
ResourcesUsed | uint16[] | CIM_DiagnosticTest
StatusDescriptions | string[] | CIM_ManagedSystemElement
TestTypes | uint16[] | CIM_DiagnosticTest

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
ClearResults | uint32 | CIM_DiagnosticTest
DiscontinueTest | uint32 | CIM_DiagnosticTest
RequestStateChange | uint32 | CIM_EnabledLogicalElement
RunDiagnostic | uint32 | CIM_DiagnosticService
RunDiagnosticService | uint32 | CIM_DiagnosticService
RunTest | uint32 | CIM_DiagnosticTest
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service