# Class CIM_SWRLimitSetting
extends CIM_SettingData

SWRLimitSetting describes the limits of the software resource. In essence it is possible to define 6 different types of limits in groups of three. Each group consists of allocation, input and output limits. One group is always expressed by technical units (the default) and the other group in domain-specific units (e.g., items per second as the input limit). Thus, they are of different types. In order to avoid inconsistencies, only one group of settings is writable. The other one is derived from the writable limits. I.e., if technical limits are specifiable by the user (the type of the settings is technical) then the other set of limits (the non-writeable and derived settings) are domain-specific. SWRLimitSetting is associated to SoftwareResource via ElementSettingData. One software resource can have multiple limit settings. Only one of the settings is the default and one (potentially another one) is operational (current). Settings can be shared by software resources.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_SWRLimitSetting

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | SWRLimitSetting describes the limits of the software resource. In essence it is possible to define 6 different types of limits in groups of three. Each group consists of allocation, input and output limits. One group is always expressed by technical units (the default) and the other group in domain-specific units (e.g., items per second as the input limit). Thus, they are of different types. In order to avoid inconsistencies, only one group of settings is writable. The other one is derived from the writable limits. I.e., if technical limits are specifiable by the user (the type of the settings is technical) then the other set of limits (the non-writeable and derived settings) are domain-specific. SWRLimitSetting is associated to SoftwareResource via ElementSettingData. One software resource can have multiple limit settings. Only one of the settings is the default and one (potentially another one) is operational (current). Settings can be shared by software resources.
Experimental | boolean | true
UMLPackagePath | string | CIM::Application::SWResources
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AllocationUnit | string | MB
Description | string | This is the unit of the allocation limits of the software resource. In general, the unit describes a quantity (i.e., items MegyBytes). A null value is only allowed if neither upper nor lower limit exist. Otherwise, the property value is read-only and assumed to correspond to the implementation of the software resource to which the settings have to apply. The default value is of the technical domain (kB per second).
ModelCorrespondence | string | CIM_SWRLimitSetting.OtherAllocationUnit, CIM_SWRLimitSetting.LimitSettingType
InputUnit | string |
Description | string | This is the unit of the input limits of the software resource. In general, the unit describes a rate (i.e., items per second or Bytes per second). A null value is only allowed if neither upper nor lower limit exist. Otherwise, the property value is read-only and assumed to be correspond to the implementation of the software resource to which the settings have to apply.
ModelCorrespondence | string | CIM_SWRLimitSetting.OtherInputUnit, CIM_SWRLimitSetting.LimitSettingType
LimitSettingType | uint16 | 2
Description | string | LimitSettingType describes whether the limits are specified in terms of technical units or domain-specific units. Domain-specific is meant to be the items unit or 'business' unit of the usage the software resource. It may range from objects or tables (in a buffer) to orders in a queue. It depends on the implementation and usage context of the software resource. The default is the technical domain. Values: Technical: The writable setting properties are assigned a technical unit e.g Kilobytes. Domain-Specific: The writable setting properties are assigned a business-like, item-oriented unit e.g messages, objects, orders, etc..
ValueMap | string | 0, 2, 3, 4..32767, 32768..65535
Values | string | Unknown, Technical, Domain-Specific, DMTF Reserved, Vendor Reserved
LowerAllocationLimit | uint32 |
Description | string | This is the lower limit of the allocation (i.e., size) of the software resource. In general, the limit is a quantity (i.e., items or Megabytes). The corresponding unit is found at the property AllocationUnit. A null value indicates that no allocation limit exists. The property value can be modified and is persisted on saving the modification.
ModelCorrespondence | string | CIM_SWRLimitSetting.AllocationUnit
Write | boolean | true
LowerInputLimit | uint32 |
Description | string | This is the lower limit of the input of the software resource. In general, the limit is a rate (i.e., items per second or Bytes per second). The corresponding unit is found at the property InputUnit. A null value indicates that no lower limit exists. The property value can be modified and is persisted on saving the modification.
ModelCorrespondence | string | CIM_SWRLimitSetting.InputUnit
Write | boolean | true
LowerOutputLimit | uint32 |
Description | string | This is the lower limit of the output of the software resource. In general, the limit is a rate (i.e., items per second or Bytes per second). The corresponding unit is found at the property OutputUnit. A null value indicates that no lower limit exists. The property value can be modified and is persisted on saving the modification.
ModelCorrespondence | string | CIM_SWRLimitSetting.OutputUnit
Write | boolean | true
OtherAllocationUnit | string |
Description | string | This is the complementary unit of the output limits. If OutputUnit is a unit of the technical domain, OtherOutputUnit is a domain-specific unit.
ModelCorrespondence | string | CIM_SWRLimitSetting.AllocationUnit
OtherInputUnit | string |
Description | string | This is the complementary unit of the input limits. If InputUnit is a unit of the technical domain, OtherInputUnit is a domain-specific unit.
ModelCorrespondence | string | CIM_SWRLimitSetting.InputUnit
OtherLowerAllocationLimit | uint32 |
Description | string | This property is not null, if the lower allocation limit of the software resource can be calculated from the property LowerAllocationLimit. If LowerAllocationLimit is described by technical units (i.e., AllocationUnit applies to the technical domain), OtherLowerAllocationLimit is described by domain-specific units.
ModelCorrespondence | string | CIM_SWRLimitSetting.OtherAllocationUnit
OtherLowerInputLimit | uint32 |
Description | string | This property is not null, if the lower input limit of the software resource can be calculated from the property LowerInputLimit. If LowerInputLimit is described by technical units (i.e., InputUnit applies to the technical domain), OtherLowerInputLimit is described by domain-specific units.
ModelCorrespondence | string | CIM_SWRLimitSetting.OtherInputUnit
OtherLowerOutputLimit | uint32 |
Description | string | This property is not null, if the lower output limit of the software resource can be calculated from the property LowerOutputLimit. If LowerOutputLimit is described by technical units (i.e., OutputUnit applies to the technical domain), OtherLowerOutputLimit is described by domain-specific units.
ModelCorrespondence | string | CIM_SWRLimitSetting.OtherOutputUnit
OtherOutputUnit | string |
Description | string | This is the complementary unit of the output limits. If OutputUnit is a unit of the technical domain, OtherOutputUnit is a domain-specific unit.
ModelCorrespondence | string | CIM_SWRLimitSetting.OutputUnit
OtherUpperAllocationLimit | uint32 |
Description | string | This property is not null, if the upper allocation limit of the software resource can be calculated from the property UpperAllocationLimit. If UpperAllocationLimit is described by technical units (i.e., AllocationUnit applies to the technical domain), OtherUpperAllocationLimit is described by domain-specific units.
ModelCorrespondence | string | CIM_SWRLimitSetting.OtherAllocationUnit
OtherUpperInputLimit | uint32 |
Description | string | This property is not null, if the upper input limit of the software resource can be calculated from the property UpperInputLimit. If UpperInputLimit is described by technical units (i.e., InputUnit applies to the technical domain), OtherUpperInputLimit is described by domain-specific units.
ModelCorrespondence | string | CIM_SWRLimitSetting.OtherInputUnit
OtherUpperOutputLimit | uint32 |
Description | string | This property is not null, if the upper output limit of the software resource can be calculated from the property UpperOutputLimit. If UpperOutputLimit is described by technical units (i.e., OutputUnit applies to the technical domain), OtherUpperOutputLimit is described by domain-specific units.
ModelCorrespondence | string | CIM_SWRLimitSetting.OtherOutputUnit
OutputUnit | string |
Description | string | This is the unit of the output limits of the software resource. In general, the unit describes a rate (i.e., items per second or Bytes per second). A null value is only allowed if neither upper nor lower limit exist. Otherwise, the property value is read-only and assumed to be correspond to the implementation of the software resource to which the settings have to apply.
ModelCorrespondence | string | CIM_SWRLimitSetting.OtherOutputUnit, CIM_SWRLimitSetting.LimitSettingType
UpperAllocationLimit | uint32 |
Description | string | This is the upper limit of the allocation (i.e., size) of the software resource. In general, the limit is a quantity (i.e., items or Megabytes). The corresponding unit is found at the property AllocationUnit. A null value indicates that no allocation limit exists. The property value can be modified and is persisted on saving the modification.
ModelCorrespondence | string | CIM_SWRLimitSetting.AllocationUnit
Write | boolean | true
UpperInputLimit | uint32 |
Description | string | This is the upper limit of the input of the software resource. In general, the limit is a rate (i.e., items per second or Bytes per second). The corresponding unit is found at the property InputUnit. A null value indicates that no upper limit exists. The property value can be modified and is persisted on saving the modification.
ModelCorrespondence | string | CIM_SWRLimitSetting.InputUnit
Write | boolean | true
UpperOutputLimit | uint32 |
Description | string | This is the upper limit of the output of the software resource. In general, the limit is a rate (i.e., items per second or Bytes per second). The corresponding unit is found at the property OutputUnit. A null value indicates that no upper limit exists. The property value can be modified and is persisted on saving the modification.
ModelCorrespondence | string | CIM_SWRLimitSetting.OutputUnit
Write | boolean | true

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_SettingData

## Class Methods