# Class CIM_OpticalDriveDiagnosticTest
extends CIM_DiagnosticTest

This class specializes CIM_DiagnosticTest to define the tests specific to Optical Disk Drives

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_DiagnosticService
|
+--CIM_DiagnosticTest
|
+--CIM_OpticalDriveDiagnosticTest

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class specializes CIM_DiagnosticTest to define the tests specific to Optical Disk Drives
Experimental | boolean | true
UMLPackagePath | string | CIM::System::Diagnostics
Version | string | 2.31.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
OpticalDriveTestType | uint16 |
Description | string | The descriptions for each Optical Disk Drive test type are below: * "Media Detection" (value=2) is specified for the test that verifies that the Optical Disk Drive can properly detect whether or not media is present. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Mechanical Tray" (value=3) is specified for the test that verifies that the physical components of the optical device tray are operating properly. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Activity Indicator" (value=3) is specified for the test that verifies that the Activity Indicator LED operates properly. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Transfer Rate" (value=5) is specified for the test that verifies that the Optical Disk Drive operates properly when performing I/O operations at all supported data transfer rates. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Sequential Internal Verify" (value=6) is specified for the test that verifies the ability to perform read and verify operations in sequential order to each sector of the media. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Sequential Read" (value=7) is specified for the test that performs a read operation in sequential order from all sectors of the media.. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Medai Verify (value=6). * "Sequential Seek" (value=8) is specified for the test that performs a seek operation in sequential order to all sectors of the media. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Medai Verify (value=6). * "Sequential Write" (value=9) is specified for the test that performs a write operation in sequential order to all sectors of the media and then verifies that the data is written accurately. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Medai Verify (value=6). * "Random Read" (value=10) is specified for the test that performs a read operation in random order from selected sectors of the media. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Medai Verify (value=6). * "Random Seek" (value=11) is specified for the test that performs a seek operation in random order from selected sectors of the media. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Medai Verify (value=6). * "Status" (value=12) is specified for the test that verifies that the Optical Disk Drive is ready to be tested. CIM_DiagnosticTest.TestTypes shall be set to Health Check (value=4). * "Reset Drive" (value=13) is specified for the test that verifies that the Optical Disk Drive properly responds to a Reset command. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "System Inteface" (value=14) is specified for the test that verifies that all system interface for cables and connectors are working properly. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Load / Eject" (value=15) is specified for the test that verifies that the Optical Disk Drive properly responds to a Load/Eject command. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2).
ModelCorrespondence | string | CIM_OpticalDriveDiagnosticTest.OtherOpticalDriveTestType
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, .., 0x8000..
Values | string | Unknown, Other, Media Detection, Mechanical Tray, Activity Indicator, Transfer Rate, Sequential Internal Verify, Sequential Read, Sequential Seek, Sequential Write, Random Read, Random Seek, Status, Reset Drive, System Inteface, Load/Eject, Vendor Reserved, DMTF Reserved
OtherOpticalDriveTestType | string |
Description | string | A string that describes the test when the OpticalDriveTestType property is set to 1 ("Other"). This property must be set to null when OpticalDriveTestType is any value other than 1.
ModelCorrespondence | string | CIM_OpticalDriveDiagnosticTest.OpticalDriveTestType

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsInUse | boolean | CIM_DiagnosticTest
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherCharacteristicDescription | string | CIM_DiagnosticTest
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
Characteristics | uint16[] | CIM_DiagnosticTest
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherCharacteristicsDescriptions | string[] | CIM_DiagnosticTest
OtherTestTypesDescriptions | string[] | CIM_DiagnosticTest
ResourcesUsed | uint16[] | CIM_DiagnosticTest
StatusDescriptions | string[] | CIM_ManagedSystemElement
TestTypes | uint16[] | CIM_DiagnosticTest

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
ClearResults | uint32 | CIM_DiagnosticTest
DiscontinueTest | uint32 | CIM_DiagnosticTest
RequestStateChange | uint32 | CIM_EnabledLogicalElement
RunDiagnostic | uint32 | CIM_DiagnosticService
RunDiagnosticService | uint32 | CIM_DiagnosticService
RunTest | uint32 | CIM_DiagnosticTest
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service