# Class CIM_USBRedirectionSAP
extends CIM_ServiceAccessPoint

USBRedirectionSAP is a logical representation of a USB redirection session. One access point represents access to a single USB redirection session.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_USBRedirectionSAP

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | USBRedirectionSAP is a logical representation of a USB redirection session. One access point represents access to a single USB redirection session.
UMLPackagePath | string | CIM::Network::USBRedirection
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ConnectionMode | uint16 |
Description | string | An enumeration specifying the type of connection mode supported by the session. A value set to 2 = "Listen" shall indicate that the SAP will listen for a connection request from the remote USB redirection server. A CIM_BindsTo association to a CIM_ProtocolEndpoint may be used to represent where the SAP is listening for the connection request. A value set to 3 = "Connect" shall indicate that the the SAP shall initiate the connection to the remote USB redirection server. A CIM_RemoteAccessAvailableToElement association to a CIM_RemoteServiceAccessPoint may be used to represent where the SAP shall connect to the remote USB redirection server.
ValueMap | string | 0, 2, 3, .., 32768..65535
Values | string | Unknown, Listen, Connect, DMTF Reserved, Vendor Specified
ResetTimeout | datetime |
Description | string | The amount of time the session shall wait after sending a Reset to the Remote System before concluding that the Remote System is not responding in a timely fashion, it may be hung or busy. When the Reset Timeout is exceeded the managed system tries to establish a new connection with the Remote System. This property uses the interval format of the datetime type
SessionTimeout | datetime |
Description | string | The amount of time the session will wait for a Remote System to establish a new connection before the USB Device is detached. This property uses the interval format of the datetime type.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_ServiceAccessPoint
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
Name | string | CIM_ServiceAccessPoint
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_ServiceAccessPoint
SystemName | string | CIM_ServiceAccessPoint
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
RequestStateChange | uint32 | CIM_EnabledLogicalElement