# Class CIM_CLPProtocolEndpoint
extends CIM_ProtocolEndpoint

A representation of a communication endpoint where the CLP protocol may be accessed.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_ProtocolEndpoint
|
+--CIM_CLPProtocolEndpoint

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A representation of a communication endpoint where the CLP protocol may be accessed.
UMLPackagePath | string | CIM::Network::ProtocolEndpoints
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CurrentDefaultTarget | string |
Description | string | Identifies the Current Default Target when a CLP Session is established. The Current Default Target is the CLP session environment setting that establishes a default base address for all command targets that are expressed as a relative target address and is used as the command target if no command target is specified in a command.
ModelCorrespondence | string | CIM_CLPSettingData.CurrentDefaultTarget
Write | boolean | true
DisplayOption | string |
Description | string | Maintains the session default value for the display option. The argument string is stored "as-is" without normalization beyond capitalization. The argument string is compliant with the SM CLP command line grammar.
ModelCorrespondence | string | CIM_CLPSettingData.DisplayOption
Write | boolean | true
KeepTime | uint16 |
Description | string | The amount of time in seconds that the CLP Session should retain a CLP command job status. A KeepTime value of zero shall be interpreted to mean keep forever.
ModelCorrespondence | string | CIM_CLPSettingData.KeepTime
PUnit | string | second
Units | string | Seconds
Write | boolean | true
OutputCount | uint32 |
Description | string | Establishes the default CLP Session command output count number when multiple items are returned in the output as described in SM CLP Specification, DMTF document DSP0214. The value 0xFFFFFFFF shall be interpreted to mean that all items are to be returned. The maximum value for the count number is determined by the class of the target.
ModelCorrespondence | string | CIM_CLPSettingData.OutputCount
Write | boolean | true
OutputFormat | uint16 |
Description | string | OutputFormat establishes the default CLP Session command output format, as described in SM CLP Specification, DMTF document DSP0214.
ModelCorrespondence | string | CIM_CLPSettingData.OutputFormat
ValueMap | string | 2, 3, 4, 5, .., 0x8000..0xFFFF
Values | string | Text, clpcsv, Keyword, clpxml, DMTF Reserved, Vendor Reserved
Write | boolean | true
OutputLanguage | string |
Description | string | The default CLP Session command output language. As described in SM CLP Specification, DMTF document DSP0214, the language value is a 3-character string identifier of language as specified in ISO 639.2; "eng" is the default.
ModelCorrespondence | string | CIM_CLPSettingData.OutputLanguage
Write | boolean | true
OutputOrder | uint16 |
Description | string | OutputOrder establishes the default CLP Session command output order when multiple items are returned in the command output as described in SM CLP Specification, DMTF document DSP0214.
ModelCorrespondence | string | CIM_CLPSettingData.OutputOrder
ValueMap | string | 2, 3, .., 0x8000..0xFFFF
Values | string | Default, Reverse, DMTF Reserved, Vendor Reserved
Write | boolean | true
OutputPosition | uint16 |
Description | string | OutputPosition establishes the default CLP Session command output beginning position when multiple items are returned in the command output, as described in SM CLP Specification, DMTF document DSP0214.
ModelCorrespondence | string | CIM_CLPSettingData.OutputPosition
ValueMap | string | 2, 3, .., 0x8000..0xFFFF
Values | string | Begin, End, DMTF Reserved, Vendor Reserved
Write | boolean | true
OutputVerbosity | uint16 |
Description | string | OutputVerbosity establishes the default CLP Session output level of detail, as described in SM CLP Specification, DMTF document DSP0214.
ModelCorrespondence | string | CIM_CLPSettingData.OutputVerbosity
ValueMap | string | 2, 3, 4, .., 0x8000..0xFFFF
Values | string | Error, Terse, Verbose, DMTF Reserved, Vendor Reserved
Write | boolean | true
WaitBehavior | boolean |
Description | string | When TRUE the CLP Session will not return a command response until all spawned jobs have completed, otherwise it may.
ModelCorrespondence | string | CIM_CLPSettingData.WaitBehavior
Write | boolean | true

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_ServiceAccessPoint
Description | string | CIM_ProtocolEndpoint
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_ProtocolEndpoint
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
Name | string | CIM_ProtocolEndpoint
NameFormat | string | CIM_ProtocolEndpoint
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherTypeDescription | string | CIM_ProtocolEndpoint
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolIFType | uint16 | CIM_ProtocolEndpoint
ProtocolType | uint16 | CIM_ProtocolEndpoint
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_ServiceAccessPoint
SystemName | string | CIM_ServiceAccessPoint
TimeOfLastStateChange | datetime | CIM_ProtocolEndpoint
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ProtocolEndpoint
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
RequestStateChange | uint32 | CIM_EnabledLogicalElement