# Class CIM_StorageVolume
extends CIM_StorageExtent

A StorageVolume is a StorageExtent that is published for use outside of the scoping System. For SCSI storage target devices, StorageVolumes are used to represent target Block devices, (peripheral device type codes 0h (i.e, direct-access), 4h (i.e., write-once), 5h (i.e., CD/DVD), 7h (i.e., optical memory), and Eh (i.e., simplified direct-access).); Stream devices, (peripheral device type codes 1h (i.e., sequential-access) and 3h (i.e., processor).). In these case, StorageVolume.Name will be derived from SCSI volume as documented in StorageExtent.Nameformat and NameNamespace Descriptions. The 'Exported' value from StorageExtent.ExtentStatus[] MUST be in all instances of StorageVolume to maintain the semantic of 'published' described above.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_StorageExtent
|
+--CIM_StorageVolume

## Direct Known Subclasses

CIM_VolumeSet

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A StorageVolume is a StorageExtent that is published for use outside of the scoping System. For SCSI storage target devices, StorageVolumes are used to represent target Block devices, (peripheral device type codes 0h (i.e, direct-access), 4h (i.e., write-once), 5h (i.e., CD/DVD), 7h (i.e., optical memory), and Eh (i.e., simplified direct-access).); Stream devices, (peripheral device type codes 1h (i.e., sequential-access) and 3h (i.e., processor).). In these case, StorageVolume.Name will be derived from SCSI volume as documented in StorageExtent.Nameformat and NameNamespace Descriptions. The 'Exported' value from StorageExtent.ExtentStatus[] MUST be in all instances of StorageVolume to maintain the semantic of 'published' described above.
UMLPackagePath | string | CIM::Device::StorageExtents
Version | string | 2.13.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Name | string |
Description | string | A unique identifier for the Volume.
MappingStrings | string | ANSI|T10|SCSI SPC-3|8.6
MaxLen | uint32 | 1024
ModelCorrespondence | string | CIM_StorageVolume.NameFormat
Override | string | Name
NameFormat | uint16 |
Description | string | A subset of StorageExtent name formats apply to StorageVolumes.
ModelCorrespondence | string | CIM_StorageExtent.Name, CIM_StorageExtent.NameNamespace, CIM_StorageExtent.OtherNameFormat
Override | string | NameFormat
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11
Values | string | Unknown, Other, VPD83NAA6, VPD83NAA5, VPD83Type2, VPD83Type1, VPD83Type0, SNVM, NodeWWN, NAA, EUI64, T10VID
NameNamespace | uint16 |
Description | string | A subset of StorageExtent name spaces apply to StorageVolume.
MappingStrings | string | SPC.INCITS-T10| VPD 83, Association 0 | Identifier
ModelCorrespondence | string | CIM_StorageExtent.Name, CIM_StorageExtent.OtherNameNamespace, CIM_StorageExtent.NameFormat
Override | string | NameNamespace
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7
Values | string | Unknown, Other, VPD83Type3, VPD83Type2, VPD83Type1, VPD80, NodeWWN, SNVM

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Access | uint16 | CIM_StorageExtent
Availability | uint16 | CIM_LogicalDevice
BlockSize | uint64 | CIM_StorageExtent
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
ConsumableBlocks | uint64 | CIM_StorageExtent
CreationClassName | string | CIM_LogicalDevice
DataOrganization | uint16 | CIM_StorageExtent
DataRedundancy | uint16 | CIM_StorageExtent
DeltaReservation | uint8 | CIM_StorageExtent
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
ErrorMethodology | string | CIM_StorageExtent
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsBasedOnUnderlyingRedundancy | boolean | CIM_StorageExtent
LastErrorCode | uint32 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
NoSinglePointOfFailure | boolean | CIM_StorageExtent
NumberOfBlocks | uint64 | CIM_StorageExtent
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherNameFormat | string | CIM_StorageExtent
OtherNameNamespace | string | CIM_StorageExtent
PackageRedundancy | uint16 | CIM_StorageExtent
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
Primordial | boolean | CIM_StorageExtent
Purpose | string | CIM_StorageExtent
RequestedState | uint16 | CIM_EnabledLogicalElement
SequentialAccess | boolean | CIM_StorageExtent
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
ExtentStatus | uint16[] | CIM_StorageExtent
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice