# Class CIM_VirtualSystemMigrationSettingData
extends CIM_SettingData

CIM_MigrationSettingData defines the parameters to control a virtual system migration implementation, as managed by a CIM_VirtualSystemMigrationService. It is expected that a migration implementation will subclass this class to add implementation-specific migration options.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_VirtualSystemMigrationSettingData

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | CIM_MigrationSettingData defines the parameters to control a virtual system migration implementation, as managed by a CIM_VirtualSystemMigrationService. It is expected that a migration implementation will subclass this class to add implementation-specific migration options.
UMLPackagePath | string | CIM::System::Virtualization
Version | string | 2.33.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Bandwidth | uint16 |
Description | string | Bandwidth indicates the bandwidth assigned to or requested for a virtual system migration operation. The special value 0 indicates: - in migration requests the default bandwidth - otherwise that bandwidths are not supported. Bandwidth and Priority may be used in conjunction. Migration processes that have the highest equal priority value share the available bandwidth based on their requested bandwidth. If not all bandwidth is consumed by this set of processes, migration processes with the next lower equal priority share the remaining bandwidth. If still more bandwidth remains, migration processes with the next lower equal priority are considered, and so forth. The unit applicable for the Bandwidth property is conveyed by the value of the BandwidthUnit property. If the value of the BandwidthUnit property matches "percent", the following restrictions apply: The value of the Bandwidth property shall be between 0 and 100, with higher values indicating a higher bandwidth. A value of 100 indicates the total available bandwidth for performing virtual system migration operations. Values between 1 and 100 should linearly correlate with the available bandwidth range. For exampe, a value of 50 should request half of the available bandwidth, a value of 33 should request one third of the bandwidth, etc. .
Gauge | boolean | true
ModelCorrespondence | string | CIM_VirtualSystemMigrationSettingData.BandwidthUnit
BandwidthUnit | string |
Description | string | This property specifies the unit used by the Bandwidth property. The value of this property shall be a legal value of the Programmatic Units qualifier as defined in Appendix C.1 of DSP0004 V2.4 or later. NOTE: Profiles like DMTF DSP1081 define means by that clients are enabled to discover the set of units supported by an implementation, along with ranges and increments for admissable values of the Bandwidth property.
IsPUnit | boolean | true
ModelCorrespondence | string | CIM_VirtualSystemMigrationSettingData.Bandwidth
MigrationType | uint16 |
Description | string | MigrationType describes a type of migration operation to be performed. A value of 2 - Virtual System is to be migrated in a 'live' manner such that the running of the Virtual System is minimally impacted during the move. A value of 3 - Virtual System will be temporarily paused prior to migration and then resume running after it is moved. A value of 4 - The Virtual System will be quiesced to a stopped state prior to migration and then restarted after it is moved.
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, Live, Resume, Restart
OtherTransportType | string |
Description | string | OtherTransportType indicates the type of transport to be applied if the value of TransportType is 1 (Other).
ModelCorrespondence | string | CIM_VirtualSystemMigrationSettingData.TransportType
Priority | uint16 |
Description | string | Priority specifies a relative migration importance which the virtual system migration implementation may use to order or otherwise give preference among multiple pending migration requests. The lower the value, the higher the priority. A value of 0 indicates: - in migration requests the default priority - otherwise that priorities are not supported
TransportType | uint16 |
Description | string | TransportType indicates the type of transport to be applied for a virtual system migration operation. - 0(Unknown) indicates that the transport type is not exposed.- 1(Other) indicates that the transport type is specified as a textual value of the OtherTransportType property. - 2(SSH) indicates the secure shell transport type. - 3(TLS) indicats the transport layer security transport type. - 4(TLS strict) indicats the transport layer security transport type with mutual authentication. - 5(TCP) indicates the TCP transport type. - 6(IPC) indicates the inter-process communication socket transport type. This transport type includes Unix domain sockets.
ModelCorrespondence | string | CIM_VirtualSystemMigrationSettingData.OtherTransportType
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 32768..
Values | string | Unknown, Other, SSH, TLS, TLS Strict, TCP, IPC, DMTF Reserved, Vendor Reserved

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
InstanceID | string | CIM_SettingData

## Class Methods