# Class CIM_FCAdapterEventCounters
extends CIM_DeviceStatisticalInformation

Note: The use of the FCAdapterEventCounters class is deprecated because FibreChannelAdapter is deprecated. FCPortStatistics should be used instead, but it redefines the level at which data is collected. Therefore, there is no direct translation of the individual counters between the two classes. This object describes event counters that were specific to a FibreChannelAdapter.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalInformation
|
+--CIM_DeviceStatisticalInformation
|
+--CIM_FCAdapterEventCounters

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_FCPortStatistics
Description | string | Note: The use of the FCAdapterEventCounters class is deprecated because FibreChannelAdapter is deprecated. FCPortStatistics should be used instead, but it redefines the level at which data is collected. Therefore, there is no direct translation of the individual counters between the two classes. This object describes event counters that were specific to a FibreChannelAdapter.
UMLPackagePath | string | CIM::Device::NetworkAdapter
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ABTSFramesReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of Abort sequence frames received.
ABTSFramesRejected | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of Abort sequence frames sent where the response was BA_RJT.
ABTSFramesSent | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of Abort sequence frames sent.
FBSYsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of frames busied by the Fabric.
FRJTsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of frames rejected by the Fabric.
PBSYsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of frames busied by the receiving Node.
PBSYsSent | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of frames busied by the Adapter itself.
PRJTsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of frames rejected by the receiving Node.
PRJTsSent | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of frames rejected by the Adapter itself.
PRLIsRejected | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of PRLI frames sent where the response was LS_RJT.
PRLOsRejected | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of PRLO frames sent where the response was LS_RJT.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CreationClassName | string | CIM_DeviceStatisticalInformation
Description | string | CIM_ManagedElement
DeviceCreationClassName | string | CIM_DeviceStatisticalInformation
DeviceID | string | CIM_DeviceStatisticalInformation
ElementName | string | CIM_ManagedElement
InstanceID | string | CIM_ManagedElement
Name | string | CIM_DeviceStatisticalInformation
SystemCreationClassName | string | CIM_DeviceStatisticalInformation
SystemName | string | CIM_DeviceStatisticalInformation

## Class Methods

### Local Class Methods

#### ResetCounter (uint32)

#### Method Qualifiers (ResetCounter)

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_FCPortStatistics.ResetSelectedStats()
Description | string | Note: The use of this method has been deprecated. Deprecated description: Method to reset the Adapter event counters. The method takes, as input, an integer that indicates which counter to reset. For this input 0 indicates all and 1 through 11 indicate a reset of the individual counters. The method returns 0 if successful, 1 if not supported, and any other value if an error occurred. A method is specified so that the instrumentation of the Device, which tabulates the errors and warnings, can also reset its internal processing and counters. In a subclass, the set of possible return codes could be specified, using a ValueMap qualifier on the method. The strings to which the ValueMap contents are 'translated' can also be specified in the subclass as a Values array qualifier.

#### Method Parameters (ResetCounter)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
SelectedCounter | uint16
Description | string | The counter to reset.
IN | boolean | true
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11
Values | string | All, ABTSFramesReceived, ABTSFramesSent, FBSYReceived, PBSYReceived, PBSYSent, FRJTReceived, PRJTReceived, PRJTSent, PRLIRejected, PRLORejected, ABTSFramesRejected