# Class CIM_InterLibraryPort
extends CIM_MediaTransferDevice

InterLibraryPorts represent hardware that transports Physical Media between connected StorageLibraries. The LibraryExchange association identifies the connected Libraries, by identifying the connected InterLibraryPorts.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_MediaTransferDevice
|
+--CIM_InterLibraryPort

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | InterLibraryPorts represent hardware that transports Physical Media between connected StorageLibraries. The LibraryExchange association identifies the connected Libraries, by identifying the connected InterLibraryPorts.
UMLPackagePath | string | CIM::Device::StorageLib
Version | string | 2.6.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Direction | uint16 |
Description | string | An enumeration expressing whether the Port is used for import into the Library/System which scopes and names it (value=1), export from the Library/System (value=2), or both (value=3).
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Import, Export, Both Import and Export
ExportCount | uint64 |
Counter | boolean | true
Description | string | The number of times that the InterLibraryPort was used to move a PhysicalMedia out of the System/StorageLibrary.
ImportCount | uint64 |
Counter | boolean | true
Description | string | The number of times that the InterLibraryPort was used to move a PhysicalMedia into the System/StorageLibrary.
LastAccessed | datetime |
Description | string | Date and time that the Port was last accessed by its System/StorageLibrary. This value may be different than that specified for the Port(s) to which this Inter LibraryPort is connected. Connected Ports are identified using the LibraryExchange association.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice