# Class CIM_FibrePortEventCounters
extends CIM_DeviceStatisticalInformation

Note: The use of the FibrePortEventCounters class is deprecated because FibrePort is deprecated. FCPortStatistics should be used instead, but it redefines the level at which data is collected. Therefore, there is no direct translation of the individual counters between the two classes. Deprecated description: This object defines error counters that are specific to a FibrePort.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalInformation
|
+--CIM_DeviceStatisticalInformation
|
+--CIM_FibrePortEventCounters

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_FCPortStatistics
Description | string | Note: The use of the FibrePortEventCounters class is deprecated because FibrePort is deprecated. FCPortStatistics should be used instead, but it redefines the level at which data is collected. Therefore, there is no direct translation of the individual counters between the two classes. Deprecated description: This object defines error counters that are specific to a FibrePort.
UMLPackagePath | string | CIM::Device::NetworkAdapter
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
EOFAbortsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: Number of frames received that contain 'EOF Abort'.
EOFAbortsTransmitted | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: Number of frames transmitted that contain 'EOF Abort'.
PLOGIsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of login frames received.
PLOGIsRejected | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of PLOGI frames sent where the response was LS_RJT.
PLOGIsSent | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of login frames sent.
PLOGOsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of logouts that were received from various targets.
PLOGOsRejected | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of PLOGO frames sent where the response was LS_RJT.
PLOGOsSent | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of logout frames sent.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CreationClassName | string | CIM_DeviceStatisticalInformation
Description | string | CIM_ManagedElement
DeviceCreationClassName | string | CIM_DeviceStatisticalInformation
DeviceID | string | CIM_DeviceStatisticalInformation
ElementName | string | CIM_ManagedElement
InstanceID | string | CIM_ManagedElement
Name | string | CIM_DeviceStatisticalInformation
SystemCreationClassName | string | CIM_DeviceStatisticalInformation
SystemName | string | CIM_DeviceStatisticalInformation

## Class Methods

### Local Class Methods

#### ResetCounter (uint32)

#### Method Qualifiers (ResetCounter)

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_FCPortStatistics.ResetSelectedStats
Description | string | Note: The use of this method has been deprecated. Deprecated description: Method to reset the Port event counters. The method takes as input an integer that indicates which counter to reset. For this input parameter, 0 indicates all and 1 through 8 indicate a reset of the individual counters. The method returns 0 if successful, 1 if not supported, and any other value if an error occurred. A method is specified so that the instrumentation of the Device, which tabulates the errors and warnings, can also reset its internal processing and counters. In a subclass, the set of possible return codes could be specified, using a ValueMap qualifier on the method. The strings to which the ValueMap contents are 'translated' can also be specified in the subclass as a Values array qualifier.

#### Method Parameters (ResetCounter)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
SelectedCounter | uint16
Description | string | The counter to reset.
IN | boolean | true
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8
Values | string | All, PLOGIsReceived, PLOGIsSent, EOFAbortsReceived, EOFAbortsTransmitted, PLOGOsReceived, PLOGOsSent, PLOGIsRejected, PLOGOsRejected