# Class CIM_WiFiPort
extends CIM_NetworkPort

WiFiPort is the logical representation of wireless local area network communications hardware that conforms to the IEEE 802.11 series of specifications. It embodies properties at the lowest layers of a network stack, such as the antennas used for transmission and reception, the address permanently embedded into the hardware, and the operational bandwidth of the device.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_LogicalPort
|
+--CIM_NetworkPort
|
+--CIM_WiFiPort

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | WiFiPort is the logical representation of wireless local area network communications hardware that conforms to the IEEE 802.11 series of specifications. It embodies properties at the lowest layers of a network stack, such as the antennas used for transmission and reception, the address permanently embedded into the hardware, and the operational bandwidth of the device.
UMLPackagePath | string | CIM::Device::Ports
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
MaxSpeed | uint64 |
Description | string | Shall contain the maximum bandwidth relative to the current operating mode specified in PortType. For example, shall contain 11000000 if PortType contains 71 ("802.11b").
Override | string | MaxSpeed
PUnit | string | bit / second
Units | string | Bits per Second
PermanentAddress | string |
Description | string | IEEE 802 EUI-48 MAC address, formatted as twelve hexadecimal digits (for example, "010203040506"), with each pair representing one of the six octets of the MAC address in "canonical" bit order. (Therefore, the Group address bit is found in the low order bit of the first character of the string.)
MappingStrings | string | MIF.DMTF|Network Adapter 802 Port|001.2
MaxLen | uint32 | 64
Override | string | PermanentAddress
PortType | uint16 |
Description | string | PortType shall contain the specific 802.11 operating mode that is currently enabled on the Port. All modes are specified in
ModelCorrespondence | string | CIM_NetworkPort.OtherNetworkPortType
Override | string | PortType
ValueMap | string | 0, 1, 70, 71, 72, 73, .., 16000..
Values | string | Unknown, Other, 802.11a, 802.11b, 802.11g, 802.11n, DMTF Reserved, Vendor Reserved
Speed | uint64 |
Description | string | The data rate at which the current PPDU (PLCP (Physical Layer Convergence Protocol) Protocol Data Unit) was received. This value is encoded in the first 4 bits of the PLCP header in each PLCP frame.
MappingStrings | string | MIB.IETF|MIB-II.ifSpeed, MIF.DMTF|Network Adapter 802 Port|001.5
Override | string | Speed
PUnit | string | bit / second
Units | string | Bits per Second
NetworkAddresses | string[] |
Description | string | IEEE 802 EUI-48 MAC addresses, each formatted as twelve hexadecimal digits (for example, "010203040506"), with each pair representing one of the six octets of the MAC address in "canonical" bit order. (Therefore, the Group address bit is found in the low order bit of the first character of the string.)
MappingStrings | string | MIF.DMTF|Network Adapter 802 Port|001.3
MaxLen | uint32 | 64
Override | string | NetworkAddresses

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
ActiveMaximumTransmissionUnit | uint64 | CIM_NetworkPort
AutoSense | boolean | CIM_NetworkPort
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
FullDuplex | boolean | CIM_NetworkPort
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LinkTechnology | uint16 | CIM_NetworkPort
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherLinkTechnology | string | CIM_NetworkPort
OtherNetworkPortType | string | CIM_NetworkPort
OtherPortType | string | CIM_LogicalPort
PortNumber | uint16 | CIM_NetworkPort
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedSpeed | uint64 | CIM_LogicalPort
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SupportedMaximumTransmissionUnit | uint64 | CIM_NetworkPort
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
UsageRestriction | uint16 | CIM_LogicalPort
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice