# Class CIM_IPAddressRange
extends CIM_CollectionOfMSEs

IPAddressRange represents a grouping of specific addresses, and provides additional semantics for this group if appropriate. The class is deprecated in lieu of the concrete class RangeOfIPAddresses since there is sufficient information for the class to be instantiated. In addition, an address range should be defined in the context of a System (for example, a network element or an admin domain). These semantics are incorporated in the RangeOfIPAddresses class.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Collection
|
+--CIM_CollectionOfMSEs
|
+--CIM_IPAddressRange

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Abstract | boolean | true
Deprecated | string | CIM_RangeOfIPAddresses
Description | string | IPAddressRange represents a grouping of specific addresses, and provides additional semantics for this group if appropriate. The class is deprecated in lieu of the concrete class RangeOfIPAddresses since there is sufficient information for the class to be instantiated. In addition, an address range should be defined in the context of a System (for example, a network element or an admin domain). These semantics are incorporated in the RangeOfIPAddresses class.
UMLPackagePath | string | CIM::Network::Collections
Version | string | 2.7.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AllocationRegion | uint16 |
Deprecated | string | No value
Description | string | This attribute defines the region that addresses can be allocated to.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8
Values | string | Unknown, Multiregional: 192.0.0.0 to 193.255.255.255, Europe: 194.0.0.0 to 195.255.255.255, Others: 196.0.0.0 to 197.255.255.255, North America: 198.0.0.0 to 199.255.255.255, Central & South America: 200.0.0.0 to 201.255.255.255, Pacific Rim: 202.0.0.0 to 203.255.255.255, Others: 204.0.0.0 to 205.255.255.255, Others: 206.0.0.0 to 207.255.255.255
EndAddress | string |
Deprecated | string | CIM_RangeOfIPAddresses.EndAddress
Description | string | The ending IP address of the AddressRange, formatted according to the appropriate convention as defined in the AddressType property of this class (e.g., 171.79.6.40).
StartAddress | string |
Deprecated | string | CIM_RangeOfIPAddresses.StartAddress
Description | string | The starting IP address of the AddressRange, formatted according to the appropriate convention as defined in the AddressType property of this class (e.g., 171.79.6.40).
TypeOfAddress | uint16 |
Deprecated | string | CIM_RangeOfIPAddresses.AddressType
Description | string | An enumeration that defines how to format the address and mask of the address range that defines this IPSubnet. Whenever possible, IPv4-compatible addresses should be used instead of IPv6 addresses (see RFC 2373, section 2.5.4). In order to have a consistent format for IPv4 addresses in a mixed IPv4/v6 environment, all IPv4 addresses and both IPv4-compatible IPv6 addresses and IPv4-mapped IPv6 addresses, per RFC 2373, section 2.5.4, should be formatted in standard IPv4 format.
ValueMap | string | 0, 1, 2
Values | string | Unknown, IPv4, IPv6

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CollectionID | string | CIM_CollectionOfMSEs
Description | string | CIM_ManagedElement
ElementName | string | CIM_ManagedElement
InstanceID | string | CIM_ManagedElement

## Class Methods