# Class CIM_TokenRingAdapter
extends CIM_NetworkAdapter

Note: The use of the CIM_TokenRingAdapter class has been deprecated, consistent with NetworkAdapter. Instead use the CIM_TokenRingPort class. Deprecated description: This class describes the capabilities and management aspects of a TokenRingAdapter.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_NetworkAdapter
|
+--CIM_TokenRingAdapter

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_TokenRingAdapter
Description | string | Note: The use of the CIM_TokenRingAdapter class has been deprecated, consistent with NetworkAdapter. Instead use the CIM_TokenRingPort class. Deprecated description: This class describes the capabilities and management aspects of a TokenRingAdapter.
UMLPackagePath | string | CIM::Device::NetworkAdapter
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AbortTransErrors | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.AbortTransErrors
Description | string | Note: The use of this method has been deprecated. Deprecated description: This counter is incremented when a station transmits an abort delimiter while transmitting data.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsAbortTransErrors
ACErrors | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.ACErrors
Description | string | Note: The use of this method has been deprecated. Deprecated description: This counter is incremented when a station receives an AMP or SMP frame in which A is equal to C, and C is equal to 0, and then receives another SMP frame with A equal to C, and C equal to 0 without first receiving an AMP frame. This condition indicates a station that cannot set the AC bits properly.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5StatsACErrors
BurstErrors | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.BurstErrors
Description | string | Note: The use of this method has been deprecated. Deprecated description: This counter is incremented when a station detects the absence of transitions for five half-bit timers (burst-five errors).
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5StatsBurstErrors
FrameCopiedErrors | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.FrameCopiedErrors
Description | string | Note: The use of this method has been deprecated. Deprecated description: This counter is incremented when a station recognizes a frame that is addressed to its specific address and detects that the FS field A bits are set to 1, which indicates a possible line hit or duplicate address.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsFrameCopiedErrors
FrequencyErrors | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.FrequencyErrors
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of times that the Device has detected that the frequency of the incoming signal differs from the expected frequency by more than that specified by the IEEE 802.5 standard.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5StatsFreqErrors
HardErrors | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.HardErrors
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of times that this Device has detected an immediately recoverable fatal error. This method indicates the number of times that this Device is either transmitting or receiving beacon MAC frames.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5StatsHardErrors
InternalErrors | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.InternalErrors
Description | string | Note: The use of this method has been deprecated. Deprecated description: This counter is incremented when a station recognizes an internal error.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsInternalErrors
LobeWires | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.LobeWires
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of times that the Device has detected an open or short circuit in the lobe data path. The adapter will be closed and RingState will signify this condition.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5StatsLobeWires
LostFrameErrors | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.LostFrameErrors
Description | string | Note: The use of this method has been deprecated. Deprecated description: This counter is incremented when a station is transmitting and its TRR timer expires. This result indicates a condition where a transmitting station in strip mode does not receive the trailer of the frame before the TRR timer goes off.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsLostFrameErrors
MaxDataSize | uint32 |
Deprecated | string | CIM_TokenRingPort.MaxDataSize
Description | string | Note: The use of this method has been deprecated. Deprecated description: The maximum size of the INFO (non-MAC) field that will be received or transmitted.
MappingStrings | string | MIB.IETF|BRIDGE-MIB.dot1dTpPortMaxInfo
ReceiveCongestions | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.ReceiveCongestions
Description | string | Note: The use of this method has been deprecated. Deprecated description: This counter is incremented when a station recognizes a frame addressed to its specific address but has no available buffer space, which indicates that the station is congested.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsReceiveCongestions
Recoverys | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.Recoverys
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of Claim Token MAC frames that are received or transmitted after the Device has received a Ring Purge MAC frame. This counter signifies the number of times that the ring has been purged and is being recovered back into a normal operating state.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5StatsRecoverys
Removes | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.Removes
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of times that the Device has received a Remove Ring Station MAC frame request. When this frame is received, the Device will enter the close state and RingState will signify this condition.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5StatsRemoves
RingOpenStatus | uint16 |
Deprecated | string | CIM_TokenRingPort.RingOpenStatus
Description | string | Note: The use of this property has been deprecated. Deprecated description: This property indicates the success, or the reason for failure, of the most recent attempt of the station to enter the ring.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5RingOpenStatus
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10
Values | string | No Open Attempted, Bad Parameter, Lobe Failed, Signal Loss, Insertion Timeout, Ring Failed, Beaconing, Duplicate MAC, Request Failed, Remove Received, Last Open Successful
RingSpeed | uint16 |
Deprecated | string | CIM_TokenRingPort.RingSpeed
Description | string | Note: The use of this method has been deprecated. Deprecated description: The bandwidth of the ring.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5RingSpeed
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, One Megabit, Four Megabit, Sixteen Megabit
RingState | uint16 |
Deprecated | string | CIM_TokenRingPort.RingState
Description | string | Note: The use of this method has been deprecated. Deprecated description: The current Device state with respect to entering or leaving the ring.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5RingState
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Opened, Closed, Opening, Closing, Open Failure, Ring Failure
RingStatus | uint32 |
Deprecated | string | CIM_TokenRingPort.RingStatus
Description | string | Note: The use of this method has been deprecated. Deprecated description: The current status that can be used to diagnose fluctuating problems that can occur on token rings, after a station has successfully been added to the ring. Before an open is completed, this object contains the value that indicates "no status" (131072). (The RingState and RingOpenStatus properties are also provided for debugging problems when the station cannot even enter the ring.) The value of the property is a sum of values, one for each currently applicable condition. The following values are defined for various conditions: 0=No Problems Detected, 32=Ring Recovery, 64=Single Station, 256=Remove Received, 512=Reserved, 1024= Auto-Removal Error, 2048=Lobe Wire Fault, 4096=Transmit Beacon, 8192=Soft Error, 16384=Hard Error, 32768=Signal Loss, 131072=No Status, Open Not Completed.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5RingStatus
SignalLossCount | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.SignalLossCount
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of times that this Device has detected the loss of signal condition from the ring.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5StatsSignalLoss
Singles | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.Singles
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of times that the Device has sensed that it is the only station on the ring. This situation occurs if the Device is the first one up on a ring or if there is a hardware problem.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5StatsSingles
SoftErrors | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.SoftErrors
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of Soft Errors that the Device has detected. This method directly corresponds to the number of Report Error MAC frames that this Device has transmitted. Soft Errors are those that are recoverable by the MAC layer protocols.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5StatsSoftErrors
TokenErrors | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.TokenErrors
Description | string | Note: The use of this method has been deprecated. Deprecated description: This counter is incremented when a station that acts as the active monitor recognizes an error condition that needs a token transmitted.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5StatsTokenErrors
TransmittedBeacons | uint32 |
Counter | boolean | true
Deprecated | string | CIM_TokenRingPortStatistics.TransmittedBeacons
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of times that this Device has transmitted a beacon frame.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token RingMIB.dot5StatsTransmitBeacons
Capabilities | uint16[] |
ArrayType | string | Indexed
Deprecated | string | CIM_TokenRingPort.Capabilities
Description | string | Note: The use of this method has been deprecated. Deprecated description: Capabilities of the TokenRingAdapter. For example, the Device might support AlertOnLan, WakeOnLan, Load Balancing, or Failover. If failover or load balancing capabilities are listed, a SpareGroup (failover) or ExtraCapacityGroup (load balancing) should also be defined to completely describe the capability.
ModelCorrespondence | string | CIM_TokenRingPort.CapabilityDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Unknown, Other, AlertOnLan, WakeOnLan, FailOver, LoadBalancing
CapabilityDescriptions | string[] |
ArrayType | string | Indexed
Deprecated | string | CIM_TokenRingPort.CapabilityDescriptions
Description | string | Note: The use of this method has been deprecated. Deprecated description: An array of free-form strings that provides more detailed explanations for any of the TokenRingAdapter features that are indicated in the Capabilities array. Note, each entry of this array is related to the entry in the Capabilities array that is located at the same index.
ModelCorrespondence | string | CIM_TokenRingAdapter.Capabilities
EnabledCapabilities | uint16[] |
Deprecated | string | CIM_TokenRingPort.EnabledCapabilities
Description | string | Note: The use of this method has been deprecated. Deprecated description: Specifies which of the capabilities from the "Capabilities" property are currently enabled.
ModelCorrespondence | string | CIM_TokenRingAdapter.Capabilities
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Unknown, Other, AlertOnLan, WakeOnLan, FailOver, LoadBalancing
NetworkAddresses | string[] |
ArrayType | string | Indexed
Deprecated | string | CIM_TokenRingAdapter.NetworkAddresses
Description | string | Note: The use of this method has been deprecated. Deprecated description: Token Ring/802.5 MAC addresses formatted as twelve hexadecimal digits (for example, "010203040506"), with each pair representing one of the six octets of the MAC address in "canonical" bit order. (Therefore, the Group address bit is found in the low order bit of the first character of the string.)
MappingStrings | string | MIF.DMTF|Network Adapter 802 Port|001.3
MaxLen | uint32 | 64
Override | string | NetworkAddresses

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AutoSense | boolean | CIM_NetworkAdapter
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
FullDuplex | boolean | CIM_NetworkAdapter
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
MaxSpeed | uint64 | CIM_NetworkAdapter
Name | string | CIM_ManagedSystemElement
OctetsReceived | uint64 | CIM_NetworkAdapter
OctetsTransmitted | uint64 | CIM_NetworkAdapter
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PermanentAddress | string | CIM_NetworkAdapter
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Speed | uint64 | CIM_NetworkAdapter
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice