# Class CIM_EthernetPort
extends CIM_NetworkPort

Capabilities and management of an EthernetPort.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_LogicalPort
|
+--CIM_NetworkPort
|
+--CIM_EthernetPort

## Direct Known Subclasses

CIM_LLDPEthernetPort

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of an EthernetPort.
ModelCorrespondence | string | CIM_NetworkPort.OtherNetworkPortType
UMLPackagePath | string | CIM::Device::Ports
Version | string | 2.35.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
MaxDataSize | uint32 |
Description | string | The maximum size of the INFO (non-MAC) field that will be received or transmitted.
MappingStrings | string | MIB.IETF|BRIDGE-MIB.dot1dTpPortMaxInfo
PoEPowerEntityType | uint16 |
Description | string | This property indicates the Power over Ethernet power entity type.
ValueMap | string | 0, 1, 2, 3, ..
Values | string | None, Other, Power Sourcing Equipment, Powered Device, DMTF Reserved
PortType | uint16 |
Description | string | The specific mode that is currently enabled for the Port. When set to 1 ("Other"), the related property OtherPortType contains a string description of the type of port.
ModelCorrespondence | string | CIM_NetworkPort.OtherNetworkPortType
Override | string | PortType
ValueMap | string | 0, 1, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 100, 101, 102, 103, 104, 105, 106, 107, 108, 109, 110, 111, 112, 200, 201, 202, 203, 204, 300, 301, 302, 303, 304, 305, 306, 16000..65535
Values | string | Unknown, Other, 10BaseT, 10-100BaseT, 100BaseT, 1000BaseT, 2500BaseT, 10GBaseT, 10GBase-CX4, 1000Base-KX, 10GBase-KX4, 10GBase-KR, 1000-10GBase-KX, 1000Base-KX10GBase-KX4KR, 10-100-1000BaseT, 100-1000-10GBaseT, 100Base-FX, 100Base-SX, 1000Base-SX, 1000Base-LX, 1000Base-CX, 10GBase-SR, 10GBase-SW, 10GBase-LX4, 10GBase-LR, 10GBase-LW, 10GBase-ER, 10GBase-EW, 10GBase-LRM, 40GBase-KR4, 40GBase-CR4, 40GBase-SR4, 40GBase-FR, 40GBase-LR4, 100GBase-CR10, 100GBase-SR10, 100GBase-LR4, 100GBase-ER4, 100GBase-KR4, 100GBase-CR4, 100GBase-KP4, Vendor Reserved
PVID | uint16 |
Description | string | Each ethernet port on an ethernet switch has a VLAN ID that is called Port VLAN ID (PVID). The PVID will be applied to the frames which are untagged or tagged with priority ( vid = 0 ). This property indicates the PVID of the Ethernet port.
Write | boolean | true
Capabilities | uint16[] |
ArrayType | string | Indexed
Description | string | Capabilities of the EthernetPort. For example, the Device might support AlertOnLan, WakeOnLan, Load Balancing, or FailOver. If failover or load balancing capabilities are listed, a SpareGroup (failover) or ExtraCapacityGroup (load balancing) should also be defined to completely describe the capability. LLDP indicates that this Ethernet Port is capable of supporting Link Layer Discovery Protocol (LLDP) communications. PoE indicates that this Ethernet Port is capable of supporting Power over Ethernet (PoE). EEE indicates that this Ethernet Port is capable of supporting Energy Efficient Ethernet (EEE). DCE indicates that this Ethernet Port is capable of supporting Data Center Ethernet. Data Center Ethernet requires support for Prioritiy-Based Flow Control (PFC), Enhanced Transmission Selection (ETS), and Data Center Bridging eXchange (DCBX) protocol. VDP indicates that this Ethernet Port is capable of supporting Virtual Station Interface (VSI) Discovery Protocol. S-Channel indicates that this Ethernet Port is capable of supporting S-Channel.
ModelCorrespondence | string | CIM_EthernetPort.CapabilityDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, ..
Values | string | Unknown, Other, AlertOnLan, WakeOnLan, FailOver, LoadBalancing, LLDP, PoE, EEE, DCE, VDP, S-Channel, DMTF Reserved
CapabilityDescriptions | string[] |
ArrayType | string | Indexed
Description | string | An array of free-form strings that provides more detailed explanations for any of the EthernetPort features that are indicated in the Capabilities array. Note, each entry of this array is related to the entry in the Capabilities array that is located at the same index.
ModelCorrespondence | string | CIM_EthernetPort.Capabilities
EnabledCapabilities | uint16[] |
ArrayType | string | Indexed
Description | string | Specifies which capabilities are enabled from the list of all supported ones, which are defined in the Capabilities array. For details on each capability, see the description of each capability in the description of property Capabilities.
ModelCorrespondence | string | CIM_EthernetPort.Capabilities, CIM_EthernetPort.OtherEnabledCapabilities
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, ..
Values | string | Unknown, Other, AlertOnLan, WakeOnLan, FailOver, LoadBalancing, LLDP, PoE, EEE, DCE, VDP, S-Channel, DMTF Reserved
NetworkAddresses | string[] |
Description | string | Ethernet/802.3 MAC addresses formatted as twelve hexadecimal digits (for example, "010203040506"), with each pair representing one of the six octets of the MAC address in "canonical" bit order. (Therefore, the Group address bit is found in the low order bit of the first character of the string.)
MappingStrings | string | MIF.DMTF|Network Adapter 802 Port|001.3
MaxLen | uint32 | 64
Override | string | NetworkAddresses
OtherEnabledCapabilities | string[] |
ArrayType | string | Indexed
Description | string | An array of free-form strings that provides more detailed explanations for any of the enabled capabilities that are specified as 'Other'.
ModelCorrespondence | string | CIM_EthernetPort.EnabledCapabilities
PortDiscriminator | string[] |
Description | string | A string array used to discriminate the supported context of this EthernetPort. The following strings are currently defined: 'SNIA:None' - indicates this EthernetPort does not provide support for any specific function. 'SNIA:iSCSI' - indicates this EthernetPort provides support for iSCSI. 'SNIA:FCoE' - indicates that this EthernetPort provides support for FC over Ethernet - FCoE.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
ActiveMaximumTransmissionUnit | uint64 | CIM_NetworkPort
AutoSense | boolean | CIM_NetworkPort
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
FullDuplex | boolean | CIM_NetworkPort
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LinkTechnology | uint16 | CIM_NetworkPort
MaxQuiesceTime | uint64 | CIM_LogicalDevice
MaxSpeed | uint64 | CIM_LogicalPort
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherLinkTechnology | string | CIM_NetworkPort
OtherNetworkPortType | string | CIM_NetworkPort
OtherPortType | string | CIM_LogicalPort
PermanentAddress | string | CIM_NetworkPort
PortNumber | uint16 | CIM_NetworkPort
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedSpeed | uint64 | CIM_LogicalPort
RequestedState | uint16 | CIM_EnabledLogicalElement
Speed | uint64 | CIM_NetworkPort
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SupportedMaximumTransmissionUnit | uint64 | CIM_NetworkPort
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
UsageRestriction | uint16 | CIM_LogicalPort
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice