# Class CIM_SecurityAssociationEndpoint
extends CIM_ProtocolEndpoint

SecurityAssociationEndpoint (SAEndpoint) represents the endpoint of a secure connection. This is typically an IP connection, although the model allows more flexibility than just IP. The SecurityAssociationEndpoint is tied to an IPProtocolEndpoint (or possibly other endpoint) using the LogicalIdentity association. Note that an endpoint is defined at both ends of the connection.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_ProtocolEndpoint
|
+--CIM_SecurityAssociationEndpoint

## Direct Known Subclasses

CIM_IKESAEndpoint
CIM_IPsecSAEndpoint

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | SecurityAssociationEndpoint (SAEndpoint) represents the endpoint of a secure connection. This is typically an IP connection, although the model allows more flexibility than just IP. The SecurityAssociationEndpoint is tied to an IPProtocolEndpoint (or possibly other endpoint) using the LogicalIdentity association. Note that an endpoint is defined at both ends of the connection.
UMLPackagePath | string | CIM::Network::IPsec
Version | string | 2.8.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
IdleDurationSeconds | uint64 | 0
Description | string | IdleDurationSeconds specifies how long the SA can be idle before it is deleted. The default value, 0, indicates that there is no idle timeout period.
Units | string | Seconds
InstallDate | datetime |
Description | string | InstallDate records when the SA (and its endpoint) was created.
MappingStrings | string | MIF.DMTF|ComponentID|001.5
Override | string | InstallDate
LifetimeKilobytes | uint64 | 0
Description | string | LifetimeKilobytes specifies the maximum number of kilobytes of data traffic to be protected by the SA. A value of zero (the default) indicates that there should be no maximum kilobyte lifetime. A non-zero value specifies the desired kilobyte lifetime. The SA is deleted when the LifetimeKilobyte value is exceeded.
Units | string | KiloBytes
LifetimeSeconds | uint64 | 0
Description | string | LifetimeSeconds specifies the maximum time that the SA will be considered valid after it has been created. A value of zero indicates that the default of 8 hours be used. A non-zero value indicates the seconds lifetime.
Units | string | Seconds
PacketLoggingActive | boolean |
Description | string | PacketLoggingActive causes a log to be kept of traffic processed by the SAEndpoint.
Write | boolean | true
RefreshThresholdKbytesPercentage | uint8 |
Description | string | RefreshThresholdKbytesPercentage is the lifetime percentage of kilobytes processed, at which a new SA should be acquired. A random value may be added to the calculated threshold to reduce network thrashing.
MaxValue | sint64 | 100
MinValue | sint64 | 0
Units | string | Percent
Write | boolean | true
RefreshThresholdSecondsPercentage | uint8 |
Description | string | RefreshThresholdSecondsPercentage is the lifetime percentage after which a new SA should be acquired, before the existing SA expires. A random period may be added to a calculated threshold to reduce network thrashing.
MaxValue | sint64 | 100
MinValue | sint64 | 0
Units | string | Percent
Write | boolean | true

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_ServiceAccessPoint
Description | string | CIM_ProtocolEndpoint
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_ProtocolEndpoint
HealthState | uint16 | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
Name | string | CIM_ProtocolEndpoint
NameFormat | string | CIM_ProtocolEndpoint
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherTypeDescription | string | CIM_ProtocolEndpoint
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolIFType | uint16 | CIM_ProtocolEndpoint
ProtocolType | uint16 | CIM_ProtocolEndpoint
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_ServiceAccessPoint
SystemName | string | CIM_ServiceAccessPoint
TimeOfLastStateChange | datetime | CIM_ProtocolEndpoint
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ProtocolEndpoint
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
RequestStateChange | uint32 | CIM_EnabledLogicalElement