# Class CIM_WiFiEndpointCapabilities
extends CIM_EnabledLogicalElementCapabilities

Describes the capabilities of a WiFiEndpoint.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Capabilities
|
+--CIM_EnabledLogicalElementCapabilities
|
+--CIM_WiFiEndpointCapabilities

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Describes the capabilities of a WiFiEndpoint.
UMLPackagePath | string | CIM::Network::Wireless
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
OtherSupportedAuthenticationMethods | string[] |
ArrayType | string | Indexed
Description | string | Shall contain additional authentication methods supported by the associated WifiEndpoint, but not listed in the valuemap for SupportedAuthenticationMethods. The positions of these strings are the lowest indices of the array, and do not correspond to the positions of the values in SupportedAuthenticationMethods.
ModelCorrespondence | string | CIM_WiFiEndpoint.OtherAuthenticationMethod
OtherSupportedEncryptionMethods | string[] |
Description | string | Shall contain additional encryption methods supported by the associated WifiEndpoint, but not listed in the valuemap for SupportedEncryptionMethods. The positions of these strings are the lowest indices of the array, and do not correspond to the positions of the values in SupportedEncryptionMethods.
ModelCorrespondence | string | CIM_WiFiEndpoint.OtherEncryptionMethod
SupportedAuthenticationMethods | uint16[] |
ArrayType | string | Indexed
Description | string | The set of IEEE 802.11 authentication methods supported by the associated WifiEndpoint. * Other (1): shall indicate that at least one authentication method not specified in the list below is supported. If SupportedAuthenticationMethods contains 1, OtherSupportedAuthenticationMethods shall not be NULL and shall not be empty. * Open System (2): shall indicate that Open System authentication is supported. SupportedAuthenticationMethods shall contain 2 only if SupportedEncryptionMethods contains 2 ("WEP") or 5 ("None"). * Shared Key (3): shall indicate Shared Key authentication is supported. SupportedAuthenticationMethods shall contain 3 only if SupportedEncryptionMethods contains 2 ("WEP") or 5 ("None"). * WPA PSK (4): shall indicate that WPA (Wi-Fi Protected Access) PSK (Pre-Shared Key) authentication is supported. SupportedAuthenticationMethods shall contain 4 only if SupportedEncryptionMethods contains 3 ("TKIP") or 4 ("CCMP"). * WPA IEEE 802.1x (5): shall indicate that WPA (Wi-Fi Protected Access) IEEE 802.1x authentication is supported. SupportedAuthenticationMethods shall contain 5 only if SupportedEncryptionMethods contains 3 ("TKIP") or 4 ("CCMP"). * WPA2 PSK (6): shall indicate that WPA2 (Wi-Fi Protected Access Version 2) PSK (Pre-Shared Key) authentication is supported. SupportedAuthenticationMethods shall contain 6 only if SupportedEncryptionMethods contains 3 ("TKIP") or 4 ("CCMP"). * WPA2 IEEE 802.1x (7): shall indicate that WPA2 (Wi-Fi Protected Access Version 2) IEEE 802.1x authentication is supported. SupportedAuthenticationMethods shall contain 7 only if SupportedEncryptionMethods contains 3 ("TKIP") or 4 ("CCMP").
MappingStrings | string | IEEE 802.11-2007 | 8
ModelCorrespondence | string | CIM_WiFiEndpoint.AuthenticationMethod
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, ..
Values | string | Other, Open System, Shared Key, WPA PSK, WPA IEEE 802.1x, WPA2 PSK, WPA2 IEEE 802.1X, DMTF Reserved
SupportedEncryptionMethods | uint16[] |
Description | string | The set of IEEE 802.11 encryption methods supported by the associated WifiEndpoint. Shall contain one or more of the values below. * Other (1): shall indicate that at least one encryption method not specified in the list below is supported. If SupportedEncryptionMethods contains 1, OtherSupportedEncryptionMethods shall not be NULL and shall not be empty. * WEP (2): shall indicate that Wired Equivalency Privacy (WEP) is supported. SupportedEncryptionMethods shall contain 2 only if SupportedAuthenticationMethods contains 2 ("Open System") or 3 ("Shared Key"). * TKIP (3): shall indicate that the Temporal Key Integrity Protocol (TKIP) is supported. SupportedEncryptionMethods shall contain 3 only if SupportedAuthenticationMethods contains 4 ("WPA PSK"), 5 ("WPA IEEE 802.1x"), 6 ("WPA2 PSK"), or 7 ("WPA2 IEEE 802.1x"). * CCMP (4): shall indicate that the Counter Mode with Cipher Block Chaining Message Authentication Code Protocol (CCMP) is supported. SupportedEncryptionMethods shall contain 4 only if SupportedAuthenticationMethods contains 4 ("WPA PSK"), 5 ("WPA IEEE 802.1x"), 6 ("WPA2 PSK"), or 7 ("WPA2 IEEE 802.1x"). * None (5): shall indicate that the associated WiFiEndpoint supports connecting to a network without encryption. SupportedEncryptionMethods shall contain 5 only if SupportedAuthenticationMethods contains 2 ("Open System") or 3 ("Shared Key").
MappingStrings | string | IEEE 802.11-2007 | 8
ModelCorrespondence | string | CIM_WiFiEndpoint.EncryptionMethod
ValueMap | string | 1, 2, 3, 4, 5, ..
Values | string | Other, WEP, TKIP, CCMP, None, DMTF Reserved

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_Capabilities
ElementNameEditSupported | boolean | CIM_EnabledLogicalElementCapabilities
ElementNameMask | string | CIM_EnabledLogicalElementCapabilities
InstanceID | string | CIM_Capabilities
MaxElementNameLen | uint16 | CIM_EnabledLogicalElementCapabilities
RequestedStatesSupported | uint16[] | CIM_EnabledLogicalElementCapabilities

## Class Methods