# Class CIM_VideoController
extends CIM_Controller

Note: The use of the CIM_VideoController class has been deprecated in lieu of CIM_DisplayController. Deprecated description: Capabilities and management of the VideoController.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Controller
|
+--CIM_VideoController

## Direct Known Subclasses

CIM_AGPVideoController
CIM_PCVideoController

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_DisplayController,CIM_VideoHead
Description | string | Note: The use of the CIM_VideoController class has been deprecated in lieu of CIM_DisplayController. Deprecated description: Capabilities and management of the VideoController.
UMLPackagePath | string | CIM::Device::Controller
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CurrentBitsPerPixel | uint32 |
Deprecated | string | CIM_VideoHead.CurrentBitsPerPixel
Description | string | The number of bits used to display each pixel.
MappingStrings | string | MIF.DMTF|Video|004.12
PUnit | string | bit
Units | string | Bits
CurrentHorizontalResolution | uint32 |
Deprecated | string | CIM_VideoHead.CurrentHorizontalResolution
Description | string | Current number of horizontal pixels.
MappingStrings | string | MIF.DMTF|Video|004.11
PUnit | string | pixel
Units | string | Pixels
CurrentNumberOfColors | uint64 |
Deprecated | string | CIM_VideoHead.CurrentNumberOfColors
Description | string | The number of colors that are supported at the current resolutions.
CurrentNumberOfColumns | uint32 |
Deprecated | string | CIM_VideoHead.CurrentNumberOfColumns
Description | string | If in character mode, the number of columns for this VideoController. Otherwise, enter 0.
MappingStrings | string | MIF.DMTF|Video|004.14
CurrentNumberOfRows | uint32 |
Deprecated | string | CIM_VideoHead.CurrentNumberOfRows
Description | string | If in character mode, the number of rows for this Video Controller. Otherwise, enter 0.
MappingStrings | string | MIF.DMTF|Video|004.13
CurrentRefreshRate | uint32 |
Deprecated | string | CIM_VideoHead.CurrentRefreshRate
Description | string | Current refresh rate in hertz.
MappingStrings | string | MIF.DMTF|Video|004.15
PUnit | string | hertz
Units | string | Hertz
CurrentScanMode | uint16 |
Deprecated | string | CIM_VideoHead.CurrentScanMode
Description | string | Current scan mode. "Interlaced" (value=3) or "Non Interlaced" (value=4) can be defined using this property.
MappingStrings | string | MIF.DMTF|Video|004.8
ValueMap | string | 1, 2, 3, 4
Values | string | Other, Unknown, Interlaced, Non Interlaced
CurrentVerticalResolution | uint32 |
Deprecated | string | CIM_VideoHead.CurrentVerticalResolution
Description | string | Current number of vertical pixels.
MappingStrings | string | MIF.DMTF|Video|004.10
PUnit | string | pixel
Units | string | Pixels
Description | string |
Deprecated | string | No value
Description | string | The Description property provides a textual description of the object.
MappingStrings | string | MIF.DMTF|Video|004.18
Override | string | Description
MaxMemorySupported | uint32 |
Deprecated | string | CIM_DisplayController.MaxMemorySupported
Description | string | Maximum amount of memory supported in bytes.
PUnit | string | byte
Units | string | Bytes
MaxRefreshRate | uint32 |
Deprecated | string | CIM_VideoHead.MaxRefreshRate
Description | string | Maximum refresh rate of the VideoController in hertz.
MappingStrings | string | MIF.DMTF|Video|004.5
PUnit | string | hertz
Units | string | Hertz
MinRefreshRate | uint32 |
Deprecated | string | CIM_VideoHead.MinRefreshRate
Description | string | Minimum refresh rate of the Video Controller in hertz.
MappingStrings | string | MIF.DMTF|Video|004.4
PUnit | string | hertz
Units | string | Hertz
NumberOfVideoPages | uint32 |
Deprecated | string | CIM_DisplayController.NumberOfVideoPages
Description | string | Number of video pages that are supported given the current resolutions and available memory.
VideoMemoryType | uint16 |
Deprecated | string | CIM_DisplayController.VideoMemoryType
Description | string | An integer enumeration that indicates the type of video memory.
MappingStrings | string | MIF.DMTF|Video|004.6
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13
Values | string | Other, Unknown, VRAM, DRAM, SRAM, WRAM, EDO RAM, Burst Synchronous DRAM, Pipelined Burst SRAM, CDRAM, 3DRAM, SDRAM, SGRAM
VideoProcessor | string |
Deprecated | string | CIM_DisplayController.VideoProcessor
Description | string | A free-form string that describes the video processor or Controller.
AcceleratorCapabilities | uint16[] |
ArrayType | string | Indexed
Deprecated | string | CIM_DisplayController.AcceleratorCapabilities
Description | string | An array of integers that indicates the graphics and 3D capabilities of the VideoController.
ModelCorrespondence | string | CIM_VideoController.CapabilityDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8
Values | string | Unknown, Other, Graphics Accelerator, 3D Accelerator, PCI Fast Write, MultiMonitor Support, PCI Mastering, Second Monochrome Adapter Support, Large Memory Address Support
CapabilityDescriptions | string[] |
ArrayType | string | Indexed
Deprecated | string | CIM_DisplayController.CapabilityDescriptions
Description | string | An array of free-form strings that provides more detailed explanations for any of the video Accelerator features that are indicated in the Capabilities array. Note, each entry of this array is related to the entry in the Capabilities array that is located at the same index.
ModelCorrespondence | string | CIM_VideoController.AcceleratorCapabilities

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
MaxNumberControlled | uint32 | CIM_Controller
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolDescription | string | CIM_Controller
ProtocolSupported | uint16 | CIM_Controller
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastReset | datetime | CIM_Controller
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice