# Class CIM_IPConfigurationService
extends CIM_Service

CIM_IPConfigurationService provides management of the IP configuration associated with a LANEndpoint or IPProtocolEndpoint or IPNetworkConnection or the global IP configuration for the ComputerSystem.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_IPConfigurationService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | CIM_IPConfigurationService provides management of the IP configuration associated with a LANEndpoint or IPProtocolEndpoint or IPNetworkConnection or the global IP configuration for the ComputerSystem.
UMLPackagePath | string | CIM::Network::IP
Version | string | 2.32.0

## Class Properties

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Local Class Methods

#### ApplySettingToIPProtocolEndpoint (uint32)

#### Method Qualifiers (ApplySettingToIPProtocolEndpoint)

Name | Data Type | Value
--- | --- | ---
Description | string | Apply the configuration represented by the CIM_IPAssignmentSettingData to the specified IPProtocolEndpoint. This will result in the value of the IsCurrent property of the CIM_ElementSettingData which associates the specified CIM_IPAssignmentSettingData and specified CIM_IPProtocolEndpoint having a value of "true". The IsCurrent property of any other instances of CIM_ElementSettingData which reference the specified CIM_IPProtocolEndpoint and an instance of CIM_IPAssignmentSettingData will have a value of "false". Each instance of CIM_IPAssignmentSettingData which is aggregated into the target CIM_IPAssignmentSettingData instance will be applied to the CIM_ProtocolEndpoint to which it is associated via an instance of CIM_ElementSettingData where the CIM_ProtocolEndpoint is associated with the target CIM_IPProtocolEndpoint via an instance of CIM_EndpointIdentity.
ValueMap | string | 0, 1, 2, 3, 4, 5, 4096, .., 32768..65535
Values | string | Completed with No Error, Not Supported, Unknown/Unspecified Error, Failed, Invalid Parameter, Busy, Method Parameters Checked - Job Started, DMTF Reserved, Vendor Reserved

#### Method Parameters (ApplySettingToIPProtocolEndpoint)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Configuration | REF CIM_IPAssignmentSettingData
Description | string | The IPAssignmentSettingData to apply.
IN | boolean | true
Required | boolean | true
Endpoint | REF CIM_IPProtocolEndpoint
Description | string | The IPProtocolEndpoint to which the configuration will be applied.
IN | boolean | true
Required | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job spawned if the operation continues after the method returns. This parameter MUST NOT be null if a value of 4096 is returned. This parameter MUST be null if any other value is returned by the method.
IN | boolean | false
OUT | boolean | true

#### ApplySettingToComputerSystem (uint32)

#### Method Qualifiers (ApplySettingToComputerSystem)

Name | Data Type | Value
--- | --- | ---
Description | string | Apply the IP Version respresented by the CIM_IPVersionSettingData to the specified ComputerSystem. The IP Version may take effect or disable immediatley or may be set to take effect or disable in the next boot, depending on ComputerSystem and the value specified for Mode. This will reflect in the IsCurrent & IsNext property of CIM_ElementSettingData associating the IPVersionSettingData with the ComputerSystem. Refer the description for the Mode parameter for more details.
ValueMap | string | 0, 1, 2, 4096, .., 32768..65535
Values | string | Completed with No Error, Not Supported, Failed, Job Started, DMTF Reserved, Vendor Reserved

#### Method Parameters (ApplySettingToComputerSystem)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Mode | uint16
Description | string | The mode in which the configuration need to be applied to the ComputerSystem. Mode 0 - implies use Mode 1 if allowed, else Mode 2. Mode 1 - Results in IsNext = 1 (Is Next), IsCurrent = 1 (Is Current) for the CIM_ElementSettingData associating the setting with ComputerSystem. Mode 2 - Results in IsNext = 1 (Is Next) for the CIM_ElementSettingData associating the setting with ComputerSystem. The value of IsCurrent will not be affected. Mode 3 - implies use Mode 4 if allowed, else Mode 5. Mode 4 - Results in IsNext = 2 (Is Not Next), IsCurrent = 2 (Is Not Current) for the CIM_ElementSettingData associating the setting with ComputerSystem. Mode 5 - Results in IsNext = 2 (Is Not Next) for the CIM_ElementSettingData associating the setting with ComputerSystem. The value of IsCurrent will not be affected. Mode 6 - Results in IsNext = 3 (Is Next For Single Use)for the CIM_ElementSettingData associating the setting with ComputerSystem. The value of IsCurrent will not be affected. To change the IsNext=3 (Is Next For Single Use) for a Setting, invoke the method with any of the other values for the mode.
IN | boolean | true
Required | boolean | true
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 32768..65535
Values | string | Mode 0, Mode 1, Mode 2, Mode 3, Mode 4, Mode 5, Mode 6, DMTF Reserved, Vendor Reserved
ComputerSystem | REF CIM_ComputerSystem
Description | string | The ComputerSystem to which the setting will be applied
IN | boolean | true
Required | boolean | true
IPVersionSettingData | REF CIM_IPVersionSettingData
Description | string | The IPVersionSettingData to be apply.
IN | boolean | true
Required | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job spawned if the operation continues after the method returns. (may be null if task completed).
IN | boolean | false
OUT | boolean | true

#### ApplySettingToIPNetworkConnection (uint32)

#### Method Qualifiers (ApplySettingToIPNetworkConnection)

Name | Data Type | Value
--- | --- | ---
Description | string | Apply the IP setting respresented by the CIM_IPAssignmentSettingData and/or the IPVersion Setting respresented by the CIM_IPVersionSettingData to the specified IPNetworkConnection. The settings may take effect or disable immediatley or may be set to take effect or disable in the next boot, depending on system, IPNetworkConnection, Setting and the value specified for Mode. This will reflect in the IsCurrent & IsNext property of instances of CIM_ElementSettingData associating the SettingData and or IPVersionSettingData with the IPNetworkConnection. For cases, enabling one setting can result in automatic disabling of another setting, it will be refelected in the properties of ElementSettingData associating those settings to the IPNetworkConnection.Refer the description for the Mode parameter for more details. At least one of the SettingData or IPVersionSettingData is required in the method call; both may be specified on the same method call.
ValueMap | string | 0, 1, 2, 4096, .., 32768..65535
Values | string | Completed with No Error, Not Supported, Failed, Job Started, DMTF Reserved, Vendor Reserved

#### Method Parameters (ApplySettingToIPNetworkConnection)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Mode | uint16
Description | string | The mode in which the configuration need to be applied to the IPNetworkConnection. Mode 0 - implies use Mode 1 if allowed, else Mode 2. Mode 1 - Results in IsNext = 1 (Is Next), IsCurrent = 1 (Is Current) for the CIM_ElementSettingData associating the setting with IPNetworkConnection. Mode 2 - Results in IsNext = 1 (Is Next) for the CIM_ElementSettingData associating the setting with IPNetworkConnection. The value of IsCurrent will not be affected. Mode 3 - implies use Mode 4 if allowed, else Mode 5. Mode 4 - Results in IsNext = 2 (Is Not Next), IsCurrent = 2 (Is Not Current) for the CIM_ElementSettingData associating the setting with IPNetworkConnection. Mode 5 - Results in IsNext = 2 (Is Not Next) for the CIM_ElementSettingData associating the setting with IPNetworkConnection. The value of IsCurrent will not be affected. Mode 6 - Results in IsNext = 3 (Is Next For Single Use)for the CIM_ElementSettingData associating the setting with IPNetworkConnection. The value of IsCurrent will not be affected. To change the IsNext=3 (Is Next For Single Use) for a Setting, invoke the method with any of the other values for the mode.
IN | boolean | true
Required | boolean | true
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 32768..65535
Values | string | Mode 0, Mode 1, Mode 2, Mode 3, Mode 4, Mode 5, Mode 6, DMTF Reserved, Vendor Reserved
IPNetworkConnection | REF CIM_IPNetworkConnection
Description | string | The IPNetworkConnection to which the setting will be applied
IN | boolean | true
Required | boolean | true
IPVersionSettingData | REF CIM_IPVersionSettingData
Description | string | The IPVersionSettingData to be apply.
IN | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job spawned if the operation continues after the method returns. (may be null if task completed).
IN | boolean | false
OUT | boolean | true
SettingData | REF CIM_IPAssignmentSettingData
Description | string | The IPAssignmentSettingData to apply.
IN | boolean | true

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
RequestStateChange | uint32 | CIM_EnabledLogicalElement
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service