# Class CIM_SwitchVirtualInterface
extends CIM_IPProtocolEndpoint

Configuration class for a switch virtual interface which is a VLAN of switch ports represented by one interface to a routing or bridging system.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_ProtocolEndpoint
|
+--CIM_IPProtocolEndpoint
|
+--CIM_SwitchVirtualInterface

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Configuration class for a switch virtual interface which is a VLAN of switch ports represented by one interface to a routing or bridging system.
UMLPackagePath | string | CIM::Network
Version | string | 2.51.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
VLANId | uint16 |
Description | string | A 12-bit VLAN ID that this interface is dependent on.
MappingStrings | string | MIB.IETF|Q-BRIDGE-MIB.VlanId
MaxValue | sint64 | 4094
MinValue | sint64 | 1

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Address | string | CIM_IPProtocolEndpoint
AddressOrigin | uint16 | CIM_IPProtocolEndpoint
AddressType | uint16 | CIM_IPProtocolEndpoint
BroadcastResetSupported | boolean | CIM_ProtocolEndpoint
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_ServiceAccessPoint
Description | string | CIM_ProtocolEndpoint
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_ProtocolEndpoint
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IPv4Address | string | CIM_IPProtocolEndpoint
IPv6Address | string | CIM_IPProtocolEndpoint
IPv6AddressType | uint16 | CIM_IPProtocolEndpoint
IPv6SubnetPrefixLength | uint16 | CIM_IPProtocolEndpoint
IPVersionSupport | uint16 | CIM_IPProtocolEndpoint
Name | string | CIM_ProtocolEndpoint
NameFormat | string | CIM_ProtocolEndpoint
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherTypeDescription | string | CIM_ProtocolEndpoint
PrefixLength | uint8 | CIM_IPProtocolEndpoint
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolIFType | uint16 | CIM_IPProtocolEndpoint
ProtocolType | uint16 | CIM_ProtocolEndpoint
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
SubnetMask | string | CIM_IPProtocolEndpoint
SystemCreationClassName | string | CIM_ServiceAccessPoint
SystemName | string | CIM_ServiceAccessPoint
TimeOfLastStateChange | datetime | CIM_ProtocolEndpoint
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ProtocolEndpoint
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
BroadcastReset | uint32 | CIM_ProtocolEndpoint
RequestStateChange | uint32 | CIM_EnabledLogicalElement