# Class CIM_ListenerDestinationWSManagement
extends CIM_ListenerDestination

CIM_ListenerDestinationWSManagement describes the destination for CIM indications to be delivered via WS-Management.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ListenerDestination
|
+--CIM_ListenerDestinationWSManagement

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | CIM_ListenerDestinationWSManagement describes the destination for CIM indications to be delivered via WS-Management.
UMLPackagePath | string | CIM::Event
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ContentEncoding | string |
Description | string | This block acts as a hint to indicate how the delivered events should be encoded. The two standard tokens defined for this purpose are "UTF-8" or "UTF-16", although other encoding formats may be specified if necessary.
DeliveryAuth | string |
Description | string | A URI identifying the WS-Management security profile to be used by the service (acting as publisher) when authenticating to the event sink (consumer) at event delivery time.
DeliveryMode | uint16 |
Description | string | Method by which the service is to deliver events to the client. Values are as follows. Push (2): the event is sent to the destination address; depending on the protocol, delivery may not be guaranteed. PushWithAck (3): the service sends the event and waits for a specific acknowledgment message from the subscriber. Events (4): the service collects events into batches and sends the batches to the subscriber. Pull (5): the service collects the events into batches and the subscriber pulls each batch from the service using wxf:Pull.
ValueMap | string | 2, 3, 4, 5, .., 32787..
Values | string | Push, PushWithAck, Events, Pull, DMTF Reserved, Vendor Reserved
Destination | string |
Description | string | The destination URL defined in the WS-Eventing Subscribe message. This must match the wsa:Address element in the wse:NotifyTo EPR. The value may be the WS-Addressing anonymous URI if the subscription uses or employs a Pull mode.
Override | string | Destination
Required | boolean | true
DestinationEndTo | string |
Description | string | Separate To address for notice of abnormal subscription termination.
Heartbeat | uint64 |
Description | string | Specifies how often heartbeat events are added to the event stream at the specified interval.
Units | string | Seconds
Locale | string |
Description | string | If the events contain localized content, the service should accept a subscription with this Locale block acting as a hint. The language of the event message is encoded in an xml:lang attribute using RFC 3066 language codes. The service should attempt to localize any descriptive content to the specified language when delivering such events.
MaxTime | uint64 |
Description | string | This element may contain a duration that indicates the maximum amount of time the service should allow to elapse while batching EVENT bodies. That is, this time may not be exceeded between the encoding of the first event in the batch and the dispatching of the batch for delivery.
Units | string | Seconds
PolyMorphismMode | uint16 |
Description | string | Specifies the treatment of Indication subclasses, whether subclasses are to be included and with what set of properties. Valid values are: None, IncludeSubclassProperties, and ExcludeSubclassProperties. Using None, only instances of the parent class are included in the output (event stream). For other modes, subclass instances are included with the sets of properties stated.
ValueMap | string | 1, 2, 3, ..
Values | string | None, IncludeSubclassProperties, ExcludeSubclassProperties, DMTF Reserved
SendBookmark | boolean |
Description | string | A property element that instructs the service to send a bookmark with each event. Bookmarks apply to all delivery modes. The bookmark is a token which represents an abstract pointer in the event stream, but whether it points to the last delivered event or the last event plus one (the upcoming event) makes no difference since the token is supplied to the same implementation during a subsequent wse:Subscribe operation. The service may thus attach any service-specific meaning and structure to the bookmark with no change to the client.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CreationClassName | string | CIM_ListenerDestination
Description | string | CIM_ManagedElement
ElementName | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_ManagedElement
Name | string | CIM_ListenerDestination
OtherPersistenceType | string | CIM_ListenerDestination
OtherProtocol | string | CIM_ListenerDestination
password | string | CIM_ListenerDestination
PersistenceType | uint16 | CIM_ListenerDestination
Protocol | uint16 | CIM_ListenerDestination
SystemCreationClassName | string | CIM_ListenerDestination
SystemName | string | CIM_ListenerDestination
username | string | CIM_ListenerDestination

## Class Methods