# Class CIM_IPEncapsulationInterface
extends CIM_ManagedSystemElement

CIM_IPEncapsulationInterface specializes CIM_IPProtocolEndpoint to provide the additional configuration properties required for an IP tunnel interface. The IPProtocolEndpoint properties represent the inner IP address of the IP packet.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_IPEncapsulationInterface

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | CIM_IPEncapsulationInterface specializes CIM_IPProtocolEndpoint to provide the additional configuration properties required for an IP tunnel interface. The IPProtocolEndpoint properties represent the inner IP address of the IP packet.
UMLPackagePath | string | CIM::Network::Protocol Endpoint(1)
Version | string | 2.52.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CASourceEndpoint | string |
Description | string | Contains the identifier for the source endpoint traffic from the customer network. It shall be an instance of CIM_ProtocolEndpoint, for this IP Tunnel a non-null value of the CASourceEndpont property shall be formatted as a URI per RFC3986. If this resource is modeled then a value should be a WBEM URI (DSP0207).
CAVRFContext | string |
Description | string | This is an optional property for configuring the Virtual Routing and Forwarding table (a CIM_VirtualRoutingAndForwarding instance) to be used to look up the route for a customer IP address from a de-capsulated packet coming from the overlay network. A non-null value of this property shall be formated as a URI per RFC3986. If this resource is modeled then a value should be a WBEM URI (DSP0207).
EncapsulationMode | uint16 |
Description | string | 1- sets the Encapsulation mode typeOther - should only be used if there is not an enumerated value 2- GRE 3- IP-in-IP 4-NVGRE 5-VXLAN
ModelCorrespondence | string | CIM_IPEncapsulationInterface.OtherEncapsulationMode
ValueMap | string | 1, 2, 3, 4, 5, .., 0x8000..0xFFFF
Values | string | Other, GRE, IP-in-IP, NVGRE, VXLAN, DMTF Reserved, Vendor Reserved
InstanceID | string |
Description | string | InstanceID is an optional property that may be used to opaquely and uniquely identify an instance of this class within the scope of the instantiating Namespace. Various subclasses of this class may override this property to make it required, or a key. Such subclasses may also modify the preferred algorithms for ensuring uniqueness that are defined below. To ensure uniqueness within the NameSpace, the value of InstanceID should be constructed using the following "preferred" algorithm: <OrgID>:<LocalID> Where <OrgID> and <LocalID> are separated by a colon (:), and where <OrgID> must include a copyrighted, trademarked, or otherwise unique name that is owned by the business entity that is creating or defining the InstanceID or that is a registered ID assigned to the business entity by a recognized global authority. (This requirement is similar to the <Schema Name>_<Class Name> structure of Schema class names.) In addition, to ensure uniqueness, <OrgID> must not contain a colon (:). When using this algorithm, the first colon to appear in InstanceID must appear between <OrgID> and <LocalID>. <LocalID> is chosen by the business entity and should not be reused to identify different underlying (real-world) elements. If not null and the above "preferred" algorithm is not used, the defining entity must assure that the resulting InstanceID is not reused across any InstanceIDs produced by this or other providers for the NameSpace of this instance. If not set to null for DMTF-defined instances, the "preferred" algorithm must be used with the <OrgID> set to CIM.
Key | boolean | true
Override | string | InstanceID
OtherEncapsulationMode | string |
Description | string | if the EncapsulationMode has a value 1 - OtherOtherEncapsulationMode should have a string describing the tunnel mode
ModelCorrespondence | string | CIM_IPEncapsulationInterface.EncapsulationMode
PASourceEndpoint | string |
Description | string | Contains the identifier for the source endpoint traffic to the Provider (overlay) network. It shall be an instance of CIM_ProtocolEndpoint, for this IP Tunnel a non-null value of the PASourceEndpont property shall be formatted as a URI per RFC3986. If this resource is modeled then a value should be a WBEM URI (DSP0207).
PAVRFContext | string |
Description | string | This is an optional property for configuring the Virtual Routing and Forwarding table (a CIM_VirtualRoutingAndForwarding instance) to be used to look up the route for a Provide IP address from a encapsulated packet coming from the overlay network. A non-null value of this property shall shall be formated as a URI per RFC3986. If this resource is modeled then a value should be a WBEM URI (DSP0207)

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
PrimaryStatus | uint16 | CIM_ManagedSystemElement
Status | string | CIM_ManagedSystemElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods