# Class CIM_VTLStatisticalDataService
extends CIM_Service

The CIM_VTLStatisticalDataService class provides Historical Resource Usage Service. This class has set of functions to collect historical values for Front-end port performance, Physical disk usage, Logical backup data, Overall system compression ratio, Deduplication efficiency and Replication traffic. All the functions returns graph object Data point history of specified resource.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_VTLStatisticalDataService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | The CIM_VTLStatisticalDataService class provides Historical Resource Usage Service. This class has set of functions to collect historical values for Front-end port performance, Physical disk usage, Logical backup data, Overall system compression ratio, Deduplication efficiency and Replication traffic. All the functions returns graph object Data point history of specified resource.
UMLPackagePath | string | CIM::Device::StorageStatistics
Version | string | 2.45.0

## Class Properties

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LoSID | string | CIM_Service
LoSOrgID | string | CIM_Service
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Local Class Methods

#### GetPhysicalCapacityUsage (uint16)

#### Method Qualifiers (GetPhysicalCapacityUsage)

Name | Data Type | Value
--- | --- | ---
Description | string | GetPhysicalCapacityUsage Provides capacity on a per storage pool and virtual library basis. If the primordial pool is used, data is returned for all pools. If the VLS Computer System is used, capacity is returned for the entire appliance. At least one of StartTime, EndTime, and Duration must be specified. - If all three are specified, then Duration is ignored. - StartTime shall not be higher than EndTime. - No time may be set in the future. - If two of the three are specified, then the third is calculated. - If only StartTime or Duration is specified, then EndTime will be set to the current time. - If only EndTime is specified, then StartTime will be set to the time the earliest data is available.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096
Values | string | Job Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, Statistics Format Not Supported, Method Reserved, Method Parameters Checked - Job Started

#### Method Parameters (GetPhysicalCapacityUsage)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
DataFormat | uint16
Description | string | Specifies the format of the 'Data' output parameter
ValueMap | string | 2
Values | string | CSV
Duration | uint64
Description | string | Specifies the duration in seconds to generate statistical data. If only Duration is specified, then EndTime will be set to current time.
EndTime | datetime
Description | string | Specifies the end time up to which the statistical data will be generated. Current time will be assumed whenever EndTime is specified null. If only EndTime is specified, then StartTime will be set to the earliest time that data is available.
StartTime | datetime
Description | string | Specifies the start time for when the data is required. If only StartTime is specified, then EndTime shall be set to current time.
Data | REF CIM_VTLStatisticalData
Description | string | Graph Object
In | boolean | false
Out | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (null if synchronous call)
In | boolean | false
Out | boolean | true
Library | REF CIM_ComputerSystem
Description | string | Reference to a VTL or the VLS
Pool | REF CIM_StoragePool
Description | string | Reference to the storage pool, concrete or primordial

#### GetLogicalCapacityUsage (uint16)

#### Method Qualifiers (GetLogicalCapacityUsage)

Name | Data Type | Value
--- | --- | ---
Description | string | GetLogicalCapacityUsage Provides logical capacity usage for the entire VLS appliance or a specific VTL depending on the ComputerSystem reference passed in. At least one of StartTime, EndTime, and Duration must be specified. - If all three are specified, then Duration is ignored. - StartTime shall not be higher than EndTime. - No time may be set in the future. - If two of the three are specified, then the third is calculated. - If only StartTime or Duration is specified, then EndTime will be set to the current time. - If only EndTime is specified, then StartTime will be set to the time the earliest data is available.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096
Values | string | Job Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, Statistics Format Not Supported, Method Reserved, Method Parameters Checked - Job Started

#### Method Parameters (GetLogicalCapacityUsage)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
DataFormat | uint16
Description | string | Specifies the format of the 'Data' output parameter
ValueMap | string | 2
Values | string | CSV
Duration | uint64
Description | string | Specifies the duration in seconds to generate statistical data. If only Duration is specified, then EndTime will be set to current time.
EndTime | datetime
Description | string | Specifies the end time up to which the statistical data will be generated. Current time will be assumed whenever EndTime is specified null. If only EndTime is specified, then StartTime will be set to the earliest time that data is available.
StartTime | datetime
Description | string | Specifies the start time for when the data is required. If only StartTime is specified, then EndTime shall be set to current time.
Data | REF CIM_VTLStatisticalData
Description | string | Graph Object
In | boolean | false
Out | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (null if synchronous call)
In | boolean | false
Out | boolean | true
Library | REF CIM_ComputerSystem
Description | string | Reference to a VTL or the VLS

#### GetSystemRatio (uint16)

#### Method Qualifiers (GetSystemRatio)

Name | Data Type | Value
--- | --- | ---
Description | string | GetSystemRatio Provides an historic of the compression ratio for the entire VLS appliance or a specific VTL depending on on the ComputerSystem reference passed in. At least one of StartTime, EndTime, and Duration must be specified. - If all three are specified, then Duration is ignored. - StartTime shall not be higher than EndTime. - No time may be set in the future. - If two of the three are specified, then the third is calculated. - If only StartTime or Duration is specified, then EndTime will be set to the current time. - If only EndTime is specified, then StartTime will be set to the time the earliest data is available.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096
Values | string | Job Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, Statistics Format Not Supported, Method Reserved, Method Parameters Checked - Job Started

#### Method Parameters (GetSystemRatio)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
DataFormat | uint16
Description | string | Specifies the format of the 'Data' output parameter
ValueMap | string | 2
Values | string | CSV
Duration | uint64
Description | string | Specifies the duration in seconds to generate statistical data. If only Duration is specified, then EndTime will be set to current time.
EndTime | datetime
Description | string | Specifies the end time up to which the statistical data will be generated. Current time will be assumed whenever EndTime is specified null. If only EndTime is specified, then StartTime will be set to the earliest time that data is available.
StartTime | datetime
Description | string | Specifies the start time for when the data is required. If only StartTime is specified, then EndTime shall be set to current time.
Data | REF CIM_VTLStatisticalData
Description | string | Graph Object
In | boolean | false
Out | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (null if synchronous call)
In | boolean | false
Out | boolean | true
Library | REF CIM_ComputerSystem
Description | string | Reference to a VTL or the VLS

#### GetDeduplicationRatio (uint16)

#### Method Qualifiers (GetDeduplicationRatio)

Name | Data Type | Value
--- | --- | ---
Description | string | GetDeduplicationRatio(CIM_ComputerSystem REF): Provides an historicof the deduplication ratio for the entire VLS appliance or a specificVTL depending on on the ComputerSystem reference passed in. At least one of StartTime, EndTime, and Duration must be specified. - If all three are specified, then Duration is ignored. - StartTime shall not be higher than EndTime. - No time may be set in the future. - If two of the three are specified, then the third is calculated. - If only StartTime or Duration is specified, then EndTime will be set to the current time. - If only EndTime is specified, then StartTime will be set to the time the earliest data is available.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096
Values | string | Job Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, Statistics Format Not Supported, Method Reserved, Method Parameters Checked - Job Started

#### Method Parameters (GetDeduplicationRatio)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
DataFormat | uint16
Description | string | Specifies the format of the 'Data' output parameter
ValueMap | string | 2
Values | string | CSV
Duration | uint64
Description | string | Specifies the duration in seconds to generate statistical data. If only Duration is specified, then EndTime will be set to current time.
EndTime | datetime
Description | string | Specifies the end time up to which the statistical data will be generated. Current time will be assumed whenever EndTime is specified null. If only EndTime is specified, then StartTime will be set to the earliest time that data is available.
StartTime | datetime
Description | string | Specifies the start time for when the data is required. If only StartTime is specified, then EndTime shall be set to current time.
Data | REF CIM_VTLStatisticalData
Description | string | Graph Object
In | boolean | false
Out | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (null if synchronous call)
In | boolean | false
Out | boolean | true
Library | REF CIM_ComputerSystem
Description | string | Reference to a VTL or the VLS

#### GetReplicationThroughput (uint16)

#### Method Qualifiers (GetReplicationThroughput)

Name | Data Type | Value
--- | --- | ---
Description | string | GetReplicationThroughput provides a historic ofthe incoming or outgoing replication throughput in MB/s. At least one of StartTime, EndTime, and Duration must be specified. - If all three are specified, then Duration is ignored. - StartTime shall not be higher than EndTime. - No time may be set in the future. - If two of the three are specified, then the third is calculated. - If only StartTime or Duration is specified, then EndTime will be set to the current time. - If only EndTime is specified, then StartTime will be set to the time the earliest data is available.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096
Values | string | Job Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, Statistics Format Not Supported, Method Reserved, Method Parameters Checked - Job Started

#### Method Parameters (GetReplicationThroughput)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
DataDirection | uint16
Description | string | Indicates incoming or outgoing traffic
ValueMap | string | 0, 1, .., 32768..65535
Values | string | In Traffic, Out Traffic, DMTF Reserved, Vendor Specific
DataFormat | uint16
Description | string | Specifies the format of the 'Data' output parameter
ValueMap | string | 2
Values | string | CSV
Duration | uint64
Description | string | Specifies the duration in seconds to generate statistical data. If only Duration is specified, then EndTime will be set to current time.
EndTime | datetime
Description | string | Specifies the end time up to which the statistical data will be generated. Current time will be assumed whenever EndTime is specified null. If only EndTime is specified, then StartTime will be set to the earliest time that data is available.
StartTime | datetime
Description | string | Specifies the start time for when the data is required. If only StartTime is specified, then EndTime shall be set to current time.
Data | REF CIM_VTLStatisticalData
Description | string | Graph Object
In | boolean | false
Out | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (null if synchronous call)
In | boolean | false
Out | boolean | true
Library | REF CIM_ComputerSystem
Description | string | Reference to a VTL or the VLS

#### GetReplicationRatio (uint16)

#### Method Qualifiers (GetReplicationRatio)

Name | Data Type | Value
--- | --- | ---
Description | string | GetReplicationRatio provides a historic of the deduplication ratio over the replication link. At least one of StartTime, EndTime, and Duration must be specified. - If all three are specified, then Duration is ignored. - StartTime shall not be higher than EndTime. - No time may be set in the future. - If two of the three are specified, then the third is calculated. - If only StartTime or Duration is specified, then EndTime will be set to the current time. - If only EndTime is specified, then StartTime will be set to the time the earliest data is available.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096
Values | string | Job Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, Statistics Format Not Supported, Method Reserved, Method Parameters Checked - Job Started

#### Method Parameters (GetReplicationRatio)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
DataFormat | uint16
Description | string | Specifies the format of the 'Data' output parameter
ValueMap | string | 2
Values | string | CSV
Duration | uint64
Description | string | Specifies the duration in seconds to generate statistical data. If only Duration is specified, then EndTime will be set to current time.
EndTime | datetime
Description | string | Specifies the end time up to which the statistical data will be generated. Current time will be assumed whenever EndTime is specified null. If only EndTime is specified, then StartTime will be set to the earliest time that data is available.
StartTime | datetime
Description | string | Specifies the start time for when the data is required. If only StartTime is specified, then EndTime shall be set to current time.
Data | REF CIM_VTLStatisticalData
Description | string | Graph Object
In | boolean | false
Out | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (null if synchronous call)
In | boolean | false
Out | boolean | true
Library | REF CIM_ComputerSystem
Description | string | Reference to a VTL or the VLS

#### GetPerformanceStatisticsReadWriteIO (uint16)

#### Method Qualifiers (GetPerformanceStatisticsReadWriteIO)

Name | Data Type | Value
--- | --- | ---
Description | string | GetPerformanceStatisticsReadWriteIO gives the front-end port performance. At least one of StartTime, EndTime, and Duration must be specified. - If all three are specified, then Duration is ignored. - StartTime shall not be higher than EndTime. - No time may be set in the future. - If two of the three are specified, then the third is calculated. - If only StartTime or Duration is specified, then EndTime will be set to the current time. - If only EndTime is specified, then StartTime will be set to the time the earliest data is available.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096
Values | string | Job Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, Statistics Format Not Supported, Method Reserved, Method Parameters Checked - Job Started

#### Method Parameters (GetPerformanceStatisticsReadWriteIO)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
DataFormat | uint16
Description | string | Specifies the format of the 'Data' output parameter
ValueMap | string | 2
Values | string | CSV
Duration | uint64
Description | string | Specifies the duration in seconds to generate statistical data. If only Duration is specified, then EndTime will be set to current time.
EndTime | datetime
Description | string | Specifies the end time up to which the statistical data will be generated. Current time will be assumed whenever EndTime is specified null. If only EndTime is specified, then StartTime will be set to the earliest time that data is available.
StartTime | datetime
Description | string | Specifies the start time for when the data is required. If only StartTime is specified, then EndTime shall be set to current time.
Data | REF CIM_VTLStatisticalData
Description | string | Graph Object
In | boolean | false
Out | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (null if synchronous call)
In | boolean | false
Out | boolean | true
Library | REF CIM_ComputerSystem
Description | string | Reference to a VTL or the VLS
tapeDrive | REF CIM_TapeDrive
Description | string | Reference to the Tape Drive for which the performance data is requested,if null performance stastics for the Virtual Library will be returned

#### GetFCPortStatisticsSRR (uint16)

#### Method Qualifiers (GetFCPortStatisticsSRR)

Name | Data Type | Value
--- | --- | ---
Description | string | GetFCPortStatisticsSRR provides the Sequence RetransmissionRequest performance statistics of a FC Port in a VLS. At least one of StartTime, EndTime, and Duration must be specified. - If all three are specified, then Duration is ignored. - StartTime shall not be higher than EndTime. - No time may be set in the future. - If two of the three are specified, then the third is calculated. - If only StartTime or Duration is specified, then EndTime will be set to the current time. - If only EndTime is specified, then StartTime will be set to the time the earliest data is available.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096
Values | string | Job Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, Statistics Format Not Supported, Method Reserved, Method Parameters Checked - Job Started

#### Method Parameters (GetFCPortStatisticsSRR)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
DataFormat | uint16
Description | string | Specifies the format of the 'Data' output parameter
ValueMap | string | 2
Values | string | CSV
Duration | uint64
Description | string | Specifies the duration in seconds to generate statistical data. If only Duration is specified, then EndTime will be set to current time.
EndTime | datetime
Description | string | Specifies the end time up to which the statistical data will be generated. Current time will be assumed whenever EndTime is specified null. If only EndTime is specified, then StartTime will be set to the earliest time that data is available.
StartTime | datetime
Description | string | Specifies the start time for when the data is required. If only StartTime is specified, then EndTime shall be set to current time.
Data | REF CIM_VTLStatisticalData
Description | string | Graph Object
In | boolean | false
Out | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (null if synchronous call)
In | boolean | false
Out | boolean | true
port | REF CIM_LogicalPort
Description | string | Port for which the Aborts metric is requested

#### GetFCPortStatisticsAborts (uint16)

#### Method Qualifiers (GetFCPortStatisticsAborts)

Name | Data Type | Value
--- | --- | ---
Description | string | GetFCPortStatisticsAborts provides the abort statistics of a FC Port in a VLS. At least one of StartTime, EndTime, and Duration must be specified. - If all three are specified, then Duration is ignored. - StartTime shall not be higher than EndTime. - No time may be set in the future. - If two of the three are specified, then the third is calculated. - If only StartTime or Duration is specified, then EndTime will be set to the current time. - If only EndTime is specified, then StartTime will be set to the time the earliest data is available.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096
Values | string | Job Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, Statistics Format Not Supported, Method Reserved, Method Parameters Checked - Job Started

#### Method Parameters (GetFCPortStatisticsAborts)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
DataFormat | uint16
Description | string | Specifies the format of the 'Data' output parameter
ValueMap | string | 2
Values | string | CSV
Duration | uint64
Description | string | Specifies the duration in seconds to generate statistical data. If only Duration is specified, then EndTime will be set to current time.
EndTime | datetime
Description | string | Specifies the end time up to which the statistical data will be generated. Current time will be assumed whenever EndTime is specified null. If only EndTime is specified, then StartTime will be set to the earliest time that data is available.
StartTime | datetime
Description | string | Specifies the start time for when the data is required. If only StartTime is specified, then EndTime shall be set to current time.
Data | REF CIM_VTLStatisticalData
Description | string | Graph Object
In | boolean | false
Out | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (null if synchronous call)
In | boolean | false
Out | boolean | true
port | REF CIM_LogicalPort
Description | string | Port for which the Aborts metric is requested

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
RequestStateChange | uint32 | CIM_EnabledLogicalElement
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service