# Class CIM_VTOCDiskPartition
extends CIM_GenericDiskPartition

VTOC is a partitioning scheme used on Solaris and some other OSes based on BSD Unix. VTOC partitions are also known as slices. VTOC allows partitions to overlap. A VTOC disk always contains 8 slices, but not all need to be in use.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_StorageExtent
|
+--CIM_MediaPartition
|
+--CIM_GenericDiskPartition
|
+--CIM_VTOCDiskPartition

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | VTOC is a partitioning scheme used on Solaris and some other OSes based on BSD Unix. VTOC partitions are also known as slices. VTOC allows partitions to overlap. A VTOC disk always contains 8 slices, but not all need to be in use.
UMLPackagePath | string | CIM::Device::StorageExtents
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AsciiLabel | string |
Description | string | A string value generated by the format utility based on the disk vendor and product IDs and the capacity.
Tag | uint16 |
Description | string | The VTOC tag. This is selected by the user to provide a about the content of the partition. These are the names and values already used in the VTOC definitions.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10
Values | string | Unassigned, Boot, Root, Swap, USR, Backup, Stand, Var, Home, Alternate Sector, CacheFS
Flags | uint16[] |
Description | string | The VTOC partition flags.
ValueMap | string | 1, 10
Values | string | Unmountable, Read Only

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Access | uint16 | CIM_StorageExtent
Allocatable | boolean | CIM_MediaPartition
AllocationState | string | CIM_LogicalDevice
Availability | uint16 | CIM_LogicalDevice
BlockSize | uint64 | CIM_StorageExtent
Bootable | boolean | CIM_MediaPartition
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CompressionRate | uint16 | CIM_StorageExtent
CompressionState | uint16 | CIM_StorageExtent
ConsumableBlocks | uint64 | CIM_StorageExtent
CreationClassName | string | CIM_LogicalDevice
DataOrganization | uint16 | CIM_StorageExtent
DataRedundancy | uint16 | CIM_StorageExtent
DeltaReservation | uint8 | CIM_StorageExtent
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
ErrorMethodology | string | CIM_StorageExtent
Extendable | boolean | CIM_MediaPartition
ExtentInterleaveDepth | uint64 | CIM_StorageExtent
ExtentStripeLength | uint64 | CIM_StorageExtent
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsBasedOnUnderlyingRedundancy | boolean | CIM_StorageExtent
IsComposite | boolean | CIM_StorageExtent
IsCompressed | boolean | CIM_StorageExtent
IsConcatenated | boolean | CIM_StorageExtent
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_StorageExtent
NameFormat | uint16 | CIM_StorageExtent
NameNamespace | uint16 | CIM_StorageExtent
NoSinglePointOfFailure | boolean | CIM_StorageExtent
NumberOfBlocks | uint64 | CIM_StorageExtent
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherNameFormat | string | CIM_StorageExtent
OtherNameNamespace | string | CIM_StorageExtent
OtherUsageDescription | string | CIM_StorageExtent
PackageRedundancy | uint16 | CIM_StorageExtent
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
Primordial | boolean | CIM_StorageExtent
Purpose | string | CIM_StorageExtent
RequestedState | uint16 | CIM_EnabledLogicalElement
SequentialAccess | boolean | CIM_StorageExtent
Signature | string | CIM_MediaPartition
SignatureAlgorithm | string | CIM_MediaPartition
SignatureState | string | CIM_MediaPartition
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
Usage | uint16 | CIM_StorageExtent
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
ClientSettableUsage | uint16[] | CIM_StorageExtent
ExtentDiscriminator | string[] | CIM_StorageExtent
ExtentStatus | uint16[] | CIM_StorageExtent
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice