# Class CIM_FCPortStatistics
extends CIM_NetworkPortStatistics

FCPortStatistics is the statistics for the FCPort.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalData
|
+--CIM_NetworkPortStatistics
|
+--CIM_FCPortStatistics

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | FCPortStatistics is the statistics for the FCPort.
UMLPackagePath | string | CIM::Device::FC
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AddressErrors | uint64 |
Counter | boolean | true
Description | string | Count of frames received with unknown addressing. An example is an unknown SID or DID. The SID or DID is not known to the routing algorithm.
BufferCreditNotProvided | uint64 |
Counter | boolean | true
Description | string | Count of occurrences when all input buffers of a port were full and outbound buffer-to-buffer credit was transitioned to zero. There is no credit to provide to the other side.
BufferCreditNotReceived | uint64 |
Counter | boolean | true
Description | string | Count of transitions in or out of BBcredit zero state. The other side is not providing any credit.
Class1FBSY | uint64 |
Counter | boolean | true
Description | string | Class1FBSY is the number of times that FBSY was returned to the port.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C1FB
Class1FRJT | uint64 |
Counter | boolean | true
Description | string | Class1FRJT is the number of times that FRJT was returned to the port.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C1FR
Class1PBSY | uint64 |
Counter | boolean | true
Description | string | Class1PBSY is the number of times that PBSY was returned to the port.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C1PB
Class1PRJT | uint64 |
Counter | boolean | true
Description | string | Class1PRJT is the number of times that PRJT was returned to the port.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C1PR
Class2FBSY | uint64 |
Counter | boolean | true
Description | string | Class2FBSY is the number of times that FBSY was returned to the port.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C2FB
Class2FRJT | uint64 |
Counter | boolean | true
Description | string | Class2FRJT is the number of times that FRJT was returned to the port.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C2FR
Class2PBSY | uint64 |
Counter | boolean | true
Description | string | Class2PBSY is the number of times that PBSY was returned to the port.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C2PB
Class2PRJT | uint64 |
Counter | boolean | true
Description | string | Class2PRJT is the number of times that PRJT was returned to the port.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C2PR
Class3FramesDiscarded | uint64 |
Counter | boolean | true
Description | string | Class3FramesDiscarded is the number of class 3 frames that were discarded upon reception.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C3DC
CRCErrors | uint64 |
Counter | boolean | true
Description | string | Number of times that the CRC in a frame does not match the CRC that is computed by the receiver. This count is part of the Link Error Status Block (LESB).
DelimiterErrors | uint64 |
Counter | boolean | true
Description | string | Count of invalid frame delimiters that are received at this port. An example is a frame with a class 2 start and a class 3 at the end.
DumpedFrames | uint64 |
Counter | boolean | true
Description | string | DumpedFrames is the number of frames that were lost due to a lack of host buffers available.
EncodingDisparityErrors | uint64 |
Counter | boolean | true
Description | string | Count of disparity errors that are received at this port.
ErrorFrames | uint64 |
Counter | boolean | true
Description | string | ErrorFrames is the number of frames that have been received in error.
FBSYFrames | uint64 |
Counter | boolean | true
Description | string | FBSYFrames is the number of times that FBSY was returned to the port.
MappingStrings | string | FC-SWAPI.T11|ErrorCounters|1.SWAPI_STATS_LBL_FBSY
FramesTooLong | uint64 |
Counter | boolean | true
Description | string | The number of frames received that were longer than 2140 octets. The value of 2140 is calculated based on an assumption of 24 header bytes plus 4 CRC bytes and 2112 bytes of payload.
FramesTooShort | uint64 |
Counter | boolean | true
Description | string | The number of frames received that were shorter than 28 octets. The value of 28 is calculated based on an assumption of 24 header bytes plus 4 CRC bytes. The count does not include SOF/EOF bytes, which are not data.
FRJTFrames | uint64 |
Counter | boolean | true
Description | string | FRJTFrames is the number of times that FRJT was returned to the port.
MappingStrings | string | FC-SWAPI.T11|ErrorCounters|1.SWAPI_STATS_LBL_FRJT
InvalidTransmissionWords | uint64 |
Counter | boolean | true
Description | string | The number of transmission words that had an invalid character (8b10b code violation) in one or more of its characters, had a K28.5 (8b10b control) in its second, third, or fourth character position, or had an incorrect Beginning Running Disparity. This count is part of the Link Error Status Block (LESB).
LinkFailures | uint64 |
Counter | boolean | true
Description | string | LinkFailure is the number of times that a link error has occurred. This count is part of the Link Error Status Block (LESB).
LinkResetsReceived | uint64 |
Counter | boolean | true
Description | string | Count of Link resets. This count is the number of LRs received.
LinkResetsTransmitted | uint64 |
Counter | boolean | true
Description | string | Count of Link resets. This count is the number of LRs transmitted.
LIPCount | uint64 |
Counter | boolean | true
Description | string | LIPCount is the number of LIP events that have occurred on an arbitrated loop.
LossOfSignalCounter | uint64 |
Counter | boolean | true
Description | string | Number of times the signal is lost on the Port since the last reset of the Device. This count is part of the Link Error Status Block (LESB).
LossOfSyncCounter | uint64 |
Counter | boolean | true
Description | string | Number of times that synchronization is lost on the Port since the last reset of the Device. Synchronization is assumed lost after a timeout period (identified by the Receiver TransmitterTimeout property) is exceeded. This count is part of the Link Error Status Block (LESB).
MulticastFramesReceived | uint64 |
Counter | boolean | true
Description | string | Count of Multicast Frames or Packets received.
MulticastFramesTransmitted | uint64 |
Counter | boolean | true
Description | string | Count of Multicast Frames or Packets transmitted.
NOSCount | uint64 |
Counter | boolean | true
Description | string | NOSCount is the number of NOS events that have occurred on the switched fabric.
PBSYFrames | uint64 |
Counter | boolean | true
Description | string | PBSYFrames is the number of times that PBSY was returned to the port.
MappingStrings | string | FC-SWAPI.T11|ErrorCounters|1.SWAPI_STATS_LBL_PBSY
PrimitiveSeqProtocolErrCount | uint64 |
Counter | boolean | true
Description | string | Count of primitive sequence protocol errors that are detected at this port. This count is part of the Link Error Status Block (LESB).
PRJTFrames | uint64 |
Counter | boolean | true
Description | string | PRJTFrames is the number of times that PRJT was returned to the port.
MappingStrings | string | FC-SWAPI.T11|ErrorCounters|1.SWAPI_STATS_LBL_PRJT
RXBroadcastFrames | uint64 |
Counter | boolean | true
Description | string | RXBroadcastFrames is the number of broadcast frames or packets received.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_RBCO
RXClass1Frames | uint64 |
Counter | boolean | true
Description | string | RXClass1Frames is the number of class 1 frames received.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C1RF
RXClass2Frames | uint64 |
Counter | boolean | true
Description | string | RXClass2Frames is the number of class 2 frames received.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C2RF
RXClass3Frames | uint64 |
Counter | boolean | true
Description | string | RXClass3Frames is the number of class 3 frames received.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C3RF
TXBroadcastFrames | uint64 |
Counter | boolean | true
Description | string | TXBroadcastFrames is the number of broadcast frames or packets transmitted.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_TBCO
TXClass1Frames | uint64 |
Counter | boolean | true
Description | string | TXClass1Frames is the number of class 1 frames transmitted.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C1TF
TXClass2Frames | uint64 |
Counter | boolean | true
Description | string | TXClass2Frames is the number of class 2 frames transmitted.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C2LF
TXClass3Frames | uint64 |
Counter | boolean | true
Description | string | TXClass3Frames is the number of class 3 frames transmitted.
MappingStrings | string | FC-SWAPI.T11|PerformanceCounters|1.SWAPI_STATS_LBL_C3TF

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
BytesReceived | uint64 | CIM_NetworkPortStatistics
BytesTransmitted | uint64 | CIM_NetworkPortStatistics
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_StatisticalData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_StatisticalData
PacketsReceived | uint64 | CIM_NetworkPortStatistics
PacketsTransmitted | uint64 | CIM_NetworkPortStatistics
RateIntervalEndTime | datetime | CIM_StatisticalData
RateIntervalStartTime | datetime | CIM_StatisticalData
SampleInterval | datetime | CIM_StatisticalData
StartStatisticTime | datetime | CIM_StatisticalData
StatisticTime | datetime | CIM_StatisticalData

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ResetSelectedStats | uint32 | CIM_StatisticalData