# Class CIM_AverageRateMeterService
extends CIM_MeterService

This is a concrete subclass of MeterService that represents a simple meter, called an Average Rate Meter. This type of meter measures the average rate at which packets are submitted to it over a specified time. Packets are defined as conformant if their average arrival rate does not exceed the specified measuring rate of the meter. Any packet that causes the specified measuring rate to be exceeded is defined to be non-conforming.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_ConditioningService
|
+--CIM_MeterService
|
+--CIM_AverageRateMeterService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This is a concrete subclass of MeterService that represents a simple meter, called an Average Rate Meter. This type of meter measures the average rate at which packets are submitted to it over a specified time. Packets are defined as conformant if their average arrival rate does not exceed the specified measuring rate of the meter. Any packet that causes the specified measuring rate to be exceeded is defined to be non-conforming.
UMLPackagePath | string | CIM::Network::QoS
Version | string | 2.7.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AverageRate | uint32 |
Description | string | This property is a 32-bit unsigned integer that defines the rate used to determine whether admitted packets are in conformance or not. The value is specified in kilobits per second.
Units | string | KiloBits per Second
DeltaInterval | uint64 |
Description | string | This property is a 64-bit unsigned integer that defines the time period over which the average measurement should be taken. The value is specified in microseconds.
Units | string | MicroSeconds

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
ConformanceLevels | uint16 | CIM_MeterService
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
Enabled | boolean | CIM_ConditioningService
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LoSID | string | CIM_Service
LoSOrgID | string | CIM_Service
MeterType | uint16 | CIM_MeterService
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherMeterType | string | CIM_MeterService
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
RequestStateChange | uint32 | CIM_EnabledLogicalElement
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service