# Class CIM_SCSIArbitraryLogicalUnit
extends CIM_LogicalDevice

SCSIArbitraryLogicalUnit represents an element that is addressed as a device, but is not accurately modeled by some other LogicalDevice subclass (such as TapeDrive or StorageVolume). One common use is 'control devices' that provide management rather than I/O functionality. For example, SCSI defines this behavior for Enclosure Services and SCSI Controller devices.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_SCSIArbitraryLogicalUnit

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | SCSIArbitraryLogicalUnit represents an element that is addressed as a device, but is not accurately modeled by some other LogicalDevice subclass (such as TapeDrive or StorageVolume). One common use is 'control devices' that provide management rather than I/O functionality. For example, SCSI defines this behavior for Enclosure Services and SCSI Controller devices.
UMLPackagePath | string | CIM::Device::DeviceElements
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
DeviceType | uint16 |
Description | string | The type of the device. For SCSI devices, this property is related to the peripheral device type that is returned in bits 0 to 4 of byte 0 of the inquiry response. Note that 'Direct Access' is included to model the common behavior of using a zero-length volume for in-band management of RAID arrays.
MappingStrings | string | ANSI|T10|SCSI SPC|Peripheral Device Type
ModelCorrespondence | string | CIM_SCSIArbitraryLogicalUnit.OtherDeviceType
Required | boolean | true
ValueMap | string | 0, 1, 2, 3, 4, 5, 6
Values | string | Unknown, Other, Direct Access, SCSI SCC Device, SCSI SES, SCSI ADI, SCSI Well Known Logical Unit
OtherDeviceType | string |
Description | string | A string that describes the device type if DeviceType is set to 1 ("Other").
ModelCorrespondence | string | CIM_SCSIArbitraryLogicalUnit.DeviceType

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AllocationState | string | CIM_LogicalDevice
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice