# Class CIM_SourceRoutingService
extends CIM_ForwardingService

SourceRoutingService represents the capability of a switch to participate in the source routing of frames received at its ports. It is a system-level Service that provides and supports local switching only. The SourceRouting Service is aggregated into a higher level SwitchService through the SwitchServiceSourceRouting association.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_NetworkService
|
+--CIM_ForwardingService
|
+--CIM_SourceRoutingService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | SourceRoutingService represents the capability of a switch to participate in the source routing of frames received at its ports. It is a system-level Service that provides and supports local switching only. The SourceRouting Service is aggregated into a higher level SwitchService through the SwitchServiceSourceRouting association.
UMLPackagePath | string | CIM::Network::SwitchingBridging
Version | string | 2.7.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
BridgeLfMode | uint16 |
Description | string | Indicates whether the bridge operates using older 3 bit length negotiation fields or the newer 6 bit length field in its RIF.
MappingStrings | string | MIB.IETF|SOURCE-ROUTING-MIB.dot1dSrBridgeLfMode
ValueMap | string | 1, 2
Values | string | Mode3, Mode6

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LoSID | string | CIM_Service
LoSOrgID | string | CIM_Service
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherProtocolType | string | CIM_ForwardingService
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolType | uint16 | CIM_ForwardingService
RequestedState | uint16 | CIM_EnabledLogicalElement
ServiceURL | string | CIM_NetworkService
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
Keywords | string[] | CIM_NetworkService
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StartupConditions | string[] | CIM_NetworkService
StartupParameters | string[] | CIM_NetworkService
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
RequestStateChange | uint32 | CIM_EnabledLogicalElement
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service