# Class CIM_DiscreteSensor
extends CIM_Sensor

A DiscreteSensor has a set of legal string values, that it can report. These values are enumerated in the Sensor's PossibleValues property. A DiscreteSensor will always have a 'current reading' that corresponds to one of the enumerated values. The use of this class is being deprecated in lieu of CIM_Sensor. Information in the CurrentReading and PossibleValues properties will typically have the same values and semantics as for the CurrentState and PossibleStates properties, inherited from Sensor.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Sensor
|
+--CIM_DiscreteSensor

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_Sensor
Description | string | A DiscreteSensor has a set of legal string values, that it can report. These values are enumerated in the Sensor's PossibleValues property. A DiscreteSensor will always have a 'current reading' that corresponds to one of the enumerated values. The use of this class is being deprecated in lieu of CIM_Sensor. Information in the CurrentReading and PossibleValues properties will typically have the same values and semantics as for the CurrentState and PossibleStates properties, inherited from Sensor.
UMLPackagePath | string | CIM::Device::Sensors
Version | string | 2.8.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CurrentReading | string |
Deprecated | string | CIM_Sensor.CurrentState
Description | string | The current value indicated by the Sensor.
MaxLen | uint32 | 64
AcceptableValues | string[] |
Deprecated | string | No value
Description | string | AcceptableValues details which of the PossibleValues strings are considered 'acceptable' (ie, 'not an error').
MaxLen | uint32 | 64
PossibleValues | string[] |
Deprecated | string | CIM_Sensor.PossibleStates
Description | string | PossibleValues enumerates the string outputs that can be reported by the DiscreteSensor.
MaxLen | uint32 | 64

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AllocationState | string | CIM_LogicalDevice
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
CurrentState | string | CIM_Sensor
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherSensorTypeDescription | string | CIM_Sensor
PollingInterval | uint64 | CIM_Sensor
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
SensorContext | string | CIM_Sensor
SensorType | uint16 | CIM_Sensor
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PossibleStates | string[] | CIM_Sensor
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice