# Class CIM_DiskDriveDiagnosticTest
extends CIM_DiagnosticTest

This class specializes CIM_DiagnosticTest to define the tests specific to disk drives.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_DiagnosticService
|
+--CIM_DiagnosticTest
|
+--CIM_DiskDriveDiagnosticTest

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class specializes CIM_DiagnosticTest to define the tests specific to disk drives.
UMLPackagePath | string | CIM::System::Diagnostics
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
DiskDriveTestType | uint16 |
Description | string | The descriptions for each Disk Drive test type are below: * "Short Self-Test" (value=2) is specified for the test that performs a small set of vendor-specific tests to verify that the disk is operating properly. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Media Verify (value=6). * "Extended Self-Test" (value=3) is specified for the tests that performs an extended set of vendor-specific tests to verify that the disk is operating properly. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Media Verify (value=6). * "Selective Self-Test" (value=4) is specified for the test that performs an extended set of vendor-specific tests to verify that the disk is operating properly, but limited to a specific LBA range of the disk. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Media Verify (value=6). * "Sequential Read" (value=5) is specified for the test that performs a read operation from all disk sectors in sequential order. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Media Verify (value=6). * "Random Read" (value=6) is specified for the test that performs a read operation from disk sectors in random order. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Media Verify (value=6). * "Sequential Read-Write-Read Compare" (value=7) is specified for the test that verifies that read and write operations are performed properly for a selected LBA range. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Media Verify (value=6). * "Random Read-Write-Read Compare" (value=8) is specified for the test that verifies that read and write operations are performed properly for a selected LBA range. Disk sectors are tested in random order. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Media Verify (value=6). * "Sequential Internal Verify" (value=9) is specified for the test that verifies the ability to perform read and verify operations from track to track and head to head in sequential order for a selected LBA range. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Media Verify (value=6). * "Status" (value=10) is specified for the test that returns information that relative health of the disk drive based upon internal analysis of failure statistics. CIM_DiagnosticTest.TestTypes shall be set to Health Check (value=4). * "Grown Defects" (value=11) is specified for the test that retrieves statistics (such as the number of remapped sectors) collected by the disk drive regarding its sector remap mechanism. CIM_DiagnosticTest.TestTypes shall be set to Stress (value=4). * "4K Alignment" (value=12) is specified for the test that verifies that blocks can be properly aligned on 4K boundaries. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Power Management" (value=13) is specified for the test that verify that all system interface for cables and connectors are working properly. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Performance" (value=14) is specified for the test that verifies that the disk operates within the vendor/product specific performance ranges for data read operation transfer rates, sequential seek times and random seek times. * "Conveyance" (value=15) is specified for testing for damage in transit. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2) and Stress (value=6).
ModelCorrespondence | string | CIM_DiskDriveDiagnosticTest.OtherDiskDriveTestType
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, .., 0x8000..
Values | string | Unknown, Other, Short Self-Test, Extended Self-Test, Selective Self-Test, Sequential Read, Random Read, Sequential Read-Write-Read Compare, Random Read-Write-Read Compare, Sequential Internal Verify, Status, Grown Defects, 4K Alignment, Power Management, Performance, Conveyance, Vendor Reserved, DMTF Reserved
OtherDiskDriveTestType | string |
Description | string | A string that describes the test when the DiskDriveTestType property is set to 1 ("Other"). This property must be set to null when DiskDriveTestType is any value other than 1.
ModelCorrespondence | string | CIM_DiskDriveDiagnosticTest.DiskDriveTestType

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsInUse | boolean | CIM_DiagnosticTest
LoSID | string | CIM_Service
LoSOrgID | string | CIM_Service
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherCharacteristicDescription | string | CIM_DiagnosticTest
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
Characteristics | uint16[] | CIM_DiagnosticTest
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherCharacteristicsDescriptions | string[] | CIM_DiagnosticTest
OtherTestTypesDescriptions | string[] | CIM_DiagnosticTest
ResourcesUsed | uint16[] | CIM_DiagnosticTest
StatusDescriptions | string[] | CIM_ManagedSystemElement
TestTypes | uint16[] | CIM_DiagnosticTest

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
ClearResults | uint32 | CIM_DiagnosticTest
DiscontinueTest | uint32 | CIM_DiagnosticTest
RequestStateChange | uint32 | CIM_EnabledLogicalElement
RunDiagnostic | uint32 | CIM_DiagnosticService
RunDiagnosticService | uint32 | CIM_DiagnosticService
RunTest | uint32 | CIM_DiagnosticTest
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service