# Class CIM_Unimodem
extends CIM_POTSModem

Unimodem is a POTSModem that supports the Unimodem 1.0 Specification.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Modem
|
+--CIM_CallBasedModem
|
+--CIM_POTSModem
|
+--CIM_Unimodem

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Unimodem is a POTSModem that supports the Unimodem 1.0 Specification.
UMLPackagePath | string | CIM::Device::Modems
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CallSetupResultCode | uint16 |
Description | string | Current call setup result code.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11
Values | string | No Previous Call, No Dial Tone Detected, Reorder Signal Detected, Network Busy, Busy Signal Detected, No Recognized Signal Detected, Voice Detected, Text Telephone Detected, Data Answering Signal Detected, Data Calling Signal Detected, Fax Answering Signal Detected, Fax Calling Signal Detected, V.8bis Signal Detected
CallWaitingEventCount | uint8 |
Counter | boolean | true
Description | string | Number of Call waiting events detected for the last or current call.
CarrierRenegotiationEventCount | uint8 |
Counter | boolean | true
Description | string | Carrier Rate renegotiation event count for the last or current call.
CarrierRetrainsGranted | uint8 |
Counter | boolean | true
Description | string | The number of carrier retrains granted during the current or last call.
CarrierRetrainsRequested | uint8 |
Counter | boolean | true
Description | string | The number of carrier retrains requested during the current or last call.
DTEDCEInterfaceMode | uint16 |
Description | string | Current DTE-DCE interface mode of the Unimodem, such as asynchronous, V.80 transparent, or framed synchronous modes.
ValueMap | string | 0, 1, 2
Values | string | Async Data, V.80 Transparent Synchronous Mode, V.80 Framed Synchronous Mode
ErrorControlFrameSize | uint16 |
Description | string | Error Control frame size in bytes for the last or current call.
PUnit | string | byte
Units | string | Bytes
ErrorControlLinkNAKs | uint8 |
Counter | boolean | true
Description | string | Error control link NAKs received for the last or current call.
ErrorControlLinkTimeouts | uint8 |
Counter | boolean | true
Description | string | Error control link timeouts in transmission for the last or current call.
EstimatedNoiseLevel | uint32 |
Description | string | Estimated noise level for the last or current call in -dBm. Values are in the range of 0-100.
Gauge | boolean | true
PUnit | string | decibel(m) * -1
Units | string | -dBm
FinalReceiveCarrierDataRate | uint32 |
Description | string | Final receive carrier data rate of the current or last call, in bits per second.
PUnit | string | bit / second
Units | string | Bits per Second
FinalTransmitCarrierDataRate | uint32 |
Description | string | Final transmit carrier data rate of the current or last call, in bits per second.
PUnit | string | bit / second
Units | string | Bits per Second
InitialReceiveCarrierDataRate | uint32 |
Description | string | Initial receive carrier data rate for the current or last call, in bits per second.
PUnit | string | bit / second
Units | string | Bits per Second
InitialTransmitCarrierDataRate | uint32 |
Description | string | Initial transmit carrier data rate for the current or last call, in bits per second.
PUnit | string | bit / second
Units | string | Bits per Second
MultiMediaMode | uint16 |
Description | string | Current multimedia mode of the Unimodem.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10
Values | string | Data Only, Fax Only, Voice Only, Voice View, ASVD V.61, ASVD V.34Q, DSVD Multi-Tech, DSVD 1.2, DSVD V.70, Video Telephony H.324, Other V.80 Call
NormalizedMeanSquaredError | uint32 |
Description | string | Normalized mean squared error for the last or current call.
ReceiveCarrierNegotiation | uint16 |
Description | string | The active receive modulation scheme.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23..65535
Values | string | V.17 (G3 Fax Call), V.21, V.22, V.22bis, V.23 Constant Carrier (1200/75), V.23 Switched Carrier (Half Duplex), V.26bis, V.26ter, V.27ter (G3 Fax Call), V.29 HD (G3 Fax Call), V.32, V.32bis, V.34, V.34 HD (G3 Fax Call), V.90 Issue 1 (Asymmetric), V.90 Issue 2 (Symmetric), Reserved (V.58), X2, K56FLEX, V.FC, V.32terbo, Bell 212A, Bell 103, Reserved for Mfgs
ReceiveCharsLost | uint64 |
Counter | boolean | true
Description | string | Number of receive characters lost for the last or current call. A DCE might limit this counter to 16 bits, but additional bits can be provided and are accounted for in this property.
ReceiveCharsSentToDTE | uint64 |
Counter | boolean | true
Description | string | Number of receive chars sent to the DTE for the last or current call. A continuous connection might exceed this value, given enough time. Typically these counters are implemented as 32-bit counters, but additional bits can be provided and are accounted for in this property. If these counters hit maximum value, the DCE manufacturer might roll over to 0.
ReceivedIFrameErrorCount | uint64 |
Counter | boolean | true
Description | string | Number of I-Frame errors detected for the last or current call, if error control protocol is running. A DCE might limit this counter to 16 bits, but additional bits can be provided and are accounted for in this property.
ReceiveFlowControl | uint16 |
Description | string | The flow control mechanism used in receiving data.
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Off, DC1/DC3, V.24 ckt 106/133
ReceiveIFrameCount | uint64 |
Counter | boolean | true
Description | string | Number of I-Frames received for the last or current call. A continuous connection might exceed this value, given enough time. Typically these counters are implemented as 32-bit counters, but additional bits can be provided and are accounted for in this property. If these counters hit maximum value, the DCE manufacturer might roll over to 0.
TemporaryCarrierLossEventCount | uint8 |
Counter | boolean | true
Description | string | Temporary carrier loss event count for the last or current call.
TerminationCause | uint16 |
Description | string | Cause of last call termination.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 49, 50
Values | string | Cause Unidentified, No Previous Call, Call Is Still in Progress, Call Waiting Signal Detected, Delayed, NMS Initiated Dial Call, NMS Initiated Leased Line Restoral, NMS Initiated Redial, NMS Initiated Dial Disconnect, Power Loss, Equipment Failure, Front Panel Disconnect Requested, Front Panel Leased Line Restoral, Automatic Leased Line Restoral, Inactivity Timer Expired, cct116 Restoral Request, cct108 Is Off Inhibits Dial, cct108 Turned Off, No Number Provided, Blacklisted Number, Call Attempts Limit Exceeded, Extension Phone Off Hook, Call Setup Fail Timer Expired, Incoming Call Detected, Loop Current Interrupted, No Dial Tone, Voice Detected, Reorder Tone, Sit Tone, Engaged Tone, Long Space Disconnect, Carrier Lost, Training Failed, No Modulation in Common, Retrain Failed, Retrain Attempt Count Exceeded, GSTN Cleardown Received, Fax Detected, In Test Mode, Intrusive Self Test Initiated, Any Key Abort, DTE Hangup Command, DTE Reset Command, Frame Reject, No Error Control Established, Protocol Violation, n400 Exceeded, Negotiation Failed, Disconnect Frame Received, Sabme Frame Received, Loss Of Synchronization
TransmitCarrierNegotiation | uint16 |
Description | string | The active transmit modulation scheme.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23..65535
Values | string | V.17 (G3 Fax Call), V.21, V.22, V.22bis, V.23 Constant Carrier (1200/75), V.23 Switched Carrier (Half Duplex), V.26bis, V.26ter, V.27ter (G3 Fax Call), V.29 HD (G3 Fax Call), V.32, V.32bis, V.34, V.34 HD (G3 Fax Call), V.90 Issue 1 (Asymmetric), V.90 Issue 2 (Symmetric), Reserved (V.58), X2, K56FLEX, V.FC, V.32terbo, Bell 212A, Bell 103, Reserved for Mfgs
TransmitCharsLost | uint64 |
Counter | boolean | true
Description | string | Number of transmit characters lost for the last or current call. A DCE might limit this counter to 16 bits, but additional bits can be provided and are accounted for in this property.
TransmitCharsSentFromDTE | uint64 |
Counter | boolean | true
Description | string | Number of transmit chars sent from the DTE for the last or current call. A continuous connection might exceed this value, given enough time. Typically these counters are implemented as 32-bit counters, but additional bits can be provided and are accounted for in this property. If these counters hit maximum value, the DCE manufacturer might roll over to 0.
TransmitFlowControl | uint16 |
Description | string | The flow control mechanism used in transmitting data.
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Off, DC1/DC3, V.24 ckt 106/133
TransmitIFrameCount | uint64 |
Counter | boolean | true
Description | string | Number of I-Frames transmitted for the last or current call. A continuous connection might exceed this value, given enough time. Typically these counters are implemented as 32- bit counters, but additional bits can be provided and are accounted for in this property. If these counters hit maximum value, the DCE manufacturer might roll over to 0.
TransmitIFrameErrorCount | uint64 |
Counter | boolean | true
Description | string | Number of I-Frame errors detected for the last or current call, if error control protocol is running. A DCE might limit this counter to 16 bits, but additional bits can be provided and are accounted for in this property.
UnimodemRevision | string |
Description | string | Diagnostic Command Specification, Unimodem revision number.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AllocationState | string | CIM_LogicalDevice
AnswerMode | uint16 | CIM_POTSModem
Availability | uint16 | CIM_LogicalDevice
BlockErrors | uint32 | CIM_CallBasedModem
BlocksReceived | uint32 | CIM_CallBasedModem
BlocksResent | uint32 | CIM_CallBasedModem
BlocksSent | uint32 | CIM_CallBasedModem
CallLength | datetime | CIM_CallBasedModem
CallSpeed | uint32 | CIM_CallBasedModem
CallStatus | uint16 | CIM_CallBasedModem
Caption | string | CIM_ManagedElement
CharsLost | uint32 | CIM_CallBasedModem
CharsReceived | uint32 | CIM_CallBasedModem
CharsSent | uint32 | CIM_CallBasedModem
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CompressionInfo | uint16 | CIM_CallBasedModem
CountrySelected | string | CIM_POTSModem
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
DialType | uint16 | CIM_POTSModem
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Equalization | uint16 | CIM_POTSModem
ErrorCleared | boolean | CIM_LogicalDevice
ErrorControlInfo | uint16 | CIM_CallBasedModem
ErrorDescription | string | CIM_LogicalDevice
FallbackEnabled | boolean | CIM_CallBasedModem
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InactivityTimeout | uint32 | CIM_POTSModem
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxBaudRateToPhone | uint32 | CIM_POTSModem
MaxBaudRateToSerialPort | uint32 | CIM_POTSModem
MaxNumberOfPasswords | uint16 | CIM_POTSModem
MaxQuiesceTime | uint64 | CIM_LogicalDevice
ModulationScheme | uint16 | CIM_CallBasedModem
Name | string | CIM_ManagedSystemElement
NumberDialed | string | CIM_CallBasedModem
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherCompressionDescription | string | CIM_CallBasedModem
OtherCompressionInfoDescription | string | CIM_CallBasedModem
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherErrorControlDescription | string | CIM_CallBasedModem
OtherErrorControlInfoDescription | string | CIM_CallBasedModem
OtherModulationDescription | string | CIM_CallBasedModem
OtherSchemeDescription | string | CIM_CallBasedModem
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
RingsBeforeAnswer | uint8 | CIM_POTSModem
SpeakerVolumeInfo | uint16 | CIM_POTSModem
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SupportsCallback | boolean | CIM_POTSModem
SupportsSynchronousConnect | boolean | CIM_POTSModem
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastReset | datetime | CIM_CallBasedModem
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
BlackListedNumbers | string[] | CIM_POTSModem
Capabilities | uint16[] | CIM_POTSModem
CapabilityDescriptions | string[] | CIM_POTSModem
CompressionSupported | uint16[] | CIM_CallBasedModem
CountriesSupported | string[] | CIM_POTSModem
CurrentPasswords | string[] | CIM_POTSModem
EnabledCapabilities | uint16[] | CIM_POTSModem
ErrorControlSupported | uint16[] | CIM_CallBasedModem
IdentifyingDescriptions | string[] | CIM_LogicalDevice
ModulationSupported | uint16[] | CIM_CallBasedModem
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice