# Class CIM_TokenRingPort
extends CIM_NetworkPort

Capabilities and management of a TokenRingPort.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_LogicalPort
|
+--CIM_NetworkPort
|
+--CIM_TokenRingPort

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of a TokenRingPort.
UMLPackagePath | string | CIM::Device::Ports
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
MaxDataSize | uint32 |
Description | string | The maximum size of the INFO (non-MAC) field that will be received or transmitted.
MappingStrings | string | MIB.IETF|BRIDGE-MIB.dot1dTpPortMaxInfo
RingOpenStatus | uint16 |
Description | string | This property indicates the success, or the reason for failure, of the most recent attempt by the station to enter the ring.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token Ring MIB.dot5RingOpenStatus
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10
Values | string | No Open Attempted, Bad Parameter, Lobe Failed, Signal Loss, Insertion Timeout, Ring Failed, Beaconing, Duplicate MAC, Request Failed, Remove Received, Last Open Successful
RingSpeed | uint16 |
Description | string | The bandwidth of the ring.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token Ring MIB.dot5RingSpeed
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, One Megabit, Four Megabit, Sixteen Megabit
RingState | uint16 |
Description | string | The current Device state with respect to entering or leaving the ring.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token Ring MIB.dot5RingState
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Opened, Closed, Opening, Closing, Open Failure, Ring Failure
RingStatus | uint32 |
Description | string | The current status that can be used to diagnose fluctuating problems that can occur on token rings, after a station has successfully been added to the ring. Before an open is completed, this object contains the value that indicates "no status" (131072). (The RingState and RingOpenStatus properties are also provided for debugging problems when the station cannot even enter the ring.) The value of the property is a sum of values, one for each currently applicable condition. The following values are defined for various conditions: 0 = No Problems Detected, 32 = Ring Recovery, 64 = Single Station, 256 = Remove Received, 512 = Reserved, 1024 = Auto-Removal Error, 2048 = Lobe Wire Fault, 4096 = Transmit Beacon, 8192 = Soft Error, 16384 = Hard Error, 32768 = Signal Loss, 131072 = No Status, Open Not Completed.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token Ring MIB.dot5RingStatus
Capabilities | uint16[] |
ArrayType | string | Indexed
Description | string | Capabilities of the TokenRingPort. For example, the Device might support AlertOnLan, WakeOnLan, Load Balancing, or Failover. If failover or load balancing capabilities are listed, a SpareGroup (failover) or ExtraCapacityGroup (load balancing) should also be defined to completely describe the capability.
ModelCorrespondence | string | CIM_TokenRingPort.CapabilityDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Unknown, Other, AlertOnLan, WakeOnLan, FailOver, LoadBalancing
CapabilityDescriptions | string[] |
ArrayType | string | Indexed
Description | string | An array of free-form strings that provides more detailed explanations for any of the TokenRingAPort features that are indicated in the Capabilities array. Note, each entry of this array is related to the entry in the Capabilities array that is located at the same index.
ModelCorrespondence | string | CIM_TokenRingPort.Capabilities
EnabledCapabilities | uint16[] |
ArrayType | string | Indexed
Description | string | Specifies which of the capabilities from the "Capabilities" property are currently enabled.
ModelCorrespondence | string | CIM_TokenRingPort.Capabilities, CIM_TokenRingPort.OtherEnabledCapabilities
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Unknown, Other, AlertOnLan, WakeOnLan, FailOver, LoadBalancing
NetworkAddresses | string[] |
Description | string | Token Ring/802.5 MAC addresses formatted as twelve hexadecimal digits (for example,"010203040506"), with each pair representing one of the six octets of the MAC address in "canonical" bit order. (Therefore, the Group address bit is found in the low order bit of the first character of the string.)
MappingStrings | string | MIF.DMTF|Network Adapter 802 Port|001.3
MaxLen | uint32 | 64
Override | string | NetworkAddresses
OtherEnabledCapabilities | string[] |
ArrayType | string | Indexed
Description | string | An array of free-form strings that provides more detailed explanations for any of the enabled capabilities that are specified as 'Other'.
ModelCorrespondence | string | CIM_TokenRingPort.EnabledCapabilities

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
ActiveMaximumTransmissionUnit | uint64 | CIM_NetworkPort
AllocationState | string | CIM_LogicalDevice
AutoSense | boolean | CIM_NetworkPort
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
FullDuplex | boolean | CIM_NetworkPort
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LinkTechnology | uint16 | CIM_NetworkPort
LocationIndicator | uint16 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
MaxSpeed | uint64 | CIM_LogicalPort
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherLinkTechnology | string | CIM_NetworkPort
OtherNetworkPortType | string | CIM_NetworkPort
OtherPortType | string | CIM_LogicalPort
PermanentAddress | string | CIM_NetworkPort
PortNumber | uint16 | CIM_NetworkPort
PortType | uint16 | CIM_LogicalPort
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedSpeed | uint64 | CIM_LogicalPort
RequestedState | uint16 | CIM_EnabledLogicalElement
Speed | uint64 | CIM_NetworkPort
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SupportedMaximumTransmissionUnit | uint64 | CIM_NetworkPort
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
UsageRestriction | uint16 | CIM_LogicalPort
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice