# Class CIM_AlarmDevice
extends CIM_LogicalDevice

An AlarmDevice is a type of Device that emits audible or visible indications related to a problem situation.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_AlarmDevice

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | An AlarmDevice is a type of Device that emits audible or visible indications related to a problem situation.
UMLPackagePath | string | CIM::Device::Sensors
Version | string | 2.8.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AlarmState | uint16 |
Description | string | The current state of the alarm.
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Off, Steady, Alternating
AudibleAlarm | boolean |
Description | string | Boolean indicating that the Alarm is audible.
AudioIndicatorIsDisabled | boolean |
Description | string | True indicates that the audio of an AlarmState indicator has been disabled (i.e. muted). A disabled state here does not imply that the AlarmState is off.
MotionAlarm | boolean |
Description | string | Boolean indicating that the Alarm causes motion of the Device.
MotionIndicatorIsDisabled | boolean |
Description | string | True indicates that the motion of an AlarmState indicator has been disabled (i.e. stopped). A disabled state here does not imply that the AlarmState is off.
Urgency | uint16 |
Description | string | Urgency is an enumerated value that indicates the relative frequency at which the Alarm flashes, vibrates and/or emits audible tones.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6
Values | string | Unknown, Other, Not Supported, Informational, Non-Critical, Critical, Unrecoverable
VisibleAlarm | boolean |
Description | string | Boolean indicating that the Alarm is visible.
VisualIndicatorIsDisabled | boolean |
Description | string | True indicates that the visual of an AlarmState indicator has been disabled (i.e. dimmed). A disabled state here does not imply that the AlarmState is off.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AllocationState | string | CIM_LogicalDevice
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Local Class Methods

#### SetAlarmState (uint32)

#### Method Qualifiers (SetAlarmState)

Name | Data Type | Value
--- | --- | ---
Description | string | SetAlarmState is a method for defining the current state of the Alarm. Its input parameter, RequestedAlarmState, is specified using the Values list of AlarmDevice's AlarmState property. SetAlarmState returns 0 if the request is successfully implemented, 1 if the specified RequestedAlarm State is not supported, and some other value if any other error occurred. In a subclass, the set of possible return codes should be specified using a ValueMap qualifier on the method. The strings to which the ValueMap contents are 'translated' should be specified as a Values array qualifier.

#### Method Parameters (SetAlarmState)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
RequestedAlarmState | uint16
Description | string | The desired state for the alarm.
IN | boolean | true
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Off, Steady, Alternating

#### SetAlarmIndicator (uint32)

#### Method Qualifiers (SetAlarmIndicator)

Name | Data Type | Value
--- | --- | ---
Description | string | SetAlarmIndicator is a method for enabling or disabling the indicator of the AlarmState function, without changing the current AlarmState. It has 3 input parameters, Audio Indicator, VisualIndicator and MotionIndicator. For all of the input parameters, a value of 0 indicates no change to the AlarmState indicator, 1 indicates Disable, and 2 indicates Enable. The method returns 0 if the request is successfully implemented, 1 if the specified request is not supported, and some other value if any other error occurred. In a subclass, the set of possible return codes should be specified using a ValueMap qualifier on the method. The strings to which the ValueMap contents are 'translated' should be specified as a Values array qualifier.

#### Method Parameters (SetAlarmIndicator)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
AudioIndicator | uint16
Description | string | The state for the audio indicator.
IN | boolean | true
ValueMap | string | 0, 1, 2
Values | string | No Change, Disable, Enable
MotionIndicator | uint16
Description | string | The state for the motion indicator.
IN | boolean | true
ValueMap | string | 0, 1, 2
Values | string | No Change, Disable, Enable
VisualIndicator | uint16
Description | string | The state for the visual indicator.
IN | boolean | true
ValueMap | string | 0, 1, 2
Values | string | No Change, Disable, Enable

#### SetUrgency (uint32)

#### Method Qualifiers (SetUrgency)

Name | Data Type | Value
--- | --- | ---
Description | string | SetUrgency is a method for defining the desired urgency level for the Alarm. Its input parameter, RequestedUrgency, is specified using the Values list of AlarmDevice's Urgency property. SetUrgency returns 0 if the request is successfully implemented, 1 if the specified Urgency level is not supported, and some other value if any other error occurred. In a subclass, the set of possible return codes should be specified using a ValueMap qualifier on the method. The strings to which the ValueMap contents are 'translated' should be specified as a Values array qualifier.

#### Method Parameters (SetUrgency)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
RequestedUrgency | uint16
Description | string | Desired urgency for the alarm.
IN | boolean | true
ValueMap | string | 1, 3, 4, 5, 6
Values | string | Other, Informational, Non-Critical, Critical, Unrecoverable

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice