# Class CIM_MediaRedirectionCapabilities
extends CIM_RedirectionServiceCapabilities

MediaRedirectionCapabilities describes the capabilities of the Media Redirection Service.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Capabilities
|
+--CIM_EnabledLogicalElementCapabilities
|
+--CIM_RedirectionServiceCapabilities
|
+--CIM_MediaRedirectionCapabilities

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | MediaRedirectionCapabilities describes the capabilities of the Media Redirection Service.
UMLPackagePath | string | CIM::Network::MediaRedirection
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ConnectionModesSupported | uint16[] |
Description | string | The connection mode used to configure the session. A value set to 2 = "Listen" shall indicate that the SAP will listen for a connection request from the remote Media redirection server. A CIM_BindsTo association to a CIM_ProtocolEndoint may be used to represent where the SAP is listening for the connection request. A value set to 3 = "Connect" shall indicate that the the SAP shall initiate the connection to the remote Media redirection server. A CIM_RemoteAccessAvailableToElement association to a CIM_RemoteServiceAccessPoint may be used to represent where the SAP shall connect to the remote Media redirection server.
ModelCorrespondence | string | CIM_MediaRedirectionSAP.ConnectionMode
ValueMap | string | 0, 2, 3, .., 32768..65535
Values | string | Unknown, Listen, Connect, DMTF Reserved, Vendor Specified
DevicesSupported | uint16[] |
ArrayType | string | Indexed
Description | string | An enumeration indicating the types of Media Devices which are supported by the Media Redirection Service. Note that each entry of this array is related to the entry in the MaxDevicesSupported array that is located at the same index.
ModelCorrespondence | string | CIM_MediaRedirectionCapabilities.MaxDevicesSupported
ValueMap | string | 0, 2, 3, 4, 5, 6, 7, 8, .., 32768..65535
Values | string | Unknown, CIM_CDROMDrive, CIM_DiskDrive, CIM_DisketteDrive, CIM_DVDDrive, CIM_MagnetoOpticalDrive, CIM_TapDrive, CIM_WORMDrive, DMTF_ Reserved, Vendor_ Specified
InfoFormatsSupported | uint16[] |
Description | string | An enumeration indicating which of the formats for CIM_RemoteServiceAccessPoint.InfoFormat are supported by the Media Redirection Service.
ModelCorrespondence | string | CIM_RemoteServiceAccessPoint.InfoFormat
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 10, 11, 12, 13, 100, 101, 102, 200, 201, 202, 203, 204, 205, .., 32768..65535
Values | string | Other, Host Name, IPv4 Address, IPv6 Address, IPX Address, DECnet Address, SNA Address, IPv4 Subnet Address, IPv6 Subnet Address, IPv4 Address Range, IPv6 Address Range, Dial String, Ethernet Address, Token Ring Address, URL, FQDN, User FQDN, DER ASN1 DN, DER ASN1 GN, Key ID, DMTF Reserved, Vendor Reserved
MaxDevicesPerSAP | uint16[] |
ArrayType | string | Indexed
Description | string | An enumeration indicating the number of Media devices per MediaRedirection Session which are supported for the devices specified in the DevicesSupported array property. Note that each entry of this array is related to the engry in the DevicesSupported array that is located at the same index.
ModelCorrespondence | string | CIM_MediaRedirectionCapabilities.DevicesSupported
MaxDevicesSupported | uint16[] |
ArrayType | string | Indexed
Description | string | An enumeration indicating the number of Media devices which are supported for the devices specified in the DevicesSupported array property. Note that each entry of this array is related to the entry in the DevicesSupported that is located at the same index.
ModelCorrespondence | string | CIM_MediaRedirectionCapabilities.DevicesSupported
SAPCapabilitiesSupported | uint16[] |
Description | string | An enumeration indicating the whether instances of USBRedirectionSAPs already exist and whether whether SAPs can be created. A value set to 2 = "Modify Timeouts" shall indicate that the timeout parameters of instances of CIM_USBRedirectionSAP can be modified by applications using 'ModifyInstance'
ValueMap | string | 0, 2, .., 32768..65535
Values | string | Unknown, Modify SAP, DMTF Reserved, Vendor Specified

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_Capabilities
ElementNameEditSupported | boolean | CIM_EnabledLogicalElementCapabilities
ElementNameMask | string | CIM_EnabledLogicalElementCapabilities
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_Capabilities
MaxElementNameLen | uint16 | CIM_EnabledLogicalElementCapabilities
RequestedStatesSupported | uint16[] | CIM_EnabledLogicalElementCapabilities
SharingModeSupported | uint16[] | CIM_RedirectionServiceCapabilities
StateAwareness | uint16[] | CIM_EnabledLogicalElementCapabilities

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
CreateGoalSettings | uint16 | CIM_Capabilities