# Class CIM_ADSLModem
extends CIM_DSLModem

The ADSLModem class represents Modems of the DSL type = ADSL, Asymmetric Digital Subscriber Line.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Modem
|
+--CIM_ConnectionBasedModem
|
+--CIM_DSLModem
|
+--CIM_ADSLModem

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | The ADSLModem class represents Modems of the DSL type = ADSL, Asymmetric Digital Subscriber Line.
UMLPackagePath | string | CIM::Device::Modems
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
LineAttenuation | uint32 |
Description | string | Measured difference in the total power transmitted by the peer Modem and the total power received by this Modem. This value is measured in tenths of dB.
Gauge | boolean | true
PUnit | string | decibel * 10^-1
Units | string | Tenths of Decibels
LineState | uint32 |
Description | string | Status indicates the current state of the connection (line). The property holds a bit map that describes the possible conditions. For example, 1) No Defect - There are no defects on the line; 2) Loss Of Framing - ATUR failure due to the inability to receive a valid frame; 4) Loss Of Signal - ATUR failure due to the inability to receive a signal; 8) Loss Of Power - ATUR failure due to loss of power; 32) Loss Of Signal Quality - Loss of Signal Quality is declared when the NoiseMargin falls below the minimum NoiseMargin, or the bit-error-rate exceeds 10^-7.
ValueMap | string | 1, 2, 4, 8, 32
Values | string | No Defect, Loss Of Framing, Loss Of Signal, Loss Of Power, Loss Of Signal Quality
MaxDataRate | uint32 |
Description | string | Indicates the maximum currently attainable data rate for the Modem. This value will be equal to or greater than the current line rate.
PUnit | string | bit / second
Units | string | Bits per Second
NoiseMargin | uint32 |
Description | string | Noise Margin of this Modem with respect to its received signal, in tenths of dB.
PUnit | string | decibel * 10^-1
Units | string | Tenths of Decibels
TotalOutputPower | uint32 |
Description | string | Measured total output power (in tenths of dB) transmitted by this Modem.
Gauge | boolean | true
PUnit | string | decibel * 10^-1
Units | string | Tenths of Decibels

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
VendorID | string
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32