# Class CIM_SBProtocolEndpoint
extends CIM_ProtocolEndpoint

CIM_SBProtocolEndpoint extends CIM_ProtocolEndpoint with properties for FC Single-Byte connectivity.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_ProtocolEndpoint
|
+--CIM_SBProtocolEndpoint

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | CIM_SBProtocolEndpoint extends CIM_ProtocolEndpoint with properties for FC Single-Byte connectivity.
UMLPackagePath | string | CIM::Device::Ports
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ConnectionType | uint16 |
Description | string | The supported connection type for this endpoint. The connection type may be needed before the port(s) are associated and also is used in some SCSI commands.
MappingStrings | string | SPC.INCITS-T10 | Protocol Identifier | Values
ModelCorrespondence | string | CIM_SCSIProtocolEndpoint.Name, CIM_SCSIProtocolEndpoint.OtherConnectionType
ValueMap | string | 1, 2
Values | string | Other, Fibre Channel
OtherConnectionType | string |
Description | string | The connection type, if ConnectionType is "Other".
ModelCorrespondence | string | CIM_SCSIProtocolEndpoint.Name, CIM_SCSIProtocolEndpoint.ConnectionType
Role | uint16 |
Description | string | For iSCSI, each SCSIProtocolEndpoint MUST act as either a target or an initiator endpoint. Other transports allow a SCSI PE to act as both an initiator and target endpoint. This property indicates which role this ProtocolEndpoint implements.
ValueMap | string | 0, 2, 3, 4
Values | string | Unknown, Initiator, Target, Both Initiator and Target
TargetRelativePortNumber | uint32 |
Description | string | For ports on a target device, the port number, relative to the storage system. 0 is reserved by T10, 1 is port A, 2 is port B, etc. These numbers are used in SCSI commands that operate on target port groups.
MappingStrings | string | SPC.INCITS-T10 | RelativeTargetPort | IdentifierFormat
MinValue | sint64 | 1

### Inherited Properties

Name | Data Type
--- | ---
BroadcastResetSupported | boolean
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
Name | string
NameFormat | string
OperatingStatus | uint16
OtherEnabledState | string
OtherTypeDescription | string
PrimaryStatus | uint16
ProtocolIFType | uint16
ProtocolType | uint16
RequestedState | uint16
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
BroadcastReset | uint32
RequestStateChange | uint32